From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Icenowy Zheng <icenowy@aosc.io>
Date: Mon, 25 Dec 2017 12:10:59 +0800
Subject: [PATCH] arm64: allwinner: dts: h6: enable USB3 port on Pine H64

Pine H64 board have a USB3 port, which is connected to the USB3 pins of
the H6 SoC, and the 5V power supply is controlled via GPIO (shared with
the power USB ports).

Enable this port.

Signed-off-by: Icenowy Zheng <icenowy@aosc.io>
Reviewed-by: Chen-Yu Tsai <wens@csie.org>
---
 arch/arm64/boot/dts/allwinner/sun50i-h6-pine-h64.dts | 9 +++++++++
 1 file changed, 9 insertions(+)

--- a/arch/arm64/boot/dts/allwinner/sun50i-h6-pine-h64.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h6-pine-h64.dts
@@ -97,6 +97,10 @@
 	status = "okay";
 };
 
+&dwc3 {
+	status = "okay";
+};
+
 &emac {
 	pinctrl-names = "default";
 	pinctrl-0 = <&ext_rgmii_pins>;
@@ -332,3 +336,8 @@
 	usb3_vbus-supply = <&reg_usb_vbus>;
 	status = "okay";
 };
+
+&usb3phy {
+	phy-supply = <&reg_usb_vbus>;
+	status = "okay";
+};
