From 34cfc53ec99e6e3356bb6e06ecd68faa4d2e4bac Mon Sep 17 00:00:00 2001
From: Christian Hewitt <christianshewitt@gmail.com>
Date: Wed, 29 Apr 2020 10:37:08 +0000
Subject: [PATCH 05/21] WIP: arm: dts: exynos5422: HC1/XU3/XU4 model name is
 ODROID not Odroid

Cosmetic change to model and audio card name for HC1/XU3/XU4 to
put ODROID in capitals (as per Hardkernel branding).

Signed-off-by: Christian Hewitt <christianshewitt@gmail.com>
---
 arch/arm/boot/dts/samsung/exynos5422-odroidhc1.dts        | 5 ++---
 arch/arm/boot/dts/samsung/exynos5422-odroidxu3-audio.dtsi | 2 +-
 arch/arm/boot/dts/samsung/exynos5422-odroidxu3-lite.dts   | 2 +-
 arch/arm/boot/dts/samsung/exynos5422-odroidxu3.dts        | 2 +-
 arch/arm/boot/dts/samsung/exynos5422-odroidxu4.dts        | 7 +++----
 5 files changed, 8 insertions(+), 10 deletions(-)

diff --git a/arch/arm/boot/dts/samsung/exynos5422-odroidhc1.dts b/arch/arm/boot/dts/samsung/exynos5422-odroidhc1.dts
index d91f7fa2cf80..6550d59ce3d8 100644
--- a/arch/arm/boot/dts/samsung/exynos5422-odroidhc1.dts
+++ b/arch/arm/boot/dts/samsung/exynos5422-odroidhc1.dts
@@ -11,9 +11,8 @@
 #include "exynos5422-odroid-core.dtsi"
 
 / {
-	model = "Hardkernel Odroid HC1";
-	compatible = "hardkernel,odroid-hc1", "samsung,exynos5800", \
-		     "samsung,exynos5";
+	model = "Hardkernel ODROID HC1";
+	compatible = "hardkernel,odroid-hc1", "samsung,exynos5800", "samsung,exynos5";
 
 	led-controller {
 		compatible = "pwm-leds";
diff --git a/arch/arm/boot/dts/samsung/exynos5422-odroidxu3-audio.dtsi b/arch/arm/boot/dts/samsung/exynos5422-odroidxu3-audio.dtsi
index 86b96f9706db..1a3940f2ead2 100644
--- a/arch/arm/boot/dts/samsung/exynos5422-odroidxu3-audio.dtsi
+++ b/arch/arm/boot/dts/samsung/exynos5422-odroidxu3-audio.dtsi
@@ -13,7 +13,7 @@
 / {
 	sound: sound {
 		compatible = "samsung,odroid-xu3-audio";
-		model = "Odroid-XU3";
+		model = "ODROID-XU3";
 
 		samsung,audio-widgets =
 			"Headphone", "Headphone Jack",
diff --git a/arch/arm/boot/dts/samsung/exynos5422-odroidxu3-lite.dts b/arch/arm/boot/dts/samsung/exynos5422-odroidxu3-lite.dts
index e3154a1cae23..4d337f9e79b8 100644
--- a/arch/arm/boot/dts/samsung/exynos5422-odroidxu3-lite.dts
+++ b/arch/arm/boot/dts/samsung/exynos5422-odroidxu3-lite.dts
@@ -14,7 +14,7 @@
 #include "exynos54xx-odroidxu-leds.dtsi"
 
 / {
-	model = "Hardkernel Odroid XU3 Lite";
+	model = "Hardkernel ODROID XU3 Lite";
 	compatible = "hardkernel,odroid-xu3-lite", "samsung,exynos5800", "samsung,exynos5";
 
 	aliases {
diff --git a/arch/arm/boot/dts/samsung/exynos5422-odroidxu3.dts b/arch/arm/boot/dts/samsung/exynos5422-odroidxu3.dts
index a378d4937ff7..21cf909b9cc8 100644
--- a/arch/arm/boot/dts/samsung/exynos5422-odroidxu3.dts
+++ b/arch/arm/boot/dts/samsung/exynos5422-odroidxu3.dts
@@ -13,7 +13,7 @@
 #include "exynos54xx-odroidxu-leds.dtsi"
 
 / {
-	model = "Hardkernel Odroid XU3";
+	model = "Hardkernel ODROID XU3";
 	compatible = "hardkernel,odroid-xu3", "samsung,exynos5800", "samsung,exynos5";
 
 	aliases {
diff --git a/arch/arm/boot/dts/samsung/exynos5422-odroidxu4.dts b/arch/arm/boot/dts/samsung/exynos5422-odroidxu4.dts
index 1c24f9b35973..caf4f50e91df 100644
--- a/arch/arm/boot/dts/samsung/exynos5422-odroidxu4.dts
+++ b/arch/arm/boot/dts/samsung/exynos5422-odroidxu4.dts
@@ -13,9 +13,8 @@
 #include "exynos5422-odroidxu3-common.dtsi"
 
 / {
-	model = "Hardkernel Odroid XU4";
-	compatible = "hardkernel,odroid-xu4", "samsung,exynos5800", \
-		     "samsung,exynos5";
+	model = "Hardkernel ODROID XU4";
+	compatible = "hardkernel,odroid-xu4", "samsung,exynos5800", "samsung,exynos5";
 
 	led-controller {
 		compatible = "pwm-leds";
@@ -31,7 +30,7 @@
 
 	sound: sound {
 		compatible = "samsung,odroid-xu3-audio";
-		model = "Odroid-XU4";
+		model = "ODROID-XU4";
 
 		samsung,audio-routing = "I2S Playback", "Mixer DAI TX";
 
-- 
2.17.1

