From 5dd9978ccd81cbb48b57580d90a2ce4bd8305c26 Mon Sep 17 00:00:00 2001
From: Jernej Skrabec <jernej.skrabec@gmail.com>
Date: Thu, 12 Oct 2023 20:19:38 +0200
Subject: [PATCH 25/25] HACK: clk: sunxi-ng: unify parent for HDMI clocks

Signed-off-by: Jernej Skrabec <jernej.skrabec@gmail.com>
---
 drivers/clk/sunxi-ng/ccu-sun50i-h6.c | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

diff --git a/drivers/clk/sunxi-ng/ccu-sun50i-h6.c b/drivers/clk/sunxi-ng/ccu-sun50i-h6.c
index 892df807275c..b63e544c86a7 100644
--- a/drivers/clk/sunxi-ng/ccu-sun50i-h6.c
+++ b/drivers/clk/sunxi-ng/ccu-sun50i-h6.c
@@ -653,7 +653,7 @@ static SUNXI_CCU_M_WITH_GATE(pcie_aux_clk, "pcie-aux", "osc24M", 0xab8,
 static SUNXI_CCU_GATE(bus_pcie_clk, "bus-pcie", "psi-ahb1-ahb2",
 		      0xabc, BIT(0), 0);
 
-static const char * const hdmi_parents[] = { "pll-video0", "pll-video1",
+static const char * const hdmi_parents[] = { "osc24M", "pll-video1",
 					      "pll-video1-4x" };
 static SUNXI_CCU_M_WITH_MUX_GATE(hdmi_clk, "hdmi", hdmi_parents, 0xb00,
 				 0, 4,		/* M */
@@ -707,8 +707,8 @@ static SUNXI_CCU_MUX_WITH_GATE(tcon_lcd0_clk, "tcon-lcd0",
 static SUNXI_CCU_GATE(bus_tcon_lcd0_clk, "bus-tcon-lcd0", "ahb3",
 		      0xb7c, BIT(0), 0);
 
-static const char * const tcon_tv0_parents[] = { "pll-video0",
-						 "pll-video0-4x",
+static const char * const tcon_tv0_parents[] = { "osc24M",
+						 "osc24M",
 						 "pll-video1",
 						 "pll-video1-4x" };
 static SUNXI_CCU_MP_WITH_MUX_GATE(tcon_tv0_clk, "tcon-tv0",
-- 
2.42.0

