From e6298e5601c435f4b847271bfcf33044a343ec6a Mon Sep 17 00:00:00 2001
From: Martin Blumenstingl <martin.blumenstingl@googlemail.com>
Date: Fri, 27 Dec 2024 22:25:13 +0100
Subject: [PATCH 17/58] FROMGIT(6.14): arm64: dts: amlogic: axg: switch to the
 new PWM controller binding

Use the new PWM controller binding which now relies on passing all
clock inputs available on the SoC (instead of passing the "wanted"
clock input for a given board).

Signed-off-by: Martin Blumenstingl <martin.blumenstingl@googlemail.com>
---
 arch/arm64/boot/dts/amlogic/meson-axg.dtsi | 24 ++++++++++++++++++----
 1 file changed, 20 insertions(+), 4 deletions(-)

diff --git a/arch/arm64/boot/dts/amlogic/meson-axg.dtsi b/arch/arm64/boot/dts/amlogic/meson-axg.dtsi
index e9b22868983d..a6924d246bb1 100644
--- a/arch/arm64/boot/dts/amlogic/meson-axg.dtsi
+++ b/arch/arm64/boot/dts/amlogic/meson-axg.dtsi
@@ -1693,8 +1693,12 @@ sec_AO: ao-secure@140 {
 			};
 
 			pwm_AO_cd: pwm@2000 {
-				compatible = "amlogic,meson-axg-ao-pwm";
+				compatible = "amlogic,meson-axg-pwm-v2", "amlogic,meson8-pwm-v2";
 				reg = <0x0 0x02000  0x0 0x20>;
+				clocks = <&xtal>,
+					 <&clkc_AO CLKID_AO_CLK81>,
+					 <&clkc CLKID_FCLK_DIV4>,
+					 <&clkc CLKID_FCLK_DIV5>;
 				#pwm-cells = <3>;
 				status = "disabled";
 			};
@@ -1728,8 +1732,12 @@ i2c_AO: i2c@5000 {
 			};
 
 			pwm_AO_ab: pwm@7000 {
-				compatible = "amlogic,meson-axg-ao-pwm";
+				compatible = "amlogic,meson-axg-pwm-v2", "amlogic,meson8-pwm-v2";
 				reg = <0x0 0x07000 0x0 0x20>;
+				clocks = <&xtal>,
+					 <&clkc_AO CLKID_AO_CLK81>,
+					 <&clkc CLKID_FCLK_DIV4>,
+					 <&clkc CLKID_FCLK_DIV5>;
 				#pwm-cells = <3>;
 				status = "disabled";
 			};
@@ -1806,15 +1814,23 @@ watchdog@f0d0 {
 			};
 
 			pwm_ab: pwm@1b000 {
-				compatible = "amlogic,meson-axg-ee-pwm";
+				compatible = "amlogic,meson-axg-pwm-v2", "amlogic,meson8-pwm-v2";
 				reg = <0x0 0x1b000 0x0 0x20>;
+				clocks = <&xtal>,
+					 <&clkc CLKID_FCLK_DIV5>,
+					 <&clkc CLKID_FCLK_DIV4>,
+					 <&clkc CLKID_FCLK_DIV3>;
 				#pwm-cells = <3>;
 				status = "disabled";
 			};
 
 			pwm_cd: pwm@1a000 {
-				compatible = "amlogic,meson-axg-ee-pwm";
+				compatible = "amlogic,meson-axg-pwm-v2", "amlogic,meson8-pwm-v2";
 				reg = <0x0 0x1a000 0x0 0x20>;
+				clocks = <&xtal>,
+					 <&clkc CLKID_FCLK_DIV5>,
+					 <&clkc CLKID_FCLK_DIV4>,
+					 <&clkc CLKID_FCLK_DIV3>;
 				#pwm-cells = <3>;
 				status = "disabled";
 			};
-- 
2.34.1

