From 71e505c40e0c57bf296d749666087d3d26305ef8 Mon Sep 17 00:00:00 2001
From: Jonas Karlman <jonas@kwiboo.se>
Date: Sun, 17 Feb 2019 22:14:38 +0000
Subject: [PATCH 45/58] WIP: mmc: core: set initial signal voltage on power off

Some boards have SD card connectors where the power rail cannot be switched
off by the driver. If the card has not been power cycled, it may still be
using 1.8V signaling after a warm re-boot. Bootroms expecting 3.3V signaling
will fail to boot from a UHS card that continue to use 1.8V signaling.

Set initial signal voltage in mmc_power_off() to allow re-boot to function.

This fixes re-boot with UHS cards on Asus Tinker Board (Rockchip RK3288),
same issue have been seen on some Rockchip RK3399 boards.

I am sending this as a RFC because I have no insights into SD/MMC subsystem,
this change fix a re-boot issue on my boards and does not break emmc/sdio.
Is this an acceptable workaround? Any advice is appreciated.

Signed-off-by: Jonas Karlman <jonas@kwiboo.se>
---
 drivers/mmc/core/core.c | 8 ++++++++
 1 file changed, 8 insertions(+)

diff --git a/drivers/mmc/core/core.c b/drivers/mmc/core/core.c
index 327029f5c59b..5ac10a847630 100644
--- a/drivers/mmc/core/core.c
+++ b/drivers/mmc/core/core.c
@@ -1368,6 +1368,14 @@ void mmc_power_off(struct mmc_host *host)
 	if (host->ios.power_mode == MMC_POWER_OFF)
 		return;
 
+	mmc_set_initial_signal_voltage(host);
+
+	/*
+	 * This delay should be sufficient to allow the power supply
+	 * to reach the minimum voltage.
+	 */
+	mmc_delay(host->ios.power_delay_ms);
+
 	mmc_pwrseq_power_off(host);
 
 	host->ios.clock = 0;
-- 
2.34.1

