From 48432d3ed3b7011051afc3d422e50cd42ebf860b Mon Sep 17 00:00:00 2001
From: Jerome Brunet <jbrunet@baylibre.com>
Date: Fri, 13 Dec 2024 15:30:17 +0100
Subject: [PATCH 13/58] FROMGIT(6.14): clk: amlogic: g12b: fix cluster A parent
 data

Several clocks used by both g12a and g12b use the g12a cpu A clock hw
pointer as clock parent. This is incorrect on g12b since the parents of
cluster A cpu clock are different. Also the hw clock provided as parent to
these children is not even registered clock on g12b.

Fix the problem by reverting to the global namespace and let CCF pick
the appropriate, as it is already done for other clocks, such as
cpu_clk_trace_div.

Fixes: 25e682a02d91 ("clk: meson: g12a: migrate to the new parent description method")
Signed-off-by: Jerome Brunet <jbrunet@baylibre.com>
---
 drivers/clk/meson/g12a.c | 36 ++++++++++++++++++++++++------------
 1 file changed, 24 insertions(+), 12 deletions(-)

diff --git a/drivers/clk/meson/g12a.c b/drivers/clk/meson/g12a.c
index ff634d3a2f95..4f92b83965d5 100644
--- a/drivers/clk/meson/g12a.c
+++ b/drivers/clk/meson/g12a.c
@@ -1139,8 +1139,18 @@ static struct clk_regmap g12a_cpu_clk_div16_en = {
 	.hw.init = &(struct clk_init_data) {
 		.name = "cpu_clk_div16_en",
 		.ops = &clk_regmap_gate_ro_ops,
-		.parent_hws = (const struct clk_hw *[]) {
-			&g12a_cpu_clk.hw
+		.parent_data = &(const struct clk_parent_data) {
+			/*
+			 * Note:
+			 * G12A and G12B have different cpu clocks (with
+			 * different struct clk_hw). We fallback to the global
+			 * naming string mechanism so this clock picks
+			 * up the appropriate one. Same goes for the other
+			 * clock using cpu cluster A clock output and present
+			 * on both G12 variant.
+			 */
+			.name = "cpu_clk",
+			.index = -1,
 		},
 		.num_parents = 1,
 		/*
@@ -1205,7 +1215,10 @@ static struct clk_regmap g12a_cpu_clk_apb_div = {
 	.hw.init = &(struct clk_init_data){
 		.name = "cpu_clk_apb_div",
 		.ops = &clk_regmap_divider_ro_ops,
-		.parent_hws = (const struct clk_hw *[]) { &g12a_cpu_clk.hw },
+		.parent_data = &(const struct clk_parent_data) {
+			.name = "cpu_clk",
+			.index = -1,
+		},
 		.num_parents = 1,
 	},
 };
@@ -1239,7 +1252,10 @@ static struct clk_regmap g12a_cpu_clk_atb_div = {
 	.hw.init = &(struct clk_init_data){
 		.name = "cpu_clk_atb_div",
 		.ops = &clk_regmap_divider_ro_ops,
-		.parent_hws = (const struct clk_hw *[]) { &g12a_cpu_clk.hw },
+		.parent_data = &(const struct clk_parent_data) {
+			.name = "cpu_clk",
+			.index = -1,
+		},
 		.num_parents = 1,
 	},
 };
@@ -1273,7 +1289,10 @@ static struct clk_regmap g12a_cpu_clk_axi_div = {
 	.hw.init = &(struct clk_init_data){
 		.name = "cpu_clk_axi_div",
 		.ops = &clk_regmap_divider_ro_ops,
-		.parent_hws = (const struct clk_hw *[]) { &g12a_cpu_clk.hw },
+		.parent_data = &(const struct clk_parent_data) {
+			.name = "cpu_clk",
+			.index = -1,
+		},
 		.num_parents = 1,
 	},
 };
@@ -1308,13 +1327,6 @@ static struct clk_regmap g12a_cpu_clk_trace_div = {
 		.name = "cpu_clk_trace_div",
 		.ops = &clk_regmap_divider_ro_ops,
 		.parent_data = &(const struct clk_parent_data) {
-			/*
-			 * Note:
-			 * G12A and G12B have different cpu_clks (with
-			 * different struct clk_hw). We fallback to the global
-			 * naming string mechanism so cpu_clk_trace_div picks
-			 * up the appropriate one.
-			 */
 			.name = "cpu_clk",
 			.index = -1,
 		},
-- 
2.34.1

