From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Jernej Skrabec <jernej.skrabec@siol.net>
Date: Sat, 16 Jan 2021 10:58:14 +0100
Subject: [PATCH] HACK: h6: Add HDMI sound card

Signed-off-by: Jernej Skrabec <jernej.skrabec@siol.net>
---
 arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi | 20 +++++++++++++++++++-
 1 file changed, 19 insertions(+), 1 deletion(-)

--- a/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
@@ -108,6 +108,24 @@
 			(GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>;
 	};
 
+	sound_hdmi: sound {
+		compatible = "simple-audio-card";
+		simple-audio-card,format = "i2s";
+		simple-audio-card,name = "allwinner-hdmi";
+		simple-audio-card,mclk-fs = <128>;
+		simple-audio-card,frame-inversion;
+
+		simple-audio-card,codec {
+			sound-dai = <&hdmi>;
+		};
+
+		simple-audio-card,cpu {
+			sound-dai = <&i2s1>;
+			dai-tdm-slot-num = <2>;
+			dai-tdm-slot-width = <32>;
+		};
+	};
+
 	soc {
 		compatible = "simple-bus";
 		#address-cells = <1>;
@@ -664,7 +682,6 @@
 			dmas = <&dma 4>, <&dma 4>;
 			resets = <&ccu RST_BUS_I2S1>;
 			dma-names = "rx", "tx";
-			status = "disabled";
 		};
 
 		spdif: spdif@5093000 {
@@ -801,6 +818,7 @@
 		};
 
 		hdmi: hdmi@6000000 {
+			#sound-dai-cells = <0>;
 			compatible = "allwinner,sun50i-h6-dw-hdmi";
 			reg = <0x06000000 0x10000>;
 			reg-io-width = <1>;
