From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Alex Bee <knaerzche@gmail.com>
Date: Mon, 31 Oct 2022 17:16:07 +0100
Subject: [PATCH 6/6] Rockchip: rk3399-evb: Don't initalize i2c bus in SPL

Since we are using this device as fallback for boards which are not supported
by mainline u-boot in combination with vendor TPL/SPL, we need to make sure
that i2c is initalized in BL33 because vendor bootchain doesn't do that in
an earlier level.
---
 arch/arm/dts/rk3399-evb-u-boot.dtsi | 10 +---------
 1 file changed, 1 insertion(+), 9 deletions(-)

diff --git a/arch/arm/dts/rk3399-evb-u-boot.dtsi b/arch/arm/dts/rk3399-evb-u-boot.dtsi
index 5e39b1493d..18733da7f9 100644
--- a/arch/arm/dts/rk3399-evb-u-boot.dtsi
+++ b/arch/arm/dts/rk3399-evb-u-boot.dtsi
@@ -9,18 +9,10 @@
 / {
 	chosen {
 		stdout-path = "serial2:1500000n8";
-		u-boot,spl-boot-order = "same-as-spl", &sdhci, &sdmmc;
+		u-boot,spl-boot-order = "same-as-spl", &sdmmc, &sdhci;
 	};
 };
 
-&i2c0 {
-	bootph-all;
-};
-
-&rk808 {
-	bootph-all;
-};
-
 &tcphy1 {
 	status = "okay";
 };
