From c55a7293d186c476de1d6245ae9804500157c4e8 Mon Sep 17 00:00:00 2001
From: Christian Hewitt <christianshewitt@gmail.com>
Date: Sat, 9 Apr 2022 06:21:58 +0000
Subject: [PATCH 63/64] WIP: arm64: dts: meson: add support for Venz V10

The Venz V10 is an Android STB based on the Amlogic P271 (GXLX)
reference design with an S905L chip and the following specs:

- 1GB DDR3 RAM
- 8GB eMMC
- 10/100 Base-T Ethernet
- RTL8189ES Wireless (802.11 b/g/n)
- HDMI 2.0b video
- 1x 3.5mm AV jack
- 2x USB 2.0 port
- IR receiver
- 1x Update/Reset button (underside)
- 1x micro SD card slot

Signed-off-by: Christian Hewitt <christianshewitt@gmail.com>
---
 arch/arm64/boot/dts/amlogic/Makefile          |   1 +
 .../dts/amlogic/meson-gxl-s905l-venz-v10.dts  | 325 ++++++++++++++++++
 2 files changed, 326 insertions(+)
 create mode 100644 arch/arm64/boot/dts/amlogic/meson-gxl-s905l-venz-v10.dts

diff --git a/arch/arm64/boot/dts/amlogic/Makefile b/arch/arm64/boot/dts/amlogic/Makefile
index b2f07ba0b342..a288f7c3c52a 100644
--- a/arch/arm64/boot/dts/amlogic/Makefile
+++ b/arch/arm64/boot/dts/amlogic/Makefile
@@ -88,3 +88,4 @@ dtb-$(CONFIG_ARCH_MESON) += meson-sm1-x96-air.dtb
 dtb-$(CONFIG_ARCH_MESON) += meson-gxbb-odroidc2-hifishield.dtb
 dtb-$(CONFIG_ARCH_MESON) += meson-gxl-s905l-p261.dtb
 dtb-$(CONFIG_ARCH_MESON) += meson-gxl-s905l-p271.dtb
+dtb-$(CONFIG_ARCH_MESON) += meson-gxl-s905l-venz-v10.dtb
diff --git a/arch/arm64/boot/dts/amlogic/meson-gxl-s905l-venz-v10.dts b/arch/arm64/boot/dts/amlogic/meson-gxl-s905l-venz-v10.dts
new file mode 100644
index 000000000000..30e799e608bb
--- /dev/null
+++ b/arch/arm64/boot/dts/amlogic/meson-gxl-s905l-venz-v10.dts
@@ -0,0 +1,325 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Copyright (c) 2016 Endless Computers, Inc.
+ * Author: Carlo Caione <carlo@endlessm.com>
+ */
+
+/dts-v1/;
+
+#include "meson-gxl-s905x.dtsi"
+#include <dt-bindings/gpio/gpio.h>
+#include <dt-bindings/leds/common.h>
+#include <dt-bindings/sound/meson-aiu.h>
+
+/ {
+	compatible = "venz,v10", "amlogic,s905l", "amlogic,meson-gxl";
+	model = "Venz V10";
+
+	aliases {
+		serial0 = &uart_AO;
+		ethernet0 = &ethmac;
+		wlan0 = &rtl8189;
+	};
+
+	chosen {
+		stdout-path = "serial0:115200n8";
+	};
+
+	memory@0 {
+		device_type = "memory";
+		reg = <0x0 0x0 0x0 0x80000000>;
+	};
+
+	dio2133: analog-amplifier {
+		compatible = "simple-audio-amplifier";
+		sound-name-prefix = "AU2";
+		VCC-supply = <&hdmi_5v>;
+		enable-gpios = <&gpio GPIOH_5 GPIO_ACTIVE_HIGH>;
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		led-standby {
+			color = <LED_COLOR_ID_BLUE>;
+			function = LED_FUNCTION_POWER;
+			gpios = <&gpio GPIODV_24 GPIO_ACTIVE_HIGH>;
+			default-state = "on";
+                };
+        };
+
+	cvbs-connector {
+		compatible = "composite-video-connector";
+
+		port {
+			cvbs_connector_in: endpoint {
+				remote-endpoint = <&cvbs_vdac_out>;
+			};
+		};
+	};
+
+	hdmi-connector {
+		compatible = "hdmi-connector";
+		type = "a";
+
+		port {
+			hdmi_connector_in: endpoint {
+				remote-endpoint = <&hdmi_tx_tmds_out>;
+			};
+		};
+	};
+
+	hdmi_5v: regulator-hdmi-5v {
+		compatible = "regulator-fixed";
+
+		regulator-name = "HDMI_5V";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+
+		gpio = <&gpio GPIOH_3 GPIO_ACTIVE_HIGH>;
+		enable-active-high;
+		regulator-always-on;
+	};
+
+	vddio_boot: regulator-vddio_boot {
+		compatible = "regulator-fixed";
+		regulator-name = "VDDIO_BOOT";
+		regulator-min-microvolt = <1800000>;
+		regulator-max-microvolt = <1800000>;
+	};
+
+	vddao_3v3: regulator-vddao_3v3 {
+		compatible = "regulator-fixed";
+		regulator-name = "VDDAO_3V3";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+	};
+
+	vddio_ao18: regulator-vddio_ao18 {
+		compatible = "regulator-fixed";
+		regulator-name = "VDDIO_AO18";
+		regulator-min-microvolt = <1800000>;
+		regulator-max-microvolt = <1800000>;
+	};
+
+	vcc_3v3: regulator-vcc_3v3 {
+		compatible = "regulator-fixed";
+		regulator-name = "VCC_3V3";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+	};
+
+	emmc_pwrseq: emmc-pwrseq {
+		compatible = "mmc-pwrseq-emmc";
+		reset-gpios = <&gpio BOOT_9 GPIO_ACTIVE_LOW>;
+	};
+
+	wifi32k: wifi32k {
+		compatible = "pwm-clock";
+		#clock-cells = <0>;
+		clock-frequency = <32768>;
+		pwms = <&pwm_ef 0 30518 0>; /* PWM_E at 32.768KHz */
+	};
+
+	sdio_pwrseq: sdio-pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		reset-gpios = <&gpio GPIOX_6 GPIO_ACTIVE_LOW>;
+		clocks = <&wifi32k>;
+		clock-names = "ext_clock";
+	};
+
+	sound {
+		compatible = "amlogic,gx-sound-card";
+		model = "VENZ-V10";
+		audio-aux-devs = <&dio2133>;
+		audio-widgets = "Line", "Lineout";
+		audio-routing = "AU2 INL", "ACODEC LOLN",
+				"AU2 INR", "ACODEC LORN",
+				"Lineout", "AU2 OUTL",
+				"Lineout", "AU2 OUTR";
+		assigned-clocks = <&clkc CLKID_MPLL0>,
+				  <&clkc CLKID_MPLL1>,
+				  <&clkc CLKID_MPLL2>;
+		assigned-clock-parents = <0>, <0>, <0>;
+		assigned-clock-rates = <294912000>,
+				       <270950400>,
+				       <393216000>;
+
+		dai-link-0 {
+			sound-dai = <&aiu AIU_CPU CPU_I2S_FIFO>;
+		};
+
+		dai-link-1 {
+			sound-dai = <&aiu AIU_CPU CPU_I2S_ENCODER>;
+			dai-format = "i2s";
+			mclk-fs = <256>;
+
+			codec-0 {
+				sound-dai = <&aiu AIU_HDMI CTRL_I2S>;
+			};
+
+			codec-1 {
+				sound-dai = <&aiu AIU_ACODEC CTRL_I2S>;
+			};
+		};
+
+		dai-link-2 {
+			sound-dai = <&aiu AIU_HDMI CTRL_OUT>;
+
+			codec-0 {
+				sound-dai = <&hdmi_tx>;
+			};
+		};
+
+		dai-link-3 {
+			sound-dai = <&aiu AIU_ACODEC CTRL_OUT>;
+
+			codec-0 {
+				sound-dai = <&acodec>;
+			};
+		};
+	};
+};
+
+&acodec {
+	AVDD-supply = <&vddio_ao18>;
+	status = "okay";
+};
+
+&aiu {
+	status = "okay";
+};
+
+&cec_AO {
+	status = "okay";
+	pinctrl-0 = <&ao_cec_pins>;
+	pinctrl-names = "default";
+	hdmi-phandle = <&hdmi_tx>;
+};
+
+&cvbs_vdac_port {
+	cvbs_vdac_out: endpoint {
+		remote-endpoint = <&cvbs_connector_in>;
+	};
+};
+
+&ethmac {
+	status = "okay";
+};
+
+&hdmi_tx {
+	status = "okay";
+	pinctrl-0 = <&hdmi_hpd_pins>, <&hdmi_i2c_pins>;
+	pinctrl-names = "default";
+	hdmi-supply = <&hdmi_5v>;
+};
+
+&hdmi_tx_tmds_port {
+	hdmi_tx_tmds_out: endpoint {
+		remote-endpoint = <&hdmi_connector_in>;
+	};
+};
+
+&ir {
+	status = "okay";
+	pinctrl-0 = <&remote_input_ao_pins>;
+	pinctrl-names = "default";
+	linux,rc-map-name = "rc-venz-v10";
+};
+
+&pwm_ef {
+	status = "okay";
+	pinctrl-0 = <&pwm_e_pins>;
+	pinctrl-names = "default";
+	clocks = <&clkc CLKID_FCLK_DIV4>;
+	clock-names = "clkin0";
+};
+
+&saradc {
+	status = "okay";
+	vref-supply = <&vddio_ao18>;
+};
+
+/* Wireless SDIO Module */
+&sd_emmc_a {
+	status = "okay";
+	pinctrl-0 = <&sdio_pins>;
+	pinctrl-1 = <&sdio_clk_gate_pins>;
+	pinctrl-names = "default", "clk-gate";
+	#address-cells = <1>;
+	#size-cells = <0>;
+
+	bus-width = <4>;
+	cap-sd-highspeed;
+	max-frequency = <100000000>;
+
+	non-removable;
+	disable-wp;
+
+	/* WiFi firmware requires power to be kept while in suspend */
+	keep-power-in-suspend;
+
+	mmc-pwrseq = <&sdio_pwrseq>;
+
+	vmmc-supply = <&vddao_3v3>;
+	vqmmc-supply = <&vddio_boot>;
+
+	rtl8189: wifi@1 {
+		reg = <1>;
+	};
+};
+
+/* SD card */
+&sd_emmc_b {
+	status = "okay";
+	pinctrl-0 = <&sdcard_pins>;
+	pinctrl-1 = <&sdcard_clk_gate_pins>;
+	pinctrl-names = "default", "clk-gate";
+
+	bus-width = <4>;
+	cap-sd-highspeed;
+	max-frequency = <50000000>;
+	disable-wp;
+
+	cd-gpios = <&gpio CARD_6 GPIO_ACTIVE_LOW>;
+
+	vmmc-supply = <&vddao_3v3>;
+	vqmmc-supply = <&vddio_boot>;
+};
+
+/* eMMC */
+&sd_emmc_c {
+	status = "okay";
+	pinctrl-0 = <&emmc_pins>, <&emmc_ds_pins>;
+	pinctrl-1 = <&emmc_clk_gate_pins>;
+	pinctrl-names = "default", "clk-gate";
+
+	bus-width = <8>;
+	cap-mmc-highspeed;
+	max-frequency = <200000000>;
+	non-removable;
+	disable-wp;
+	mmc-ddr-1_8v;
+	mmc-hs200-1_8v;
+
+	mmc-pwrseq = <&emmc_pwrseq>;
+	vmmc-supply = <&vcc_3v3>;
+	vqmmc-supply = <&vddio_boot>;
+};
+
+/* This UART is brought out to the DB9 connector */
+&uart_AO {
+	status = "okay";
+	pinctrl-0 = <&uart_ao_a_pins>;
+	pinctrl-names = "default";
+};
+
+&usb {
+	status = "okay";
+	dr_mode = "host";
+};
+
+&usb2_phy0 {
+	/* HDMI_5V is the supply for the USB VBUS */
+	phy-supply = <&hdmi_5v>;
+};
-- 
2.34.1

