From 96ab278661207096c013ad1b39ed36f5f9a35ffd Mon Sep 17 00:00:00 2001
From: Lucas Stach <l.stach@pengutronix.de>
Date: Tue, 13 Feb 2018 12:47:09 +0100
Subject: [PATCH 46/49] arm64: dts: fsl: imx8mq-evk: enable DCSS and HDMI

Signed-off-by: Lucas Stach <l.stach@pengutronix.de>
---
 arch/arm64/boot/dts/freescale/imx8mq-evk.dts | 22 ++++++++++++++++++++
 1 file changed, 22 insertions(+)

diff --git a/arch/arm64/boot/dts/freescale/imx8mq-evk.dts b/arch/arm64/boot/dts/freescale/imx8mq-evk.dts
index 2418cca00bc5..71eeda6de3d7 100644
--- a/arch/arm64/boot/dts/freescale/imx8mq-evk.dts
+++ b/arch/arm64/boot/dts/freescale/imx8mq-evk.dts
@@ -132,6 +132,16 @@ opp-800M {
 	};
 };
 
+&dcss {
+	status = "okay";
+
+	port {
+		dcss_out: endpoint {
+			remote-endpoint = <&hdmi_in>;
+		};
+	};
+};
+
 &dphy {
 	status = "okay";
 };
@@ -168,6 +178,18 @@ wl-reg-on-hog {
 	};
 };
 
+&hdmi {
+	compatible = "cdn,imx8mq-hdmi";
+	lane-mapping = <0xe4>;
+	status = "okay";
+
+	port {
+		hdmi_in: endpoint {
+			remote-endpoint = <&dcss_out>;
+		};
+	};
+};
+
 &i2c1 {
 	clock-frequency = <100000>;
 	pinctrl-names = "default";
-- 
2.29.2

