From 0327e9fc14269069711cd2d45d60130b318532fe Mon Sep 17 00:00:00 2001
From: Lucas Stach <l.stach@pengutronix.de>
Date: Tue, 13 Feb 2018 12:30:58 +0100
Subject: [PATCH 45/49] arm64: dts: fsl: imx8mq: add HDP bridge node

Signed-off-by: Lucas Stach <l.stach@pengutronix.de>
---
 arch/arm64/boot/dts/freescale/imx8mq.dtsi | 10 ++++++++++
 1 file changed, 10 insertions(+)

diff --git a/arch/arm64/boot/dts/freescale/imx8mq.dtsi b/arch/arm64/boot/dts/freescale/imx8mq.dtsi
index b75252a65c44..aad21d6f1da7 100644
--- a/arch/arm64/boot/dts/freescale/imx8mq.dtsi
+++ b/arch/arm64/boot/dts/freescale/imx8mq.dtsi
@@ -1103,6 +1103,16 @@ bus@32c00000 { /* AIPS4 */
 			#size-cells = <1>;
 			ranges = <0x32c00000 0x32c00000 0x400000>;
 
+			hdmi: hdmi@32c00000 {
+				reg = <0x32c00000 0x33800>,     /* HDP registers */
+				      <0x32e40000 0x40000>,     /* HDP SEC register */
+				      <0x32e2f000 0x10>;        /* RESET register */
+				interrupts = <GIC_SPI 16 IRQ_TYPE_LEVEL_HIGH>,
+				             <GIC_SPI 25 IRQ_TYPE_LEVEL_HIGH>;
+				interrupt-names = "plug_in", "plug_out";
+				status = "disabled";
+			};
+
 			dcss: display-controller@32e00000 {
 				compatible = "nxp,imx8mq-dcss";
 				reg = <0x32e00000 0x2d000>, <0x32e2f000 0x1000>;
-- 
2.29.2

