From 66f1e78fbe2a3d6726e90986a8ecc09098d3d3a6 Mon Sep 17 00:00:00 2001
From: Neil Armstrong <neil.armstrong@linaro.org>
Date: Thu, 9 Nov 2023 10:00:08 +0100
Subject: [PATCH 30/64] FROMLIST(v8): clk: meson: add vclk driver

The VCLK and VCLK_DIV clocks have supplementary bits.

The VCLK has a "SOFT RESET" bit to toggle after the whole
VCLK sub-tree rate has been set, this is implemented in
the gate enable callback.

The VCLK_DIV clocks as enable and reset bits used to disable
and reset the divider, associated with CLK_SET_RATE_GATE it ensures
the rate is set while the divider is disabled and in reset mode.

The VCLK_DIV enable bit isn't implemented as a gate since it's part
of the divider logic and vendor does this exact sequence to ensure
the divider is correctly set.

Signed-off-by: Neil Armstrong <neil.armstrong@linaro.org>
---
 drivers/clk/meson/Kconfig  |   5 ++
 drivers/clk/meson/Makefile |   1 +
 drivers/clk/meson/vclk.c   | 141 +++++++++++++++++++++++++++++++++++++
 drivers/clk/meson/vclk.h   |  51 ++++++++++++++
 4 files changed, 198 insertions(+)
 create mode 100644 drivers/clk/meson/vclk.c
 create mode 100644 drivers/clk/meson/vclk.h

diff --git a/drivers/clk/meson/Kconfig b/drivers/clk/meson/Kconfig
index 29ffd14d267b..59a40a49f8e1 100644
--- a/drivers/clk/meson/Kconfig
+++ b/drivers/clk/meson/Kconfig
@@ -30,6 +30,10 @@ config COMMON_CLK_MESON_VID_PLL_DIV
 	tristate
 	select COMMON_CLK_MESON_REGMAP
 
+config COMMON_CLK_MESON_VCLK
+	tristate
+	select COMMON_CLK_MESON_REGMAP
+
 config COMMON_CLK_MESON_CLKC_UTILS
 	tristate
 
@@ -140,6 +144,7 @@ config COMMON_CLK_G12A
 	select COMMON_CLK_MESON_EE_CLKC
 	select COMMON_CLK_MESON_CPU_DYNDIV
 	select COMMON_CLK_MESON_VID_PLL_DIV
+	select COMMON_CLK_MESON_VCLK
 	select MFD_SYSCON
 	help
 	  Support for the clock controller on Amlogic S905D2, S905X2 and S905Y2
diff --git a/drivers/clk/meson/Makefile b/drivers/clk/meson/Makefile
index 9ee4b954c896..9ba43fe7a07a 100644
--- a/drivers/clk/meson/Makefile
+++ b/drivers/clk/meson/Makefile
@@ -12,6 +12,7 @@ obj-$(CONFIG_COMMON_CLK_MESON_PLL) += clk-pll.o
 obj-$(CONFIG_COMMON_CLK_MESON_REGMAP) += clk-regmap.o
 obj-$(CONFIG_COMMON_CLK_MESON_SCLK_DIV) += sclk-div.o
 obj-$(CONFIG_COMMON_CLK_MESON_VID_PLL_DIV) += vid-pll-div.o
+obj-$(CONFIG_COMMON_CLK_MESON_VCLK) += vclk.o
 
 # Amlogic Clock controllers
 
diff --git a/drivers/clk/meson/vclk.c b/drivers/clk/meson/vclk.c
new file mode 100644
index 000000000000..47f08a52b49f
--- /dev/null
+++ b/drivers/clk/meson/vclk.c
@@ -0,0 +1,141 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * Copyright (c) 2023 Neil Armstrong <neil.armstrong@linaro.org>
+ */
+
+#include <linux/module.h>
+#include "vclk.h"
+
+/* The VCLK gate has a supplementary reset bit to pulse after ungating */
+
+static inline struct clk_regmap_vclk_data *
+clk_get_regmap_vclk_data(struct clk_regmap *clk)
+{
+	return (struct clk_regmap_vclk_data *)clk->data;
+}
+
+static int clk_regmap_vclk_enable(struct clk_hw *hw)
+{
+	struct clk_regmap *clk = to_clk_regmap(hw);
+	struct clk_regmap_vclk_data *vclk = clk_get_regmap_vclk_data(clk);
+
+	meson_parm_write(clk->map, &vclk->enable, 1);
+
+	/* Do a reset pulse */
+	meson_parm_write(clk->map, &vclk->reset, 1);
+	meson_parm_write(clk->map, &vclk->reset, 0);
+
+	return 0;
+}
+
+static void clk_regmap_vclk_disable(struct clk_hw *hw)
+{
+	struct clk_regmap *clk = to_clk_regmap(hw);
+	struct clk_regmap_vclk_data *vclk = clk_get_regmap_vclk_data(clk);
+
+	meson_parm_write(clk->map, &vclk->enable, 0);
+}
+
+static int clk_regmap_vclk_is_enabled(struct clk_hw *hw)
+{
+	struct clk_regmap *clk = to_clk_regmap(hw);
+	struct clk_regmap_vclk_data *vclk = clk_get_regmap_vclk_data(clk);
+
+	return meson_parm_read(clk->map, &vclk->enable);
+}
+
+const struct clk_ops clk_regmap_vclk_ops = {
+	.enable = clk_regmap_vclk_enable,
+	.disable = clk_regmap_vclk_disable,
+	.is_enabled = clk_regmap_vclk_is_enabled,
+};
+EXPORT_SYMBOL_GPL(clk_regmap_vclk_ops);
+
+/* The VCLK Divider has supplementary reset & enable bits */
+
+static inline struct clk_regmap_vclk_div_data *
+clk_get_regmap_vclk_div_data(struct clk_regmap *clk)
+{
+	return (struct clk_regmap_vclk_div_data *)clk->data;
+}
+
+static unsigned long clk_regmap_vclk_div_recalc_rate(struct clk_hw *hw,
+						     unsigned long prate)
+{
+	struct clk_regmap *clk = to_clk_regmap(hw);
+	struct clk_regmap_vclk_div_data *vclk = clk_get_regmap_vclk_div_data(clk);
+
+	return divider_recalc_rate(hw, prate, meson_parm_read(clk->map, &vclk->div),
+				   vclk->table, vclk->flags, vclk->div.width);
+}
+
+static int clk_regmap_vclk_div_determine_rate(struct clk_hw *hw,
+					      struct clk_rate_request *req)
+{
+	struct clk_regmap *clk = to_clk_regmap(hw);
+	struct clk_regmap_vclk_div_data *vclk = clk_get_regmap_vclk_div_data(clk);
+
+	return divider_determine_rate(hw, req, vclk->table, vclk->div.width,
+				      vclk->flags);
+}
+
+static int clk_regmap_vclk_div_set_rate(struct clk_hw *hw, unsigned long rate,
+					unsigned long parent_rate)
+{
+	struct clk_regmap *clk = to_clk_regmap(hw);
+	struct clk_regmap_vclk_div_data *vclk = clk_get_regmap_vclk_div_data(clk);
+	int ret;
+
+	ret = divider_get_val(rate, parent_rate, vclk->table, vclk->div.width,
+			      vclk->flags);
+	if (ret < 0)
+		return ret;
+
+	meson_parm_write(clk->map, &vclk->div, ret);
+
+	return 0;
+};
+
+static int clk_regmap_vclk_div_enable(struct clk_hw *hw)
+{
+	struct clk_regmap *clk = to_clk_regmap(hw);
+	struct clk_regmap_vclk_div_data *vclk = clk_get_regmap_vclk_div_data(clk);
+
+	/* Unreset the divider when ungating */
+	meson_parm_write(clk->map, &vclk->reset, 0);
+	meson_parm_write(clk->map, &vclk->enable, 1);
+
+	return 0;
+}
+
+static void clk_regmap_vclk_div_disable(struct clk_hw *hw)
+{
+	struct clk_regmap *clk = to_clk_regmap(hw);
+	struct clk_regmap_vclk_div_data *vclk = clk_get_regmap_vclk_div_data(clk);
+
+	/* Reset the divider when gating */
+	meson_parm_write(clk->map, &vclk->enable, 0);
+	meson_parm_write(clk->map, &vclk->reset, 1);
+}
+
+static int clk_regmap_vclk_div_is_enabled(struct clk_hw *hw)
+{
+	struct clk_regmap *clk = to_clk_regmap(hw);
+	struct clk_regmap_vclk_div_data *vclk = clk_get_regmap_vclk_div_data(clk);
+
+	return meson_parm_read(clk->map, &vclk->enable);
+}
+
+const struct clk_ops clk_regmap_vclk_div_ops = {
+	.recalc_rate = clk_regmap_vclk_div_recalc_rate,
+	.determine_rate = clk_regmap_vclk_div_determine_rate,
+	.set_rate = clk_regmap_vclk_div_set_rate,
+	.enable = clk_regmap_vclk_div_enable,
+	.disable = clk_regmap_vclk_div_disable,
+	.is_enabled = clk_regmap_vclk_div_is_enabled,
+};
+EXPORT_SYMBOL_GPL(clk_regmap_vclk_div_ops);
+
+MODULE_DESCRIPTION("Amlogic vclk clock driver");
+MODULE_AUTHOR("Neil Armstrong <neil.armstrong@linaro.org>");
+MODULE_LICENSE("GPL v2");
diff --git a/drivers/clk/meson/vclk.h b/drivers/clk/meson/vclk.h
new file mode 100644
index 000000000000..4f25d7ad2717
--- /dev/null
+++ b/drivers/clk/meson/vclk.h
@@ -0,0 +1,51 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (c) 2023 Neil Armstrong <neil.armstrong@linaro.org>
+ */
+
+#ifndef __VCLK_H
+#define __VCLK_H
+
+#include "clk-regmap.h"
+#include "parm.h"
+
+/**
+ * struct clk_regmap_vclk_data - vclk regmap backed specific data
+ *
+ * @enable:	vclk enable field
+ * @reset:	vclk reset field
+ * @flags:	hardware-specific flags
+ *
+ * Flags:
+ * Same as clk_gate except CLK_GATE_HIWORD_MASK which is ignored
+ */
+struct clk_regmap_vclk_data {
+	struct parm enable;
+	struct parm reset;
+	u8 flags;
+};
+
+extern const struct clk_ops clk_regmap_vclk_ops;
+
+/**
+ * struct clk_regmap_vclk_div_data - vclk_div regmap back specific data
+ *
+ * @div:	divider field
+ * @enable:	vclk divider enable field
+ * @reset:	vclk divider reset field
+ * @table:	array of value/divider pairs, last entry should have div = 0
+ *
+ * Flags:
+ * Same as clk_divider except CLK_DIVIDER_HIWORD_MASK which is ignored
+ */
+struct clk_regmap_vclk_div_data {
+	struct parm div;
+	struct parm enable;
+	struct parm reset;
+	const struct clk_div_table *table;
+	u8 flags;
+};
+
+extern const struct clk_ops clk_regmap_vclk_div_ops;
+
+#endif /* __VCLK_H */
-- 
2.34.1

