From e2dfeecc7473e47a20c14814ff4d0cfdcb85fea3 Mon Sep 17 00:00:00 2001
From: Neil Armstrong <neil.armstrong@linaro.org>
Date: Thu, 9 Nov 2023 10:00:10 +0100
Subject: [PATCH 32/64] FROMLIST(v8): drm/meson: gate px_clk when setting rate

Disable the px_clk when setting the rate to recover a fully
configured and correctly reset VCLK clock tree after the rate
is set.

Fixes: 77d9e1e6b846 ("drm/meson: add support for MIPI-DSI transceiver")
Signed-off-by: Neil Armstrong <neil.armstrong@linaro.org>
---
 drivers/gpu/drm/meson/meson_dw_mipi_dsi.c | 7 +++++++
 1 file changed, 7 insertions(+)

diff --git a/drivers/gpu/drm/meson/meson_dw_mipi_dsi.c b/drivers/gpu/drm/meson/meson_dw_mipi_dsi.c
index e5fe4e994f43..72abe2057ec3 100644
--- a/drivers/gpu/drm/meson/meson_dw_mipi_dsi.c
+++ b/drivers/gpu/drm/meson/meson_dw_mipi_dsi.c
@@ -95,6 +95,7 @@ static int dw_mipi_dsi_phy_init(void *priv_data)
 		return ret;
 	}
 
+	clk_disable_unprepare(mipi_dsi->px_clk);
 	ret = clk_set_rate(mipi_dsi->px_clk, mipi_dsi->mode->clock * 1000);
 
 	if (ret) {
@@ -103,6 +104,12 @@ static int dw_mipi_dsi_phy_init(void *priv_data)
 		return ret;
 	}
 
+	ret = clk_prepare_enable(mipi_dsi->px_clk);
+	if (ret) {
+		dev_err(mipi_dsi->dev, "Failed to enable DSI Pixel clock (ret %d)\n", ret);
+		return ret;
+	}
+
 	switch (mipi_dsi->dsi_device->format) {
 	case MIPI_DSI_FMT_RGB888:
 		dpi_data_format = DPI_COLOR_24BIT;
-- 
2.34.1

