From 7ae256c16de158201ec34e0ec7bacc24d713c7af Mon Sep 17 00:00:00 2001
From: Christian Hewitt <christianshewitt@gmail.com>
Date: Thu, 21 Jan 2021 01:35:36 +0000
Subject: [PATCH 06/36] LOCAL: arm64: dts: meson: add rtc/vrtc aliases to
 Khadas VIM

Add aliases to ensure the vrtc time (which normally proves first) is /dev/rtc1
while the onboard rtc chip claims /dev/rtc0.

Signed-off-by: Christian Hewitt <christianshewitt@gmail.com>
---
 arch/arm64/boot/dts/amlogic/meson-gxl-s905x-khadas-vim.dts | 2 ++
 1 file changed, 2 insertions(+)

diff --git a/arch/arm64/boot/dts/amlogic/meson-gxl-s905x-khadas-vim.dts b/arch/arm64/boot/dts/amlogic/meson-gxl-s905x-khadas-vim.dts
index a80f0ea2773b..0741d34945bb 100644
--- a/arch/arm64/boot/dts/amlogic/meson-gxl-s905x-khadas-vim.dts
+++ b/arch/arm64/boot/dts/amlogic/meson-gxl-s905x-khadas-vim.dts
@@ -29,6 +29,8 @@ button-function {
 	aliases {
 		serial2 = &uart_AO_B;
 		ethernet0 = &ethmac;
+		rtc0 = &rtc;
+		rtc1 = &vrtc;
 	};
 
 	gpio-keys-polled {
-- 
2.34.1

