From d12722830ea4f562e91586927ec21b64d0369544 Mon Sep 17 00:00:00 2001
From: Bitterblue Smith <rtl8821cerfe2@gmail.com>
Date: Wed, 23 Oct 2024 17:00:59 +0300
Subject: [PATCH] wifi: rtw88: Add some definitions for RTL8821AU/RTL8812AU

Add 8821A and 8812A chip type enums.

Add cck_high_power member to struct rtw_hal. This will be used to
calculate the RX signal strength of RTL8812AU.

Add various register definitions which will be used by the new drivers.

Move some existing register definitions from rtw8821c.h and rtw8822b.h.
They were duplicated in those headers and will also be used by the new
drivers.

Signed-off-by: Bitterblue Smith <rtl8821cerfe2@gmail.com>
Signed-off-by: Ping-Ke Shih <pkshih@realtek.com>
Link: https://patch.msgid.link/9279a9cd-6f86-4dc3-a095-7c36cb9b9d06@gmail.com
---
 drivers/net/wireless/realtek/rtw88/main.h     |   3 +
 drivers/net/wireless/realtek/rtw88/reg.h      | 174 ++++++++++++++++++
 drivers/net/wireless/realtek/rtw88/rtw8821c.h |  24 ---
 drivers/net/wireless/realtek/rtw88/rtw8822b.h |  12 --
 4 files changed, 177 insertions(+), 36 deletions(-)

diff --git a/drivers/net/wireless/realtek/rtw88/main.h b/drivers/net/wireless/realtek/rtw88/main.h
index 05cfb235f272..a2bef559cfb8 100644
--- a/drivers/net/wireless/realtek/rtw88/main.h
+++ b/drivers/net/wireless/realtek/rtw88/main.h
@@ -189,6 +189,8 @@ enum rtw_chip_type {
 	RTW_CHIP_TYPE_8723D,
 	RTW_CHIP_TYPE_8821C,
 	RTW_CHIP_TYPE_8703B,
+	RTW_CHIP_TYPE_8821A,
+	RTW_CHIP_TYPE_8812A,
 };
 
 enum rtw_tx_queue_type {
@@ -1934,6 +1936,7 @@ struct rtw_hal {
 	u32 antenna_rx;
 	u8 bfee_sts_cap;
 	bool txrx_1ss;
+	bool cck_high_power;
 
 	/* protect tx power section */
 	struct mutex tx_power_mutex;
diff --git a/drivers/net/wireless/realtek/rtw88/reg.h b/drivers/net/wireless/realtek/rtw88/reg.h
index 4d9b8668e8b0..e4d506cf9c33 100644
--- a/drivers/net/wireless/realtek/rtw88/reg.h
+++ b/drivers/net/wireless/realtek/rtw88/reg.h
@@ -9,6 +9,7 @@
 #define BIT_FEN_EN_25_1		BIT(13)
 #define BIT_FEN_ELDR		BIT(12)
 #define BIT_FEN_CPUEN		BIT(2)
+#define BIT_FEN_USBA		BIT(2)
 #define BIT_FEN_BB_GLB_RST	BIT(1)
 #define BIT_FEN_BB_RSTB		BIT(0)
 #define BIT_R_DIS_PRST		BIT(6)
@@ -16,6 +17,10 @@
 #define REG_SYS_PW_CTRL		0x0004
 #define BIT_PFM_WOWL		BIT(3)
 #define BIT_APFM_OFFMAC		BIT(9)
+#define REG_APS_FSMCO		0x0004
+#define APS_FSMCO_MAC_ENABLE	BIT(8)
+#define APS_FSMCO_MAC_OFF	BIT(9)
+#define APS_FSMCO_HW_POWERDOWN	BIT(15)
 #define REG_SYS_CLK_CTRL	0x0008
 #define BIT_CPU_CLK_EN		BIT(14)
 
@@ -58,6 +63,8 @@
 #define BIT_SHIFT_LDO25_VOLTAGE	4
 #define BIT_LDO25_EN		BIT(7)
 
+#define REG_ACLK_MON		0x3e
+
 #define REG_GPIO_MUXCFG		0x0040
 #define BIT_FSPI_EN		BIT(19)
 #define BIT_EN_SIC		BIT(12)
@@ -90,6 +97,8 @@
 #define BIT_USB_SUS_DIS		BIT(8)
 #define BIT_SDIO_PAD_E5		BIT(18)
 
+#define REG_RF_B_CTRL		0x76
+
 #define REG_AFE_CTRL_4		0x0078
 #define BIT_CK320M_AFE_EN	BIT(4)
 #define BIT_EN_SYN		BIT(15)
@@ -134,6 +143,11 @@
 #define REG_PMC_DBG_CTRL1	0xa8
 #define BITS_PMC_BT_IQK_STS	GENMASK(22, 21)
 
+#define REG_HIMR0		0xb0
+#define REG_HISR0		0xb4
+#define REG_HIMR1		0xb8
+#define REG_HISR1		0xbc
+
 #define REG_PAD_CTRL2		0x00C4
 #define BIT_RSM_EN_V1		BIT(16)
 #define BIT_NO_PDN_CHIPOFF_V1	BIT(17)
@@ -185,6 +199,15 @@
 #define MAC_TRX_ENABLE	(BIT_HCI_TXDMA_EN | BIT_HCI_RXDMA_EN | BIT_TXDMA_EN | \
 			BIT_RXDMA_EN | BIT_PROTOCOL_EN | BIT_SCHEDULE_EN | \
 			BIT_MACTXEN | BIT_MACRXEN)
+#define REG_PBP			0x104
+#define PBP_RX_MASK		0x0f
+#define PBP_TX_MASK		0xf0
+#define PBP_64			0x0
+#define PBP_128			0x1
+#define PBP_256			0x2
+#define PBP_512			0x3
+#define PBP_1024		0x4
+
 #define BIT_SHIFT_TXDMA_VOQ_MAP	4
 #define BIT_MASK_TXDMA_VOQ_MAP	0x3
 #define BIT_TXDMA_VOQ_MAP(x)                                                   \
@@ -256,6 +279,8 @@
 #define REG_HMEBOX1		0x01D4
 #define REG_HMEBOX2		0x01D8
 #define REG_HMEBOX3		0x01DC
+#define REG_LLT_INIT		0x01E0
+#define BIT_LLT_WRITE_ACCESS	BIT(30)
 #define REG_HMEBOX0_EX		0x01F0
 #define REG_HMEBOX1_EX		0x01F4
 #define REG_HMEBOX2_EX		0x01F8
@@ -298,6 +323,7 @@
 
 #define REG_AUTO_LLT		0x0224
 #define BIT_AUTO_INIT_LLT	BIT(16)
+#define REG_DWBCN1_CTRL		0x0228
 #define REG_RQPN_CTRL_1		0x0228
 #define REG_RQPN_CTRL_2		0x022C
 #define BIT_LD_RQPN		BIT(31)
@@ -329,6 +355,7 @@
 #define BIT_DMA_BURST_SIZE_1024	0
 
 #define REG_RXPKTNUM		0x02B0
+#define REG_EARLY_MODE_CONTROL	0x02BC
 
 #define REG_INT_MIG		0x0304
 #define REG_HCI_MIX_CFG		0x03FC
@@ -336,6 +363,7 @@
 
 #define REG_BCNQ_INFO		0x0418
 #define BIT_MGQ_CPU_EMPTY	BIT(24)
+#define REG_TXPKT_EMPTY		0x041A
 #define REG_FWHW_TXQ_CTRL	0x0420
 #define BIT_EN_BCNQ_DL		BIT(22)
 #define BIT_EN_WR_FREE_TAIL	BIT(20)
@@ -362,10 +390,12 @@
 #define REG_AMPDU_MAX_TIME_V1	0x0455
 #define REG_BCNQ1_BDNY_V1	0x0456
 #define REG_AMPDU_MAX_TIME	0x0456
+#define REG_AMPDU_MAX_LENGTH	0x0458
 #define REG_WMAC_LBK_BF_HD	0x045D
 #define REG_TX_HANG_CTRL	0x045E
 #define BIT_EN_GNT_BT_AWAKE	BIT(3)
 #define BIT_EN_EOF_V1		BIT(2)
+#define REG_FAST_EDCA_CTRL	0x0460
 #define REG_DATA_SC		0x0483
 #define REG_ARFR2_V1		0x048C
 #define REG_ARFRH2_V1		0x0490
@@ -390,6 +420,8 @@
 #define REG_PRECNT_CTRL		0x04E5
 #define BIT_BTCCA_CTRL		(BIT(0) | BIT(1))
 #define BIT_EN_PRECNT		BIT(11)
+#define REG_TX_RPT_CTRL		0x04EC
+#define REG_TX_RPT_TIME		0x04F0
 #define REG_DUMMY_PAGE4_V1	0x04FC
 
 #define REG_EDCA_VO_PARAM	0x0500
@@ -400,6 +432,7 @@
 #define BIT_MASK_CWMAX		GENMASK(15, 12)
 #define BIT_MASK_CWMIN		GENMASK(11, 8)
 #define BIT_MASK_AIFS		GENMASK(7, 0)
+#define REG_BCNTCFG		0x0510
 #define REG_PIFS		0x0512
 #define REG_SIFS		0x0514
 #define BIT_SHIFT_SIFS_OFDM_CTX	8
@@ -526,6 +559,8 @@
 #define REG_BT_COEX_V2		0x0762
 #define BIT_GNT_BT_POLARITY	BIT(12)
 #define BIT_LTE_COEX_EN		BIT(7)
+#define REG_GNT_BT		0x0765
+#define BIT_PTA_SW_CTL		GENMASK(4, 3)
 #define REG_BT_COEX_ENH_INTR_CTRL	0x76E
 #define BIT_R_GRANTALL_WLMASK	BIT(3)
 #define BIT_STATIS_BT_EN	BIT(2)
@@ -543,14 +578,43 @@
 #define REG_FPGA0_RFMOD		0x0800
 #define BIT_CCKEN		BIT(24)
 #define BIT_OFDMEN		BIT(25)
+#define REG_CCK_RPT_FORMAT	0x0804
+#define BIT_CCK_RPT_FORMAT	BIT(16)
+#define REG_RXPSEL		0x0808
+#define BIT_RX_PSEL_RST		(BIT(28) | BIT(29))
+#define REG_TXPSEL		0x080C
 #define REG_RX_GAIN_EN		0x081c
+#define REG_CCASEL		0x082C
+#define REG_PDMFTH		0x0830
+#define REG_BWINDICATION	0x0834
+#define REG_CCA2ND		0x0838
+#define REG_L1PKTH		0x0848
+#define REG_CLKTRK		0x0860
+#define REG_ADCCLK		0x08AC
+#define REG_HSSI_READ		0x08B0
+#define REG_FPGA0_XCD_RF_PARA	0x08B4
+#define REG_RX_MCS_LIMIT	0x08BC
+#define REG_ADC160		0x08C4
+#define REG_ANTSEL_SW		0x0900
+#define REG_DAC_RSTB		0x090c
+#define REG_SINGLE_TONE_CONT_TX	0x0914
 
 #define REG_RFE_CTRL_E		0x0974
 #define REG_2ND_CCA_CTRL	0x0976
+#define REG_IQK_COM00		0x0978
+#define REG_IQK_COM32		0x097c
+#define REG_IQK_COM64		0x0980
+#define REG_IQK_COM96		0x0984
+
+#define REG_FAS			0x09a4
+#define REG_RXSB		0x0a00
+#define REG_CCK_RX		0x0a04
+#define REG_CCK_PD_TH		0x0a0a
 
 #define REG_CCK0_FAREPORT	0xa2c
 #define BIT_CCK0_2RX		BIT(18)
 #define BIT_CCK0_MRC		BIT(22)
+#define REG_FA_CCK		0x0a5c
 
 #define REG_DIS_DPD		0x0a70
 #define DIS_DPD_MASK		GENMASK(9, 0)
@@ -566,13 +630,109 @@
 #define DIS_DPD_RATEVHT2SS_MCS1	BIT(9)
 #define DIS_DPD_RATEALL		GENMASK(9, 0)
 
+#define REG_CNTRST		0x0b58
+
+#define REG_3WIRE_SWA		0x0c00
+#define REG_RX_IQC_AB_A		0x0c10
+#define REG_TXSCALE_A		0x0c1c
+#define BB_SWING_MASK		GENMASK(31, 21)
+#define REG_TX_AGC_A_CCK_11_CCK_1		0xc20
+#define REG_TX_AGC_A_OFDM18_OFDM6		0xc24
+#define REG_TX_AGC_A_OFDM54_OFDM24		0xc28
+#define REG_TX_AGC_A_MCS3_MCS0			0xc2c
+#define REG_TX_AGC_A_MCS7_MCS4			0xc30
+#define REG_TX_AGC_A_MCS11_MCS8			0xc34
+#define REG_TX_AGC_A_MCS15_MCS12		0xc38
+#define REG_TX_AGC_A_NSS1_INDEX3_NSS1_INDEX0	0xc3c
+#define REG_TX_AGC_A_NSS1_INDEX7_NSS1_INDEX4	0xc40
+#define REG_TX_AGC_A_NSS2_INDEX1_NSS1_INDEX8	0xc44
+#define REG_TX_AGC_A_NSS2_INDEX5_NSS2_INDEX2	0xc48
+#define REG_TX_AGC_A_NSS2_INDEX9_NSS2_INDEX6	0xc4c
+#define REG_RXIGI_A		0x0c50
+#define REG_TX_PWR_TRAINING_A	0x0c54
+#define REG_CK_MONHA		0x0c5c
+#define REG_AFE_PWR1_A		0x0c60
+#define REG_AFE_PWR2_A		0x0c64
+#define REG_RX_WAIT_CCA_TX_CCK_RFON_A	0x0c68
+#define REG_OFDM0_XA_TX_IQ_IMBALANCE	0x0c80
+#define REG_OFDM0_A_TX_AFE	0x0c84
+#define REG_OFDM0_XB_TX_IQ_IMBALANCE	0x0c88
+#define REG_TSSI_TRK_SW		0x0c8c
+#define REG_LSSI_WRITE_A	0x0c90
+#define REG_PREDISTA		0x0c90
+#define REG_TXAGCIDX		0x0c94
+
+#define REG_RFE_PINMUX_A	0x0cb0
+#define REG_RFE_INV_A		0x0cb4
 #define REG_RFE_CTRL8		0x0cb4
 #define BIT_MASK_RFE_SEL89	GENMASK(7, 0)
+#define PTA_CTRL_PIN		0x66
+#define DPDT_CTRL_PIN		0x77
+#define RFE_INV_MASK		0x3ff00000
+#define REG_RFECTL_A		0x0cb8
 #define REG_RFE_INV8		0x0cbd
 #define BIT_MASK_RFE_INV89	GENMASK(1, 0)
 #define REG_RFE_INV16		0x0cbe
 #define BIT_RFE_BUF_EN		BIT(3)
 
+#define REG_IQK_DPD_CFG		0x0cc4
+#define REG_CFG_PMPD		0x0cc8
+#define REG_IQC_Y		0x0ccc
+#define REG_IQC_X		0x0cd4
+#define REG_INTPO_SETA		0x0ce8
+
+#define REG_IQKA_END		0x0d00
+#define REG_PI_READ_A		0x0d04
+#define REG_SI_READ_A		0x0d08
+#define REG_IQKB_END		0x0d40
+#define REG_PI_READ_B		0x0d44
+#define REG_SI_READ_B		0x0d48
+
+#define REG_3WIRE_SWB		0x0e00
+#define REG_RX_IQC_AB_B		0x0e10
+#define REG_TXSCALE_B		0x0e1c
+#define REG_TX_AGC_B_CCK_11_CCK_1		0xe20
+#define REG_TX_AGC_B_OFDM18_OFDM6		0xe24
+#define REG_TX_AGC_B_OFDM54_OFDM24		0xe28
+#define REG_TX_AGC_B_MCS3_MCS0			0xe2c
+#define REG_TX_AGC_B_MCS7_MCS4			0xe30
+#define REG_TX_AGC_B_MCS11_MCS8			0xe34
+#define REG_TX_AGC_B_MCS15_MCS12		0xe38
+#define REG_TX_AGC_B_NSS1_INDEX3_NSS1_INDEX0	0xe3c
+#define REG_TX_AGC_B_NSS1_INDEX7_NSS1_INDEX4	0xe40
+#define REG_TX_AGC_B_NSS2_INDEX1_NSS1_INDEX8	0xe44
+#define REG_TX_AGC_B_NSS2_INDEX5_NSS2_INDEX2	0xe48
+#define REG_TX_AGC_B_NSS2_INDEX9_NSS2_INDEX6	0xe4c
+#define REG_RXIGI_B		0x0e50
+#define REG_TX_PWR_TRAINING_B	0x0e54
+#define REG_CK_MONHB		0x0e5c
+#define REG_AFE_PWR1_B		0x0e60
+#define REG_AFE_PWR2_B		0x0e64
+#define REG_RX_WAIT_CCA_TX_CCK_RFON_B	0x0e68
+#define REG_TXTONEB		0x0e80
+#define REG_RXTONEB		0x0e84
+#define REG_TXPITMB		0x0e88
+#define REG_RXPITMB		0x0e8c
+#define REG_LSSI_WRITE_B	0x0e90
+#define REG_PREDISTB		0x0e90
+#define REG_INIDLYB		0x0e94
+#define REG_RFE_PINMUX_B	0x0eb0
+#define REG_RFE_INV_B		0x0eb4
+#define REG_RFECTL_B		0x0eb8
+#define REG_BPBDB		0x0ec4
+#define REG_PHYTXONB		0x0ec8
+#define REG_IQKYB		0x0ecc
+#define REG_IQKXB		0x0ed4
+#define REG_INTPO_SETB		0x0ee8
+
+#define REG_CRC_CCK		0x0f04
+#define REG_CCA_OFDM		0x0f08
+#define REG_CRC_VHT		0x0f0c
+#define REG_CRC_HT		0x0f10
+#define REG_CRC_OFDM		0x0f14
+#define REG_FA_OFDM		0x0f48
+#define REG_CCA_CCK		0x0fcc
+
 #define REG_ANAPARSW_MAC_0	0x1010
 #define BIT_CF_L_V2		GENMASK(29, 28)
 
@@ -709,6 +869,10 @@
 
 #define REG_IGN_GNTBT4	0x4160
 
+#define REG_USB_MOD	0xf008
+#define REG_USB3_RXITV	0xf050
+#define REG_USB_HRPWM	0xfe58
+
 #define RF_MODE		0x00
 #define RF_MODOPT	0x01
 #define RF_WLINT	0x01
@@ -716,7 +880,13 @@
 #define RF_DTXLOK	0x08
 #define RF_CFGCH	0x18
 #define BIT_BAND	GENMASK(18, 16)
+#define RF18_BAND_MASK	(BIT(16) | BIT(9) | BIT(8))
+#define RF18_CHANNEL_MASK	(MASKBYTE0)
+#define RF18_RFSI_MASK	(BIT(18) | BIT(17))
 #define RF_RCK		0x1d
+#define RF_MODE_TABLE_ADDR	0x30
+#define RF_MODE_TABLE_DATA0	0x31
+#define RF_MODE_TABLE_DATA1	0x32
 #define RF_LUTWA	0x33
 #define RF_LUTWD1	0x3e
 #define RF_LUTWD0	0x3f
@@ -725,10 +895,14 @@
 #define RF_T_METER	0x42
 #define RF_BSPAD	0x54
 #define RF_GAINTX	0x56
+#define RF_TXMOD	0x58
 #define RF_TXATANK	0x64
+#define RF_TXA_PREPAD	0x65
 #define RF_TRXIQ	0x66
 #define RF_RXIQGEN	0x8d
+#define RF_RXBB2	0x8f
 #define RF_SYN_PFD	0xb0
+#define RF_LCK		0xb4
 #define RF_XTALX2	0xb8
 #define RF_SYN_CTRL	0xbb
 #define RF_MALSEL	0xbe
diff --git a/drivers/net/wireless/realtek/rtw88/rtw8821c.h b/drivers/net/wireless/realtek/rtw88/rtw8821c.h
index 91ed921407bb..7a33ebd612ed 100644
--- a/drivers/net/wireless/realtek/rtw88/rtw8821c.h
+++ b/drivers/net/wireless/realtek/rtw88/rtw8821c.h
@@ -214,19 +214,10 @@ extern const struct rtw_chip_info rtw8821c_hw_spec;
 #define BIT_FEN_EN	BIT(26)
 #define REG_INIRTS_RATE_SEL 0x0480
 #define REG_HTSTFWT	0x800
-#define REG_RXPSEL	0x808
-#define BIT_RX_PSEL_RST		(BIT(28) | BIT(29))
-#define REG_TXPSEL	0x80c
 #define REG_RXCCAMSK	0x814
-#define REG_CCASEL	0x82c
-#define REG_PDMFTH	0x830
-#define REG_CCA2ND	0x838
 #define REG_L1WT	0x83c
 #define REG_L1PKWT	0x840
 #define REG_MRC		0x850
-#define REG_CLKTRK	0x860
-#define REG_ADCCLK	0x8ac
-#define REG_ADC160	0x8c4
 #define REG_ADC40	0x8c8
 #define REG_CHFIR	0x8f0
 #define REG_CDDTXP	0x93c
@@ -234,14 +225,11 @@ extern const struct rtw_chip_info rtw8821c_hw_spec;
 #define REG_ACBB0	0x948
 #define REG_ACBBRXFIR	0x94c
 #define REG_ACGG2TBL	0x958
-#define REG_FAS		0x9a4
-#define REG_RXSB	0xa00
 #define REG_ADCINI	0xa04
 #define REG_PWRTH	0xa08
 #define REG_CCA_FLTR	0xa20
 #define REG_TXSF2	0xa24
 #define REG_TXSF6	0xa28
-#define REG_FA_CCK	0xa5c
 #define REG_RXDESC	0xa2c
 #define REG_ENTXCCK	0xa80
 #define BTG_LNA		0xfc84
@@ -252,12 +240,8 @@ extern const struct rtw_chip_info rtw8821c_hw_spec;
 #define REG_PWRTH2	0xaa8
 #define REG_CSRATIO	0xaaa
 #define REG_TXFILTER	0xaac
-#define REG_CNTRST	0xb58
 #define REG_AGCTR_A	0xc08
-#define REG_TXSCALE_A	0xc1c
 #define REG_TXDFIR	0xc20
-#define REG_RXIGI_A	0xc50
-#define REG_TXAGCIDX	0xc94
 #define REG_TRSW	0xca0
 #define REG_RFESEL0	0xcb0
 #define REG_RFESEL8	0xcb4
@@ -269,14 +253,6 @@ extern const struct rtw_chip_info rtw8821c_hw_spec;
 #define B_WLA_SWITCH	BIT(23)
 #define REG_RFEINV	0xcbc
 #define REG_AGCTR_B	0xe08
-#define REG_RXIGI_B	0xe50
-#define REG_CRC_CCK	0xf04
-#define REG_CRC_OFDM	0xf14
-#define REG_CRC_HT	0xf10
-#define REG_CRC_VHT	0xf0c
-#define REG_CCA_OFDM	0xf08
-#define REG_FA_OFDM	0xf48
-#define REG_CCA_CCK	0xfcc
 #define REG_DMEM_CTRL	0x1080
 #define BIT_WL_RST	BIT(16)
 #define REG_ANTWT	0x1904
diff --git a/drivers/net/wireless/realtek/rtw88/rtw8822b.h b/drivers/net/wireless/realtek/rtw88/rtw8822b.h
index cf85e63966a1..0514958fb57c 100644
--- a/drivers/net/wireless/realtek/rtw88/rtw8822b.h
+++ b/drivers/net/wireless/realtek/rtw88/rtw8822b.h
@@ -151,21 +151,12 @@ _rtw_write32s_mask(struct rtw_dev *rtwdev, u32 addr, u32 mask, u32 data)
 #define RTW8822B_EDCCA_MAX	0x7f
 #define RTW8822B_EDCCA_SRC_DEF	1
 #define REG_HTSTFWT	0x800
-#define REG_RXPSEL	0x808
-#define BIT_RX_PSEL_RST		(BIT(28) | BIT(29))
-#define REG_TXPSEL	0x80c
 #define REG_RXCCAMSK	0x814
-#define REG_CCASEL	0x82c
-#define REG_PDMFTH	0x830
-#define REG_CCA2ND	0x838
 #define REG_L1WT	0x83c
 #define REG_L1PKWT	0x840
 #define REG_MRC		0x850
-#define REG_CLKTRK	0x860
 #define REG_EDCCA_POW_MA	0x8a0
 #define BIT_MA_LEVEL	GENMASK(1, 0)
-#define REG_ADCCLK	0x8ac
-#define REG_ADC160	0x8c4
 #define REG_ADC40	0x8c8
 #define REG_EDCCA_DECISION	0x8dc
 #define BIT_EDCCA_OPTION	BIT(5)
@@ -176,7 +167,6 @@ _rtw_write32s_mask(struct rtw_dev *rtwdev, u32 addr, u32 mask, u32 data)
 #define REG_ACBB0	0x948
 #define REG_ACBBRXFIR	0x94c
 #define REG_ACGG2TBL	0x958
-#define REG_RXSB	0xa00
 #define REG_ADCINI	0xa04
 #define REG_TXSF2	0xa24
 #define REG_TXSF6	0xa28
@@ -184,14 +174,12 @@ _rtw_write32s_mask(struct rtw_dev *rtwdev, u32 addr, u32 mask, u32 data)
 #define REG_ENTXCCK	0xa80
 #define REG_AGCTR_A	0xc08
 #define REG_TXDFIR	0xc20
-#define REG_RXIGI_A	0xc50
 #define REG_TRSW	0xca0
 #define REG_RFESEL0	0xcb0
 #define REG_RFESEL8	0xcb4
 #define REG_RFECTL	0xcb8
 #define REG_RFEINV	0xcbc
 #define REG_AGCTR_B	0xe08
-#define REG_RXIGI_B	0xe50
 #define REG_ANTWT	0x1904
 #define REG_IQKFAILMSK	0x1bf0
 
-- 
2.43.0

