# Use direct path to firmware as update script doesn't dereference sym links.
FIRMWARE_ROOT="/usr/lib/kernel-overlays/base/lib/firmware/raspberrypi/bootloader"
FIRMWARE_BACKUP_DIR="/storage/.config/rpifw-backup"
BOOTFS=${BOOTFS:-/flash}
