From c7999f0a3a7f275756a10a87849bb8fa47d315d3 Mon Sep 17 00:00:00 2001
From: Jernej Skrabec <jernej.skrabec@gmail.com>
Date: Mon, 9 Oct 2023 20:16:27 +0200
Subject: [PATCH 20/23] media: cedrus: Increase H6 clock rate

Vendor driver runs Cedrus at 648 MHz, supposedly to be able to decode
4k HEVC at 60 fps.

Signed-off-by: Jernej Skrabec <jernej.skrabec@gmail.com>
---
 drivers/staging/media/sunxi/cedrus/cedrus.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/drivers/staging/media/sunxi/cedrus/cedrus.c b/drivers/staging/media/sunxi/cedrus/cedrus.c
index 8e248d4a0aec..8d1ad841f66f 100644
--- a/drivers/staging/media/sunxi/cedrus/cedrus.c
+++ b/drivers/staging/media/sunxi/cedrus/cedrus.c
@@ -646,7 +646,7 @@ static const struct cedrus_variant sun50i_h6_cedrus_variant = {
 			  CEDRUS_CAPABILITY_H265_DEC |
 			  CEDRUS_CAPABILITY_H265_10_DEC |
 			  CEDRUS_CAPABILITY_VP8_DEC,
-	.mod_rate	= 600000000,
+	.mod_rate	= 648000000,
 };
 
 static const struct of_device_id cedrus_dt_match[] = {
-- 
2.42.0

