From fa93ac195068575da6bb5484bac9f95561d3f92c Mon Sep 17 00:00:00 2001
From: Bitterblue Smith <rtl8821cerfe2@gmail.com>
Date: Wed, 23 Oct 2024 17:15:13 +0300
Subject: [PATCH 17/24] wifi: rtw88: 8812a: Mitigate beacon loss

The RTL8812AU has a reception problem, maybe only in the 5 GHz band.
Sometimes, in some positions, it stops receiving anything even though
the distance to the AP is only ~3 meters and there are no obstacles.
Moving it a few centimeters fixes it.

Switch the initial gain to maximum coverage when there is beacon loss.
This only helps sometimes. This is similar to what the official driver
does.

Signed-off-by: Bitterblue Smith <rtl8821cerfe2@gmail.com>
Signed-off-by: Ping-Ke Shih <pkshih@realtek.com>
Link: https://patch.msgid.link/203f5043-4fe1-4f35-8b8f-d3b6f44e1fd9@gmail.com
---
 drivers/net/wireless/realtek/rtw88/phy.c | 7 +++++++
 1 file changed, 7 insertions(+)

diff --git a/drivers/net/wireless/realtek/rtw88/phy.c b/drivers/net/wireless/realtek/rtw88/phy.c
index b52108f2b147..40c36118f579 100644
--- a/drivers/net/wireless/realtek/rtw88/phy.c
+++ b/drivers/net/wireless/realtek/rtw88/phy.c
@@ -530,6 +530,13 @@ static void rtw_phy_dig(struct rtw_dev *rtwdev)
 	 */
 	rtw_phy_dig_recorder(dm_info, cur_igi, fa_cnt);
 
+	/* Mitigate beacon loss and connectivity issues, mainly (only?)
+	 * in the 5 GHz band
+	 */
+	if (rtwdev->chip->id == RTW_CHIP_TYPE_8812A && rtwdev->beacon_loss &&
+	    linked && dm_info->total_fa_cnt < DIG_PERF_FA_TH_EXTRA_HIGH)
+		cur_igi = DIG_CVRG_MIN;
+
 	if (cur_igi != pre_igi)
 		rtw_phy_dig_write(rtwdev, cur_igi);
 }
-- 
2.39.5

