From c5ccfb8981662498ead114cfc284c9d4f01ce78b Mon Sep 17 00:00:00 2001
From: Alex Bee <knaerzche@gmail.com>
Date: Tue, 18 Aug 2020 11:38:04 +0200
Subject: [PATCH 32/59] WIP/1001: arm64: dts: add resets to vdec for RK3399

---
 arch/arm64/boot/dts/rockchip/rk3399-base.dtsi | 5 +++++
 1 file changed, 5 insertions(+)

diff --git a/arch/arm64/boot/dts/rockchip/rk3399-base.dtsi b/arch/arm64/boot/dts/rockchip/rk3399-base.dtsi
index ec5ca40b2159..b031d77f3763 100644
--- a/arch/arm64/boot/dts/rockchip/rk3399-base.dtsi
+++ b/arch/arm64/boot/dts/rockchip/rk3399-base.dtsi
@@ -1463,6 +1463,11 @@ vdec: video-codec@ff660000 {
 		clock-names = "axi", "ahb", "cabac", "core";
 		iommus = <&vdec_mmu>;
 		power-domains = <&power RK3399_PD_VDU>;
+		resets = <&cru SRST_H_VDU>, <&cru SRST_A_VDU>,
+			 <&cru SRST_VDU_CORE>, <&cru SRST_VDU_CA>,
+			 <&cru SRST_A_VDU_NOC>, <&cru SRST_H_VDU_NOC>;
+		reset-names = "video_h", "video_a", "video_core", "video_cabac",
+			       "niu_a", "niu_h";
 	};
 
 	vdec_mmu: iommu@ff660480 {
-- 
2.34.1

