From 918d5d5a9a90d3c6e0f8920cec6818bd9d70eabf Mon Sep 17 00:00:00 2001
From: Bitterblue Smith <rtl8821cerfe2@gmail.com>
Date: Wed, 23 Oct 2024 17:06:14 +0300
Subject: [PATCH 05/24] wifi: rtw88: Allow different C2H RA report sizes

The RTL8821AU and RTL8812AU have smaller RA report size, only 4 bytes.
Avoid the "invalid ra report c2h length" error.

Also, use a struct and u8_get_bits() to access the RA report C2H.

Signed-off-by: Bitterblue Smith <rtl8821cerfe2@gmail.com>
Signed-off-by: Ping-Ke Shih <pkshih@realtek.com>
Link: https://patch.msgid.link/c3e73c3a-fb2f-4013-9f06-d5274211e282@gmail.com
---
 drivers/net/wireless/realtek/rtw88/fw.c       | 21 +++++++++++++------
 drivers/net/wireless/realtek/rtw88/fw.h       | 17 +++++++++++----
 drivers/net/wireless/realtek/rtw88/main.h     |  1 +
 drivers/net/wireless/realtek/rtw88/rtw8703b.c |  1 +
 drivers/net/wireless/realtek/rtw88/rtw8723d.c |  1 +
 drivers/net/wireless/realtek/rtw88/rtw8821c.c |  1 +
 drivers/net/wireless/realtek/rtw88/rtw8822b.c |  1 +
 drivers/net/wireless/realtek/rtw88/rtw8822c.c |  1 +
 8 files changed, 34 insertions(+), 10 deletions(-)

diff --git a/drivers/net/wireless/realtek/rtw88/fw.c b/drivers/net/wireless/realtek/rtw88/fw.c
index 813c12148819..168e19187ba7 100644
--- a/drivers/net/wireless/realtek/rtw88/fw.c
+++ b/drivers/net/wireless/realtek/rtw88/fw.c
@@ -139,25 +139,30 @@ static u16 get_max_amsdu_len(u32 bit_rate)
 struct rtw_fw_iter_ra_data {
 	struct rtw_dev *rtwdev;
 	u8 *payload;
+	u8 length;
 };
 
 static void rtw_fw_ra_report_iter(void *data, struct ieee80211_sta *sta)
 {
 	struct rtw_fw_iter_ra_data *ra_data = data;
+	struct rtw_c2h_ra_rpt *ra_rpt = (struct rtw_c2h_ra_rpt *)ra_data->payload;
 	struct rtw_sta_info *si = (struct rtw_sta_info *)sta->drv_priv;
 	u8 mac_id, rate, sgi, bw;
 	u8 mcs, nss;
 	u32 bit_rate;
 
-	mac_id = GET_RA_REPORT_MACID(ra_data->payload);
+	mac_id = ra_rpt->mac_id;
 	if (si->mac_id != mac_id)
 		return;
 
 	si->ra_report.txrate.flags = 0;
 
-	rate = GET_RA_REPORT_RATE(ra_data->payload);
-	sgi = GET_RA_REPORT_SGI(ra_data->payload);
-	bw = GET_RA_REPORT_BW(ra_data->payload);
+	rate = u8_get_bits(ra_rpt->rate_sgi, RTW_C2H_RA_RPT_RATE);
+	sgi = u8_get_bits(ra_rpt->rate_sgi, RTW_C2H_RA_RPT_SGI);
+	if (ra_data->length >= offsetofend(typeof(*ra_rpt), bw))
+		bw = ra_rpt->bw;
+	else
+		bw = si->bw_mode;
 
 	if (rate < DESC_RATEMCS0) {
 		si->ra_report.txrate.legacy = rtw_desc_to_bitrate(rate);
@@ -197,14 +202,18 @@ static void rtw_fw_ra_report_iter(void *data, struct ieee80211_sta *sta)
 static void rtw_fw_ra_report_handle(struct rtw_dev *rtwdev, u8 *payload,
 				    u8 length)
 {
+	struct rtw_c2h_ra_rpt *ra_rpt = (struct rtw_c2h_ra_rpt *)payload;
 	struct rtw_fw_iter_ra_data ra_data;
 
-	if (WARN(length < 7, "invalid ra report c2h length\n"))
+	if (WARN(length < rtwdev->chip->c2h_ra_report_size,
+		 "invalid ra report c2h length %d\n", length))
 		return;
 
-	rtwdev->dm_info.tx_rate = GET_RA_REPORT_RATE(payload);
+	rtwdev->dm_info.tx_rate = u8_get_bits(ra_rpt->rate_sgi,
+					      RTW_C2H_RA_RPT_RATE);
 	ra_data.rtwdev = rtwdev;
 	ra_data.payload = payload;
+	ra_data.length = length;
 	rtw_iterate_stas_atomic(rtwdev, rtw_fw_ra_report_iter, &ra_data);
 }
 
diff --git a/drivers/net/wireless/realtek/rtw88/fw.h b/drivers/net/wireless/realtek/rtw88/fw.h
index e999c24e4634..404de1b0c407 100644
--- a/drivers/net/wireless/realtek/rtw88/fw.h
+++ b/drivers/net/wireless/realtek/rtw88/fw.h
@@ -85,6 +85,19 @@ struct rtw_c2h_adaptivity {
 	u8 option;
 } __packed;
 
+struct rtw_c2h_ra_rpt {
+	u8 rate_sgi;
+	u8 mac_id;
+	u8 byte2;
+	u8 status;
+	u8 byte4;
+	u8 ra_ratio;
+	u8 bw;
+} __packed;
+
+#define RTW_C2H_RA_RPT_RATE	GENMASK(6, 0)
+#define RTW_C2H_RA_RPT_SGI	BIT(7)
+
 struct rtw_h2c_register {
 	u32 w0;
 	u32 w1;
@@ -364,10 +377,6 @@ struct rtw_fw_hdr_legacy {
 #define GET_CHAN_SWITCH_CENTRAL_CH(c2h_payload)	(c2h_payload[2])
 #define GET_CHAN_SWITCH_ID(c2h_payload)		(c2h_payload[3])
 #define GET_CHAN_SWITCH_STATUS(c2h_payload)	(c2h_payload[4])
-#define GET_RA_REPORT_RATE(c2h_payload)		(c2h_payload[0] & 0x7f)
-#define GET_RA_REPORT_SGI(c2h_payload)		((c2h_payload[0] & 0x80) >> 7)
-#define GET_RA_REPORT_BW(c2h_payload)		(c2h_payload[6])
-#define GET_RA_REPORT_MACID(c2h_payload)	(c2h_payload[1])
 
 #define GET_BCN_FILTER_NOTIFY_TYPE(c2h_payload)	(c2h_payload[1] & 0xf)
 #define GET_BCN_FILTER_NOTIFY_EVENT(c2h_payload)	(c2h_payload[1] & 0x10)
diff --git a/drivers/net/wireless/realtek/rtw88/main.h b/drivers/net/wireless/realtek/rtw88/main.h
index 95b5acf975c6..9f474dbed965 100644
--- a/drivers/net/wireless/realtek/rtw88/main.h
+++ b/drivers/net/wireless/realtek/rtw88/main.h
@@ -1201,6 +1201,7 @@ struct rtw_chip_info {
 
 	u8 usb_tx_agg_desc_num;
 	bool hw_feature_report;
+	u8 c2h_ra_report_size;
 
 	u8 default_1ss_tx_path;
 
diff --git a/drivers/net/wireless/realtek/rtw88/rtw8703b.c b/drivers/net/wireless/realtek/rtw88/rtw8703b.c
index c4793e10d9dc..e541443adb15 100644
--- a/drivers/net/wireless/realtek/rtw88/rtw8703b.c
+++ b/drivers/net/wireless/realtek/rtw88/rtw8703b.c
@@ -1961,6 +1961,7 @@ const struct rtw_chip_info rtw8703b_hw_spec = {
 	.ampdu_density = IEEE80211_HT_MPDU_DENSITY_16,
 	.usb_tx_agg_desc_num = 1, /* Not sure if this chip has USB interface */
 	.hw_feature_report = true,
+	.c2h_ra_report_size = 7,
 
 	.path_div_supported = false,
 	.ht_supported = true,
diff --git a/drivers/net/wireless/realtek/rtw88/rtw8723d.c b/drivers/net/wireless/realtek/rtw88/rtw8723d.c
index bf87c92087da..6a9115775faf 100644
--- a/drivers/net/wireless/realtek/rtw88/rtw8723d.c
+++ b/drivers/net/wireless/realtek/rtw88/rtw8723d.c
@@ -2132,6 +2132,7 @@ const struct rtw_chip_info rtw8723d_hw_spec = {
 	.dig_min = 0x20,
 	.usb_tx_agg_desc_num = 1,
 	.hw_feature_report = true,
+	.c2h_ra_report_size = 7,
 	.ht_supported = true,
 	.vht_supported = false,
 	.lps_deep_mode_supported = 0,
diff --git a/drivers/net/wireless/realtek/rtw88/rtw8821c.c b/drivers/net/wireless/realtek/rtw88/rtw8821c.c
index 44ef2e246724..6cb7e9aaa437 100644
--- a/drivers/net/wireless/realtek/rtw88/rtw8821c.c
+++ b/drivers/net/wireless/realtek/rtw88/rtw8821c.c
@@ -1969,6 +1969,7 @@ const struct rtw_chip_info rtw8821c_hw_spec = {
 	.dig_min = 0x1c,
 	.usb_tx_agg_desc_num = 3,
 	.hw_feature_report = true,
+	.c2h_ra_report_size = 7,
 	.ht_supported = true,
 	.vht_supported = true,
 	.lps_deep_mode_supported = BIT(LPS_DEEP_MODE_LCLK),
diff --git a/drivers/net/wireless/realtek/rtw88/rtw8822b.c b/drivers/net/wireless/realtek/rtw88/rtw8822b.c
index 3b25536a253e..ca8813fdf9fb 100644
--- a/drivers/net/wireless/realtek/rtw88/rtw8822b.c
+++ b/drivers/net/wireless/realtek/rtw88/rtw8822b.c
@@ -2512,6 +2512,7 @@ const struct rtw_chip_info rtw8822b_hw_spec = {
 	.dig_min = 0x1c,
 	.usb_tx_agg_desc_num = 3,
 	.hw_feature_report = true,
+	.c2h_ra_report_size = 7,
 	.ht_supported = true,
 	.vht_supported = true,
 	.lps_deep_mode_supported = BIT(LPS_DEEP_MODE_LCLK),
diff --git a/drivers/net/wireless/realtek/rtw88/rtw8822c.c b/drivers/net/wireless/realtek/rtw88/rtw8822c.c
index 936d4bf82c8f..ca98da8e4000 100644
--- a/drivers/net/wireless/realtek/rtw88/rtw8822c.c
+++ b/drivers/net/wireless/realtek/rtw88/rtw8822c.c
@@ -5331,6 +5331,7 @@ const struct rtw_chip_info rtw8822c_hw_spec = {
 	.dig_min = 0x20,
 	.usb_tx_agg_desc_num = 3,
 	.hw_feature_report = true,
+	.c2h_ra_report_size = 7,
 	.default_1ss_tx_path = BB_PATH_A,
 	.path_div_supported = true,
 	.ht_supported = true,
-- 
2.39.5

