From 6b9309988072e3b5b7b3900a1254507316eb72cf Mon Sep 17 00:00:00 2001
From: Lukas Rusak <lorusak@gmail.com>
Date: Tue, 9 Mar 2021 10:47:27 -0800
Subject: [PATCH 2/4] arm64: dts: fsl: imx8mq-pico-pi: enable DCSS and HDMI

Adapted for [PATCH v16] Initial support Cadence MHDP8501(HDMI/DP) for i.MX8MQ
Adapted for [PATCH v19] Initial support Cadence MHDP8501(HDMI/DP) for i.MX8MQ
---
 .../boot/dts/freescale/imx8mq-pico-pi.dts     | 31 +++++++++++++++++++
 1 file changed, 31 insertions(+)

diff --git a/arch/arm64/boot/dts/freescale/imx8mq-pico-pi.dts b/arch/arm64/boot/dts/freescale/imx8mq-pico-pi.dts
index 89cbec5c41b2..5e2b1a84a85e 100644
--- a/arch/arm64/boot/dts/freescale/imx8mq-pico-pi.dts
+++ b/arch/arm64/boot/dts/freescale/imx8mq-pico-pi.dts
@@ -54,6 +54,43 @@ ethphy0: ethernet-phy@1 {
 			reg = <1>;
 		};
 	};
+
+	hdmi_connector: connector {
+		compatible = "hdmi-connector";
+		label = "X11";
+		type = "a";
+
+		port {
+			hdmi_connector_in: endpoint {
+			};
+		};
+	};
+};
+
+&dcss {
+	status = "okay";
+};
+
+&hdmi_connector {
+	port {
+		hdmi_connector_in: endpoint {
+			remote-endpoint = <&mhdp_out>;
+		};
+	};
+};
+
+&mhdp {
+	status = "okay";
+	ports {
+		port@1 {
+			reg = <1>;
+
+			mhdp_out: endpoint {
+				remote-endpoint = <&hdmi_connector_in>;
+				data-lanes = <0 1 2 3>;
+			};
+		};
+	};
 };
 
 &i2c1 {
-- 
2.43.0

