From ebadcb81bd3167f9360cb86b92eee02a43a224b2 Mon Sep 17 00:00:00 2001
From: Bitterblue Smith <rtl8821cerfe2@gmail.com>
Date: Wed, 23 Oct 2024 17:13:10 +0300
Subject: [PATCH 13/24] wifi: rtw88: usb: Set pkt_info.ls for the reserved page

"ls" meaning "last segment". Without this RTL8812AU can't upload the
reserved page in USB 2 mode. (Somehow it's fine in USB 3 mode.)

Also tested with RTL8822CU, RTL8812BU, RTL8811CU, RTL8723DU, RTL8811AU.

Signed-off-by: Bitterblue Smith <rtl8821cerfe2@gmail.com>
Signed-off-by: Ping-Ke Shih <pkshih@realtek.com>
Link: https://patch.msgid.link/e443f5d9-4b53-4f64-985c-64313ec80bef@gmail.com
---
 drivers/net/wireless/realtek/rtw88/usb.c | 1 +
 1 file changed, 1 insertion(+)

diff --git a/drivers/net/wireless/realtek/rtw88/usb.c b/drivers/net/wireless/realtek/rtw88/usb.c
index a0ce3a306221..05025fed5b68 100644
--- a/drivers/net/wireless/realtek/rtw88/usb.c
+++ b/drivers/net/wireless/realtek/rtw88/usb.c
@@ -532,6 +532,7 @@ static int rtw_usb_write_data_rsvd_page(struct rtw_dev *rtwdev, u8 *buf,
 	pkt_info.tx_pkt_size = size;
 	pkt_info.qsel = TX_DESC_QSEL_BEACON;
 	pkt_info.offset = chip->tx_pkt_desc_sz;
+	pkt_info.ls = true;
 
 	return rtw_usb_write_data(rtwdev, &pkt_info, buf);
 }
-- 
2.39.5

