From patchwork Tue Dec 17 06:51:43 2024
Content-Type: text/plain; charset="utf-8"
MIME-Version: 1.0
Content-Transfer-Encoding: 7bit
Subject: [PATCH v20 0/8] Initial support Cadence MHDP8501(HDMI/DP) for i.MX8MQ
From: Sandor Yu <Sandor.yu@nxp.com>
Message-Id: <cover.1734340233.git.Sandor.yu@nxp.com>
To: dmitry.baryshkov@linaro.org, andrzej.hajda@intel.com,
 neil.armstrong@linaro.org, Laurent.pinchart@ideasonboard.com,
 jonas@kwiboo.se, jernej.skrabec@gmail.com, airlied@gmail.com,
 daniel@ffwll.ch, robh+dt@kernel.org, krzysztof.kozlowski+dt@linaro.org,
 shawnguo@kernel.org, s.hauer@pengutronix.de, festevam@gmail.com,
 vkoul@kernel.org, dri-devel@lists.freedesktop.org,
 devicetree@vger.kernel.org, linux-arm-kernel@lists.infradead.org,
 linux-kernel@vger.kernel.org, linux-phy@lists.infradead.org,
 mripard@kernel.org
Cc: kernel@pengutronix.de, linux-imx@nxp.com, Sandor.yu@nxp.com,
 oliver.brown@nxp.com, alexander.stein@ew.tq-group.com, sam@ravnborg.org
Date: Tue, 17 Dec 2024 14:51:42 +0800

The patch set initial support Cadence MHDP8501(HDMI/DP) DRM bridge
driver and Cadence HDP-TX PHY(HDMI/DP) driver for Freescale i.MX8MQ.

The patch set compose of DRM bridge drivers and PHY driver.

Both of them need by patch #1 and #3 to pass build.

DRM bridges driver patches:
  #1: soc: cadence: Create helper functions for Cadence MHDP
  #2: drm: bridge: cadence: Update mhdp8546 mailbox access functions
  #3: phy: Add HDMI configuration options
  #4: dt-bindings: display: bridge: Add Cadence MHDP8501
  #5: drm: bridge: Cadence: Add MHDP8501 DP/HDMI driver

PHY driver patches:
  #1: soc: cadence: Create helper functions for Cadence MHDP
  #3: phy: Add HDMI configuration options
  #6: dt-bindings: phy: Add Freescale iMX8MQ DP and HDMI PHY
  #7: phy: freescale: Add DisplayPort/HDMI Combo-PHY driver for i.MX8MQ

i.MX8M/TQMa8Mx DT patches:
  #8: Add DT nodes for DCSS/HDMI pipeline
  #9: Enable HDMI for TQMa8Mx/MBa8Mx

v19->v20:
Patch #1: soc: cadence: Create helper functions for Cadence MHDP
Patch #2: drm: bridge: cadence: Update mhdp8546 mailbox access functions
- The two patches are split from Patch #1 in v19.
  The MHDP helper functions have been moved in a new "cadence" directory
  under the SOC directory in patch #1, in order to promote code reuse
  among MHDP8546, MHDP8501, and the i.MX8MQ HDMI/DP PHY drivers,

Patch #3: phy: Add HDMI configuration options
- Add a-b tag

Patch #4: dt-bindings: display: bridge: Add Cadence MHDP8501
- remove data type link of data-lanes

Patch #5: drm: bridge: Cadence: Add MHDP8501 DP/HDMI driver
- Dump mhdp FW version by debugfs
- Combine HDMI and DP cable detect functions into one function
- Combine HDMI and DP cable bridge_mode_valid() functions into one function
- Rename cdns_hdmi_reset_link() to cdns_hdmi_handle_hotplug()
- Add comments for EDID in cdns_hdmi_handle_hotplug() and cdns_dp_check_link_state()
- Add atomic_get_input_bus_fmts() and bridge_atomic_check() for DP driver
- Remove bpc and color_fmt init in atomic_enable() function.
- More detail comments for DDC adapter only support SCDC_I2C_SLAVE_ADDRESS
  read and write in HDMI driver.

Patch #7: phy: freescale: Add DisplayPort/HDMI Combo-PHY driver for i.MX8MQ
- implify DP configuration handling by directly copying
  the configuration options to the driver's internal structure.
- return the error code directly instead of logging an error message in `hdptx_clk_enable`
- Remove redundant ref_clk_rate check


v18->v19:
Patch #1
- use guard(mutex)
- Add kerneldocs for all new APIs.
- Detail comments for mailbox access specific case.
- remove cdns_mhdp_dp_reg_write() because it is not needed by driver now.

Patch #3
- move property data-lanes to endpoint of port@1

Patch #4
- get endpoint for data-lanes as it had move to endpoint of port@1
- update clock management as devm_clk_get_enabled() introduced.
- Fix clear_infoframe() function is not work issue.
- Manage PHY power state via phy_power_on() and phy_power_off().

Patch #6
- Simplify the PLL table by removing unused and constant data
- Remove PHY power management, controller driver will handle them.
- Remove enum dp_link_rate
- introduce read_pll_timeout.
- update clock management as devm_clk_get_enabled() introduced.
- remove cdns_hdptx_phy_init() and cdns_hdptx_phy_remove().

Patch #8:
- move property data-lanes to endpoint of port@1

v17->v18:
Patch #1
- Create three ordinary mailbox access APIs
    cdns_mhdp_mailbox_send
    cdns_mhdp_mailbox_send_recv
    cdns_mhdp_mailbox_send_recv_multi
- Create three secure mailbox access APIs
    cdns_mhdp_secure_mailbox_send
    cdns_mhdp_secure_mailbox_send_recv
    cdns_mhdp_secure_mailbox_send_recv_multi
- MHDP8546 DP and HDCP commands that need access mailbox are rewrited
  with above 6 API functions.

Patch #3
- remove lane-mapping and replace it with data-lanes
- remove r-b tag as property changed.

Patch #4
- MHDP8501 HDMI and DP commands that need access mailbox are rewrited
  with new API functions created in patch #1.
- replace lane-mapping with data-lanes, use the value from data-lanes
  to reorder HDMI and DP lane mapping.
- create I2C adapter for HDMI SCDC, remove cdns_hdmi_scdc_write() function.
- Rewrite cdns_hdmi_sink_config() function, use HDMI SCDC helper function
  drm_scdc_set_high_tmds_clock_ratio() and drm_scdc_set_scrambling()
  to config HDMI sink TMDS.
- Remove struct video_info from HDMI driver.
- Remove tmds_char_rate_valid() be called in bridge_mode_valid(),
  community had patch in reviewing to implement the function.
- Remove warning message print when get unknown HPD cable status.
- Add more detail comments for HDP plugin and plugout interrupt.
- use dev_dbg to repleace DRM_INFO when cable HPD status changed.
- Remove t-b tag as above code change.

Patch #6
- fix build error as code rebase to latest kernel version.

Patch #8:
- replace lane-mapping with data-lanes


v16->v17:
Patch #1:
- Replaces the local mutex mbox_mutex with a global mutex mhdp_mailbox_mutex
Patch #2:
- remove hdmi.h
- add 2024 year to copyright
- Add r-b tag.
Patch #3:
- Add lane-mapping property.
Patch #4:
- Reset the HDMI/DP link when an HPD (Hot Plug Detect) event is detected
- Move the HDMI protocol settings from hdmi_ctrl_init() to a new function
  cdns_hdmi_set_hdmi_mode_type(), to align with the introduced link reset functionality.
- Implement logic to check the type of HDMI sink.
  If the sink is not a hdmi display, set the default mode to DVI.
- Implement hdmi_reset_infoframe function
- Reorder certain bit definitions in the header file to follow a descending order.
- Add "lane-mapping" property for both HDMI and DP, remove platform data from driver.
  lane-mapping should be setting in dts according different board layout.
- Remove variable mode in struct cdns_mhdp8501_device, video mode could get from struct drm_crtc_state
- Remove variable char_rate in  struct cdns_mhdp8501_device, it could get from struct struct drm_connector_state.hdmi
- Replaces the local mutex mbox_mutex with a global mutex mhdp_mailbox_mutex
- Remove mutext protect for phy_api access functions.
Patch #6:
- Remove mbox_mutex

v15->v16:
Patch #2:
- Remove pixel_clk_rate, bpc and color_space fields from struct
  phy_configure_opts_hdmi, they were replaced by
  unsigned long long tmds_char_rate.
- Remove r-b and a-c tags because this patch have important change.
Patch #4:
- Add DRM_BRIDGE_OP_HDMI flags for HDMI driver,
- Introduce the hdmi info frame helper functions,
  added hdmi_clear_infoframe(), hdmi_write_infoframe() and
  hdmi_tmds_char_rate_valid() according Dmitry's patch
  'make use of the HDMI connector infrastructure' patchset ([2]).
- mode_fixup() is replaced by atomic_check().
- Fix video mode 4Kp30 did not work on some displays that support
  LTE_340Mcsc_scramble.
- updated for tmds_char_rate added in patch #2. 
Patch #6:
- updated for tmds_char_rate added in patch #2. 

v14->v15:
Patch #6 + #7:
-  Merged PHY driver into a single combo PHY driver
Patch #7 + #8:
- Add DT patches for a running HDMI setup

v13->v14:
Patch #4:
- Rebase to next-20240219, replace get_edid function by edid_read
  function as commits d807ad80d811b ("drm/bridge: add ->edid_read
  hook and drm_bridge_edid_read()") and 27b8f91c08d99 ("drm/bridge:
  remove ->get_edid callback") had change the API.

v12->v13:
Patch #4:
- Explicitly include linux/platform_device.h for cdns-mhdp8501-core.c
- Fix build warning
- Order bit bpc and color_space in descending shit. 
Patch #7:
- Fix build warning

v11->v12:
Patch #1: 
- Move status initialize out of mbox_mutex.
- Reorder API functions in alphabetical.
- Add notes for malibox access functions.
- Add year 2024 to copyright.
Patch #4:
- Replace DRM_INFO with dev_info or dev_warn.
- Replace DRM_ERROR with dev_err.
- Return ret when cdns_mhdp_dpcd_read failed in function cdns_dp_aux_transferi().
- Remove unused parmeter in function cdns_dp_get_msa_misc
  and use two separate variables for color space and bpc.
- Add year 2024 to copyright.
Patch #6:
- Return error code to replace -1 for function wait_for_ack().
- Set cdns_phy->power_up = false in phy_power_down function.
- Remove "RATE_8_1 = 810000", it is not used in driver.
- Add year 2024 to copyright.
Patch #7:
- Adjust clk disable order.
- Return error code to replace -1 for function wait_for_ack().
- Use bool for variable pclk_in.
- Add year 2024 to copyright.

v10->v11:
- rewrite cdns_mhdp_set_firmware_active() in mhdp8546 core driver,
use cdns_mhdp_mailbox_send() to replace cdns_mhdp_mailbox_write()
same as the other mailbox access functions.
- use static for cdns_mhdp_mailbox_write() and cdns_mhdp_mailbox_read()
and remove them from EXPORT_SYMBOL_GPL().
- remove MODULE_ALIAS() from mhdp8501 driver.

v9->v10:
- Create mhdp helper driver to replace macro functions,
move all mhdp mailbox access functions and common functions
into the helper driver.
Patch #1:drm: bridge: Cadence: Creat mhdp helper driver
it is totaly different with v9.

v8->v9:
- Remove compatible string "cdns,mhdp8501" that had removed
  from dt-bindings file in v8.
- Add Dmitry's R-b tag to patch #2
- Add Krzysztof's R-b tag to patch #3

v7->v8:
MHDP8501 HDMI/DP:
- Correct DT node name to "display-bridge".
- Remove "cdns,mhdp8501" from mhdp8501 dt-binding doc.

HDMI/DP PHY:
- Introduced functions `wait_for_ack` and `wait_for_ack_clear` to handle
  waiting with acknowledgment bits set and cleared respectively.
- Use FIELD_PRE() to set bitfields for both HDMI and DP PHY.

v6->v7:
MHDP8501 HDMI/DP:
- Combine HDMI and DP driver into one mhdp8501 driver.
  Use the connector type to load the corresponding functions.
- Remove connector init functions.
- Add <linux/hdmi.h> in phy_hdmi.h to reuse 'enum hdmi_colorspace'.

HDMI/DP PHY:
- Lowercase hex values
- Fix parameters indent issue on some functions
- Replace 'udelay' with 'usleep_range'

v5->v6:
HDMI/DP bridge driver
- 8501 is the part number of Cadence MHDP on i.MX8MQ.
  Use MHDP8501 to name hdmi/dp drivers and files. 
- Add compatible "fsl,imx8mq-mhdp8501-dp" for i.MX8MQ DP driver
- Add compatible "fsl,imx8mq-mhdp8501-hdmi" for i.MX8MQ HDMI driver
- Combine HDMI and DP dt-bindings into one file cdns,mhdp8501.yaml
- Fix HDMI scrambling is not enable issue when driver working in 4Kp60
  mode.
- Add HDMI/DP PHY API mailbox protect.

HDMI/DP PHY driver:
- Rename DP and HDMI PHY files and move to folder phy/freescale/
- Remove properties num_lanes and link_rate from DP PHY driver.
- Combine HDMI and DP dt-bindings into one file fsl,imx8mq-dp-hdmi-phy.yaml
- Update compatible string to "fsl,imx8mq-dp-phy".
- Update compatible string to "fsl,imx8mq-hdmi-phy".

v4->v5:
- Drop "clk" suffix in clock name.
- Add output port property in the example of hdmi/dp.

v3->v4:
dt-bindings:
- Correct dt-bindings coding style and address review comments.
- Add apb_clk description.
- Add output port for HDMI/DP connector
PHY:
- Alphabetically sorted in Kconfig and Makefile for DP and HDMI PHY
- Remove unused registers define from HDMI and DP PHY drivers.
- More description in phy_hdmi.h.
- Add apb_clk to HDMI and DP phy driver.
HDMI/DP:
- Use get_unaligned_le32() to replace hardcode type conversion
  in HDMI AVI infoframe data fill function.
- Add mailbox mutex lock in HDMI/DP driver for phy functions
  to reslove race conditions between HDMI/DP and PHY drivers.
- Add apb_clk to both HDMI and DP driver.
- Rename some function names and add prefix with "cdns_hdmi/cdns_dp".
- Remove bpc 12 and 16 optional that not supported.

v2->v3:
Address comments for dt-bindings files.
- Correct dts-bindings file names 
  Rename phy-cadence-hdptx-dp.yaml to cdns,mhdp-imx8mq-dp.yaml
  Rename phy-cadence-hdptx-hdmi.yaml to cdns,mhdp-imx8mq-hdmi.yaml
- Drop redundant words and descriptions.
- Correct hdmi/dp node name.

v2 is a completely different version compared to v1.
Previous v1 can be available here [1].

v1->v2:
- Reuse Cadence mailbox access functions from mhdp8546 instead of
  rockchip DP.
- Mailbox access functions be convert to marco functions
  that will be referenced by HDP-TX PHY(HDMI/DP) driver too.
- Plain bridge instead of component driver.
- Standalone Cadence HDP-TX PHY(HDMI/DP) driver.
- Audio driver are removed from the patch set, it will be add in another
  patch set later.

[1] https://patchwork.kernel.org/project/linux-rockchip/cover/cover.1590982881.git.Sandor.yu@nxp.com/

Alexander Stein (2):
  arm64: dts: imx8mq: Add DCSS + HDMI/DP display pipeline
  arm64: dts: imx8mq: tqma8mq-mba8mx: Enable HDMI support

Sandor Yu (7):
  soc: cadence: Create helper functions for Cadence MHDP
  drm: bridge: cadence: Update mhdp8546 mailbox access functions
  phy: Add HDMI configuration options
  dt-bindings: display: bridge: Add Cadence MHDP8501
  drm: bridge: Cadence: Add MHDP8501 DP/HDMI driver
  dt-bindings: phy: Add Freescale iMX8MQ DP and HDMI PHY
  phy: freescale: Add DisplayPort/HDMI Combo-PHY driver for i.MX8MQ

 .../display/bridge/cdns,mhdp8501.yaml         |  121 ++
 .../bindings/phy/fsl,imx8mq-dp-hdmi-phy.yaml  |   51 +
 .../dts/freescale/imx8mq-tqma8mq-mba8mx.dts   |   26 +
 arch/arm64/boot/dts/freescale/imx8mq.dtsi     |   68 +
 arch/arm64/boot/dts/freescale/mba8mx.dtsi     |   11 +
 drivers/gpu/drm/bridge/cadence/Kconfig        |   17 +
 drivers/gpu/drm/bridge/cadence/Makefile       |    2 +
 .../drm/bridge/cadence/cdns-mhdp8501-core.c   |  379 +++++
 .../drm/bridge/cadence/cdns-mhdp8501-core.h   |  380 +++++
 .../gpu/drm/bridge/cadence/cdns-mhdp8501-dp.c |  694 ++++++++++
 .../drm/bridge/cadence/cdns-mhdp8501-hdmi.c   |  745 ++++++++++
 .../drm/bridge/cadence/cdns-mhdp8546-core.c   |  487 ++-----
 .../drm/bridge/cadence/cdns-mhdp8546-core.h   |   47 +-
 .../drm/bridge/cadence/cdns-mhdp8546-hdcp.c   |  212 +--
 .../drm/bridge/cadence/cdns-mhdp8546-hdcp.h   |   18 +-
 drivers/phy/freescale/Kconfig                 |   10 +
 drivers/phy/freescale/Makefile                |    1 +
 drivers/phy/freescale/phy-fsl-imx8mq-hdptx.c  | 1231 +++++++++++++++++
 drivers/soc/Kconfig                           |    1 +
 drivers/soc/Makefile                          |    1 +
 drivers/soc/cadence/Kconfig                   |    9 +
 drivers/soc/cadence/Makefile                  |    3 +
 drivers/soc/cadence/cdns-mhdp-helper.c        |  565 ++++++++
 include/linux/phy/phy-hdmi.h                  |   19 +
 include/linux/phy/phy.h                       |    7 +-
 include/soc/cadence/cdns-mhdp-helper.h        |  129 ++
 26 files changed, 4572 insertions(+), 662 deletions(-)
 create mode 100644 Documentation/devicetree/bindings/display/bridge/cdns,mhdp8501.yaml
 create mode 100644 Documentation/devicetree/bindings/phy/fsl,imx8mq-dp-hdmi-phy.yaml
 create mode 100644 drivers/gpu/drm/bridge/cadence/cdns-mhdp8501-core.c
 create mode 100644 drivers/gpu/drm/bridge/cadence/cdns-mhdp8501-core.h
 create mode 100644 drivers/gpu/drm/bridge/cadence/cdns-mhdp8501-dp.c
 create mode 100644 drivers/gpu/drm/bridge/cadence/cdns-mhdp8501-hdmi.c
 create mode 100644 drivers/phy/freescale/phy-fsl-imx8mq-hdptx.c
 create mode 100644 drivers/soc/cadence/Kconfig
 create mode 100644 drivers/soc/cadence/Makefile
 create mode 100644 drivers/soc/cadence/cdns-mhdp-helper.c
 create mode 100644 include/linux/phy/phy-hdmi.h
 create mode 100644 include/soc/cadence/cdns-mhdp-helper.h

-- 
2.34.1



From patchwork Tue Dec 17 06:51:43 2024
Content-Type: text/plain; charset="utf-8"
MIME-Version: 1.0
Content-Transfer-Encoding: 7bit
Subject: [v20,1/9] soc: cadence: Create helper functions for Cadence MHDP
From: Sandor Yu <Sandor.yu@nxp.com>
X-Patchwork-Id: 629288
Message-Id: 
 <7fd5d54e2594aadd66598888ddf512f3d6d30e5d.1734340233.git.Sandor.yu@nxp.com>
To: dmitry.baryshkov@linaro.org, andrzej.hajda@intel.com,
 neil.armstrong@linaro.org, Laurent.pinchart@ideasonboard.com,
 jonas@kwiboo.se, jernej.skrabec@gmail.com, airlied@gmail.com,
 daniel@ffwll.ch, robh+dt@kernel.org, krzysztof.kozlowski+dt@linaro.org,
 shawnguo@kernel.org, s.hauer@pengutronix.de, festevam@gmail.com,
 vkoul@kernel.org, dri-devel@lists.freedesktop.org,
 devicetree@vger.kernel.org, linux-arm-kernel@lists.infradead.org,
 linux-kernel@vger.kernel.org, linux-phy@lists.infradead.org,
 mripard@kernel.org
Cc: kernel@pengutronix.de, linux-imx@nxp.com, Sandor.yu@nxp.com,
 oliver.brown@nxp.com, alexander.stein@ew.tq-group.com, sam@ravnborg.org
Date: Tue, 17 Dec 2024 14:51:43 +0800

Cadence MHDP IP includes a firmware. Driver and firmware communicate
through a mailbox. The basic mailbox access functions in this patch
are derived from the DRM bridge MHDP8546 driver.
New mailbox access functions have been created based on different mailbox
return values and security types, making them reusable across different
MHDP driver versions and SOCs.

These helper fucntions will be reused in both the DRM bridge driver MDHP8501
and the i.MX8MQ HDPTX PHY driver.

Six mailbox access helper functions are introduced.
Three for non-secure mailbox access:
 - cdns_mhdp_mailbox_send()
 - cdns_mhdp_mailbox_send_recv()
 - cdns_mhdp_mailbox_send_recv_multi()
The other three for secure mailbox access:
 - cdns_mhdp_secure_mailbox_send()
 - cdns_mhdp_secure_mailbox_send_recv()
 - cdns_mhdp_secure_mailbox_send_recv_multi()

All MHDP commands that need to be passed through the mailbox
should be rewritten using these new helper functions.

The register read/write and DP DPCD read/write command functions
are also included in this new helper driver.

Signed-off-by: Sandor Yu <Sandor.yu@nxp.com>
---
v19->v20:
- new patch in v20.
  The patch split from Patch #1 in v19 and move to a new folder drivers/soc/cadence

 drivers/soc/Kconfig                    |   1 +
 drivers/soc/Makefile                   |   1 +
 drivers/soc/cadence/Kconfig            |   9 +
 drivers/soc/cadence/Makefile           |   3 +
 drivers/soc/cadence/cdns-mhdp-helper.c | 565 +++++++++++++++++++++++++
 include/soc/cadence/cdns-mhdp-helper.h | 129 ++++++
 6 files changed, 708 insertions(+)
 create mode 100644 drivers/soc/cadence/Kconfig
 create mode 100644 drivers/soc/cadence/Makefile
 create mode 100644 drivers/soc/cadence/cdns-mhdp-helper.c
 create mode 100644 include/soc/cadence/cdns-mhdp-helper.h

diff --git a/drivers/soc/Kconfig b/drivers/soc/Kconfig
index 6a8daeb8c4b96..f6c18114b2d68 100644
--- a/drivers/soc/Kconfig
+++ b/drivers/soc/Kconfig
@@ -6,6 +6,7 @@ source "drivers/soc/apple/Kconfig"
 source "drivers/soc/aspeed/Kconfig"
 source "drivers/soc/atmel/Kconfig"
 source "drivers/soc/bcm/Kconfig"
+source "drivers/soc/cadence/Kconfig"
 source "drivers/soc/canaan/Kconfig"
 source "drivers/soc/cirrus/Kconfig"
 source "drivers/soc/fsl/Kconfig"
diff --git a/drivers/soc/Makefile b/drivers/soc/Makefile
index 2037a8695cb28..a5fa4f4d15321 100644
--- a/drivers/soc/Makefile
+++ b/drivers/soc/Makefile
@@ -7,6 +7,7 @@ obj-y				+= apple/
 obj-y				+= aspeed/
 obj-$(CONFIG_ARCH_AT91)		+= atmel/
 obj-y				+= bcm/
+obj-y				+= cadence/
 obj-$(CONFIG_ARCH_CANAAN)	+= canaan/
 obj-$(CONFIG_EP93XX_SOC)        += cirrus/
 obj-$(CONFIG_ARCH_DOVE)		+= dove/
diff --git a/drivers/soc/cadence/Kconfig b/drivers/soc/cadence/Kconfig
new file mode 100644
index 0000000000000..b668790660fa5
--- /dev/null
+++ b/drivers/soc/cadence/Kconfig
@@ -0,0 +1,9 @@
+# SPDX-License-Identifier: GPL-2.0
+
+config CDNS_MHDP_HELPER
+	tristate "Cadence MHDP Helper driver"
+	help
+	  Enable Cadence MHDP helpers for mailbox, HDMI and DP.
+	  This driver provides a foundational layer of mailbox communication for
+	  various Cadence MHDP IP implementations, such as HDMI and DisplayPort.
+
diff --git a/drivers/soc/cadence/Makefile b/drivers/soc/cadence/Makefile
new file mode 100644
index 0000000000000..a1f42e1936ca5
--- /dev/null
+++ b/drivers/soc/cadence/Makefile
@@ -0,0 +1,3 @@
+# SPDX-License-Identifier: GPL-2.0-only
+
+obj-$(CONFIG_CDNS_MHDP_HELPER) += cdns-mhdp-helper.o
diff --git a/drivers/soc/cadence/cdns-mhdp-helper.c b/drivers/soc/cadence/cdns-mhdp-helper.c
new file mode 100644
index 0000000000000..f74b4cae134a2
--- /dev/null
+++ b/drivers/soc/cadence/cdns-mhdp-helper.c
@@ -0,0 +1,565 @@
+// SPDX-License-Identifier: GPL-2.0-only
+/*
+ * Copyright (C) 2023, 2024 NXP Semiconductor, Inc.
+ *
+ */
+#include <linux/dev_printk.h>
+#include <linux/module.h>
+#include <soc/cadence/cdns-mhdp-helper.h>
+
+/* Protects mailbox communications with the firmware */
+static DEFINE_MUTEX(mhdp_mailbox_mutex);
+
+/* Mailbox helper functions */
+static int mhdp_mailbox_read(void __iomem *regs)
+{
+	int ret, empty;
+
+	WARN_ON(!mutex_is_locked(&mhdp_mailbox_mutex));
+
+	ret = readx_poll_timeout(readl, regs + CDNS_MAILBOX_EMPTY,
+				 empty, !empty, MAILBOX_RETRY_US,
+				 MAILBOX_TIMEOUT_US);
+	if (ret < 0)
+		return ret;
+
+	return readl(regs + CDNS_MAILBOX_RX_DATA) & 0xff;
+}
+
+static int mhdp_mailbox_write(void __iomem *regs, u8 val)
+{
+	int ret, full;
+
+	WARN_ON(!mutex_is_locked(&mhdp_mailbox_mutex));
+
+	ret = readx_poll_timeout(readl, regs + CDNS_MAILBOX_FULL,
+				 full, !full, MAILBOX_RETRY_US,
+				 MAILBOX_TIMEOUT_US);
+	if (ret < 0)
+		return ret;
+
+	writel(val, regs + CDNS_MAILBOX_TX_DATA);
+
+	return 0;
+}
+
+static int mhdp_mailbox_recv_header(void __iomem *regs,
+				    u8 module_id, u8 opcode,
+				    u16 req_size)
+{
+	u32 mbox_size, i;
+	u8 header[4];
+	int ret;
+
+	/* read the header of the message */
+	for (i = 0; i < sizeof(header); i++) {
+		ret = mhdp_mailbox_read(regs);
+		if (ret < 0)
+			return ret;
+
+		header[i] = ret;
+	}
+
+	mbox_size = get_unaligned_be16(header + 2);
+
+	/*
+	 * If the message in mailbox is not what we want, we need to
+	 * clear the mailbox by reading its contents.
+	 * Response data length for HDCP TX HDCP_TRAN_IS_REC_ID_VALID depend on case.
+	 */
+	if (opcode != header[0] ||
+	    module_id != header[1] ||
+	   (opcode != HDCP_TRAN_IS_REC_ID_VALID && req_size != mbox_size)) {
+		for (i = 0; i < mbox_size; i++)
+			if (mhdp_mailbox_read(regs) < 0)
+				break;
+
+		return -EINVAL;
+	}
+
+	return 0;
+}
+
+static int mhdp_mailbox_recv_data(void __iomem *regs,
+				  u8 *buff, u16 buff_size)
+{
+	u32 i;
+	int ret;
+
+	for (i = 0; i < buff_size; i++) {
+		ret = mhdp_mailbox_read(regs);
+		if (ret < 0)
+			return ret;
+
+		buff[i] = ret;
+	}
+
+	return 0;
+}
+
+static int mhdp_mailbox_send(void __iomem *regs, u8 module_id,
+			     u8 opcode, u16 size, u8 *message)
+{
+	u8 header[4];
+	int ret, i;
+
+	header[0] = opcode;
+	header[1] = module_id;
+	put_unaligned_be16(size, header + 2);
+
+	for (i = 0; i < sizeof(header); i++) {
+		ret = mhdp_mailbox_write(regs, header[i]);
+		if (ret)
+			return ret;
+	}
+
+	for (i = 0; i < size; i++) {
+		ret = mhdp_mailbox_write(regs, message[i]);
+		if (ret)
+			return ret;
+	}
+
+	return 0;
+}
+
+/**
+ * cdns_mhdp_mailbox_send - Sends a message via the MHDP mailbox.
+ *
+ * This function sends a message via the MHDP mailbox.
+ *
+ * @base: Pointer to the CDNS MHDP base structure.
+ * @module_id: ID of the module to send the message to.
+ * @opcode: Operation code of the message.
+ * @size: Size of the message data.
+ * @message: Pointer to the message data.
+ *
+ * Returns: 0 on success, negative error code on failure.
+ */
+int cdns_mhdp_mailbox_send(struct cdns_mhdp_base *base, u8 module_id,
+			   u8 opcode, u16 size, u8 *message)
+{
+	guard(mutex)(&mhdp_mailbox_mutex);
+
+	return mhdp_mailbox_send(base->regs, module_id, opcode, size, message);
+}
+EXPORT_SYMBOL_GPL(cdns_mhdp_mailbox_send);
+
+/**
+ * cdns_mhdp_mailbox_send_recv - Sends a message and receives a response.
+ *
+ * This function sends a message via the mailbox and then receives a response.
+ *
+ * @base: Pointer to the CDNS MHDP base structure.
+ * @module_id: ID of the module to send the message to.
+ * @opcode: Operation code of the message.
+ * @msg_size: Size of the message data.
+ * @msg: Pointer to the message data.
+ * @resp_size: Size of the response buffer.
+ * @resp: Pointer to the response buffer.
+ *
+ * Returns: 0 on success, negative error code on failure.
+ */
+int cdns_mhdp_mailbox_send_recv(struct cdns_mhdp_base *base,
+				u8 module_id, u8 opcode,
+				u16 msg_size, u8 *msg,
+				u16 resp_size, u8 *resp)
+{
+	int ret;
+
+	guard(mutex)(&mhdp_mailbox_mutex);
+
+	ret = mhdp_mailbox_send(base->regs, module_id,
+				opcode, msg_size, msg);
+	if (ret) {
+		dev_err(base->dev, "ModuleID=%d, CMD=%d send failed: %d\n",
+			module_id, opcode, ret);
+		return ret;
+	}
+
+	ret = mhdp_mailbox_recv_header(base->regs, module_id,
+				       opcode, resp_size);
+	if (ret) {
+		dev_err(base->dev, "ModuleID=%d, CMD=%d recv header failed: %d\n",
+			module_id, opcode, ret);
+		return ret;
+	}
+
+	ret = mhdp_mailbox_recv_data(base->regs, resp, resp_size);
+	if (ret)
+		dev_err(base->dev, "ModuleID=%d, CMD=%d recv data failed: %d\n",
+			module_id, opcode, ret);
+	return ret;
+}
+EXPORT_SYMBOL_GPL(cdns_mhdp_mailbox_send_recv);
+
+/**
+ * cdns_mhdp_mailbox_send_recv_multi - Sends a message and receives multiple responses.
+ *
+ * This function sends a message to a specified module via the MHDP mailbox and
+ * then receives multiple responses from the module.
+ *
+ * @param base: Pointer to the CDNS MHDP base structure.
+ * @param module_id: ID of the module to send the message to.
+ * @param opcode: Operation code of the message.
+ * @param msg_size: Size of the message data.
+ * @param msg: Pointer to the message data.
+ * @param opcode_resp: Operation code of the response.
+ * @param resp1_size: Size of the first response buffer.
+ * @param resp1: Pointer to the first response buffer.
+ * @param resp2_size: Size of the second response buffer.
+ * @param resp2: Pointer to the second response buffer.
+ *
+ * Returns: 0 on success, negative error code on failure.
+ */
+int cdns_mhdp_mailbox_send_recv_multi(struct cdns_mhdp_base *base,
+				      u8 module_id, u8 opcode,
+				      u16 msg_size, u8 *msg,
+				      u8 opcode_resp,
+				      u16 resp1_size, u8 *resp1,
+				      u16 resp2_size, u8 *resp2)
+{
+	int ret;
+
+	guard(mutex)(&mhdp_mailbox_mutex);
+
+	ret = mhdp_mailbox_send(base->regs, module_id,
+				opcode, msg_size, msg);
+	if (ret) {
+		dev_err(base->dev, "ModuleID=%d, CMD=%d send failed: %d\n",
+			module_id, opcode, ret);
+		return ret;
+	}
+
+	ret = mhdp_mailbox_recv_header(base->regs, module_id, opcode_resp,
+				       resp1_size + resp2_size);
+	if (ret) {
+		dev_err(base->dev, "ModuleID=%d, Resp_CMD=%d recv header failed: %d\n",
+			module_id, opcode_resp, ret);
+		return ret;
+	}
+
+	ret = mhdp_mailbox_recv_data(base->regs, resp1, resp1_size);
+	if (ret) {
+		dev_err(base->dev, "ModuleID=%d, Resp_CMD=%d recv data1 failed: %d\n",
+			module_id, opcode_resp, ret);
+		return ret;
+	}
+
+	ret = mhdp_mailbox_recv_data(base->regs, resp2, resp2_size);
+	if (ret)
+		dev_err(base->dev, "ModuleID=%d, Resp_CMD=%d recv data1 failed: %d\n",
+			module_id, opcode_resp, ret);
+	return ret;
+}
+EXPORT_SYMBOL_GPL(cdns_mhdp_mailbox_send_recv_multi);
+
+/**
+ * cdns_mhdp_secure_mailbox_send - Sends a secure message via the mailbox.
+ *
+ * This function sends a secure message to a specified module via the MHDP mailbox.
+ *
+ * @param base: Pointer to the CDNS MHDP base structure.
+ * @param module_id: ID of the module to send the message to.
+ * @param opcode: Operation code of the message.
+ * @param size: Size of the message data.
+ * @param message: Pointer to the message data.
+ *
+ * Returns: 0 on success, negative error code on failure.
+ */
+int cdns_mhdp_secure_mailbox_send(struct cdns_mhdp_base *base, u8 module_id,
+				  u8 opcode, u16 size, u8 *message)
+{
+	guard(mutex)(&mhdp_mailbox_mutex);
+
+	return mhdp_mailbox_send(base->sapb_regs, module_id, opcode, size, message);
+}
+EXPORT_SYMBOL_GPL(cdns_mhdp_secure_mailbox_send);
+
+/**
+ * cdns_mhdp_secure_mailbox_send_recv - Sends a secure message and receives a response.
+ *
+ * This function sends a secure message to a specified module via the mailbox and
+ * then receives a response from the module.
+ *
+ * @param base: Pointer to the CDNS MHDP base structure.
+ * @param module_id: ID of the module to send the message to.
+ * @param opcode: Operation code of the message.
+ * @param msg_size: Size of the message data.
+ * @param msg: Pointer to the message data.
+ * @param resp_size: Size of the response buffer.
+ * @param resp: Pointer to the response buffer.
+ *
+ * Returns: 0 on success, negative error code on failure.
+ */
+int cdns_mhdp_secure_mailbox_send_recv(struct cdns_mhdp_base *base,
+				       u8 module_id, u8 opcode,
+				       u16 msg_size, u8 *msg,
+				       u16 resp_size, u8 *resp)
+{
+	int ret;
+
+	guard(mutex)(&mhdp_mailbox_mutex);
+
+	ret = mhdp_mailbox_send(base->sapb_regs, module_id,
+				opcode, msg_size, msg);
+	if (ret) {
+		dev_err(base->dev, "ModuleID=%d, CMD=%d send failed: %d\n",
+			module_id, opcode, ret);
+		return ret;
+	}
+
+	ret = mhdp_mailbox_recv_header(base->sapb_regs, module_id,
+				       opcode, resp_size);
+	if (ret) {
+		dev_err(base->dev, "ModuleID=%d, CMD=%d recv header failed: %d\n",
+			module_id, opcode, ret);
+		return ret;
+	}
+
+	ret = mhdp_mailbox_recv_data(base->sapb_regs, resp, resp_size);
+	if (ret)
+		dev_err(base->dev, "ModuleID=%d, CMD=%d recv data failed: %d\n",
+			module_id, opcode, ret);
+	return ret;
+}
+EXPORT_SYMBOL_GPL(cdns_mhdp_secure_mailbox_send_recv);
+
+/**
+ * cdns_mhdp_secure_mailbox_send_recv_multi - Sends a secure message and receives multiple responses.
+ *
+ * This function sends a secure message to a specified module and receives multiple responses.
+ *
+ * @param base: Pointer to the CDNS MHDP base structure.
+ * @param module_id: ID of the module to send the message to.
+ * @param opcode: Operation code of the message.
+ * @param msg_size: Size of the message data.
+ * @param msg: Pointer to the message data.
+ * @param opcode_resp: Operation code of the response.
+ * @param resp1_size: Size of the first response buffer.
+ * @param resp1: Pointer to the first response buffer.
+ * @param resp2_size: Size of the second response buffer.
+ * @param resp2: Pointer to the second response buffer.
+ *
+ * Returns: 0 on success, negative error code on failure.
+ */
+int cdns_mhdp_secure_mailbox_send_recv_multi(struct cdns_mhdp_base *base,
+					     u8 module_id, u8 opcode,
+					     u16 msg_size, u8 *msg,
+					     u8 opcode_resp,
+					     u16 resp1_size, u8 *resp1,
+					     u16 resp2_size, u8 *resp2)
+{
+	int ret;
+
+	guard(mutex)(&mhdp_mailbox_mutex);
+
+	ret = mhdp_mailbox_send(base->sapb_regs, module_id,
+				opcode, msg_size, msg);
+	if (ret) {
+		dev_err(base->dev, "ModuleID=%d, CMD=%d send failed: %d\n",
+			module_id, opcode, ret);
+		return ret;
+	}
+
+	ret = mhdp_mailbox_recv_header(base->sapb_regs, module_id,
+				       opcode_resp,
+				       resp1_size + resp2_size);
+	if (ret) {
+		dev_err(base->dev, "ModuleID=%d, Resp_CMD=%d recv header failed: %d\n",
+			module_id, opcode_resp, ret);
+		return ret;
+	}
+
+	ret = mhdp_mailbox_recv_data(base->sapb_regs, resp1, resp1_size);
+	if (ret) {
+		dev_err(base->dev, "ModuleID=%d, Resp_CMD=%d recv data1 failed: %d\n",
+			module_id, opcode_resp, ret);
+		return ret;
+	}
+
+	/*
+	 * Response data length for HDCP TX HDCP_TRAN_IS_REC_ID_VALID depend on
+	 * the number of HDCP receivers in resp1[0].
+	 * 1 for regular case, more can be in repeater.
+	 */
+	if (module_id == MB_MODULE_ID_HDCP_TX &&
+	    opcode == HDCP_TRAN_IS_REC_ID_VALID)
+		ret = mhdp_mailbox_recv_data(base->sapb_regs, resp2, 5 * resp1[0]);
+	else
+		ret = mhdp_mailbox_recv_data(base->sapb_regs, resp2, resp2_size);
+	if (ret)
+		dev_err(base->dev, "ModuleID=%d, Resp_CMD=%d recv data2 failed: %d\n",
+			module_id, opcode_resp, ret);
+	return ret;
+}
+EXPORT_SYMBOL_GPL(cdns_mhdp_secure_mailbox_send_recv_multi);
+
+/**
+ * cdns_mhdp_reg_read - Reads a general register value.
+ *
+ * This function reads the value from a general register
+ * using the mailbox.
+ *
+ * @param base: Pointer to the CDNS MHDP base structure.
+ * @param addr: Address of the register to read.
+ * @param value: Pointer to store the read value.
+ *
+ * Returns: 0 on success, negative error code on failure.
+ */
+int cdns_mhdp_reg_read(struct cdns_mhdp_base *base, u32 addr, u32 *value)
+{
+	u8 msg[4], resp[8];
+	int ret;
+
+	put_unaligned_be32(addr, msg);
+
+	ret = cdns_mhdp_mailbox_send_recv(base, MB_MODULE_ID_GENERAL,
+					  GENERAL_REGISTER_READ,
+					  sizeof(msg), msg, sizeof(resp), resp);
+	if (ret)
+		goto out;
+
+	/* Returned address value should be the same as requested */
+	if (memcmp(msg, resp, sizeof(msg))) {
+		ret = -EINVAL;
+		goto out;
+	}
+
+	*value = get_unaligned_be32(resp + 4);
+out:
+	if (ret) {
+		dev_err(base->dev, "Failed to read register\n");
+		*value = 0;
+	}
+
+	return ret;
+}
+EXPORT_SYMBOL_GPL(cdns_mhdp_reg_read);
+
+/**
+ * cdns_mhdp_reg_write - Writes a value to a general register.
+ *
+ * This function writes a value to a general register using the mailbox.
+ *
+ * @param base: Pointer to the CDNS MHDP base structure.
+ * @param addr: Address of the register to write to.
+ * @param val: Value to write to the register.
+ *
+ * Returns: 0 on success, negative error code on failure.
+ */
+int cdns_mhdp_reg_write(struct cdns_mhdp_base *base, u32 addr, u32 val)
+{
+	u8 msg[8];
+
+	put_unaligned_be32(addr, msg);
+	put_unaligned_be32(val, msg + 4);
+
+	return cdns_mhdp_mailbox_send(base, MB_MODULE_ID_GENERAL,
+				     GENERAL_REGISTER_WRITE,
+				     sizeof(msg), msg);
+}
+EXPORT_SYMBOL_GPL(cdns_mhdp_reg_write);
+
+/* DPTX helper functions */
+/**
+ * cdns_mhdp_dp_reg_write_bit - Writes a bit field to a DP register.
+ *
+ * This function writes a specific bit field within a DP register
+ * using the MHDP mailbox.
+ *
+ * @param base: Pointer to the CDNS MHDP base structure.
+ * @param addr: Address of the DP register.
+ * @param start_bit: Starting bit position within the register.
+ * @param bits_no: Number of bits to write.
+ * @param val: Value to write to the bit field.
+ *
+ * Returns: 0 on success, negative error code on failure.
+ */
+int cdns_mhdp_dp_reg_write_bit(struct cdns_mhdp_base *base, u16 addr,
+			       u8 start_bit, u8 bits_no, u32 val)
+{
+	u8 field[8];
+
+	put_unaligned_be16(addr, field);
+	field[2] = start_bit;
+	field[3] = bits_no;
+	put_unaligned_be32(val, field + 4);
+
+	return cdns_mhdp_mailbox_send(base, MB_MODULE_ID_DP_TX,
+				      DPTX_WRITE_FIELD, sizeof(field), field);
+}
+EXPORT_SYMBOL_GPL(cdns_mhdp_dp_reg_write_bit);
+
+/**
+ * cdns_mhdp_dpcd_read - Reads data from a DPCD register.
+ *
+ * This function reads data from a specified DPCD register
+ * using the MHDP mailbox.
+ *
+ * @param base: Pointer to the CDNS MHDP base structure.
+ * @param addr: Address of the DPCD register to read.
+ * @param data: Buffer to store the read data.
+ * @param len: Length of the data to read.
+ *
+ * Returns: 0 on success, negative error code on failure.
+ */
+int cdns_mhdp_dpcd_read(struct cdns_mhdp_base *base,
+			u32 addr, u8 *data, u16 len)
+{
+	u8 msg[5], reg[5];
+
+	put_unaligned_be16(len, msg);
+	put_unaligned_be24(addr, msg + 2);
+
+	return cdns_mhdp_mailbox_send_recv_multi(base,
+						 MB_MODULE_ID_DP_TX,
+						 DPTX_READ_DPCD,
+						 sizeof(msg), msg,
+						 DPTX_READ_DPCD,
+						 sizeof(reg), reg,
+						 len, data);
+}
+EXPORT_SYMBOL_GPL(cdns_mhdp_dpcd_read);
+
+/**
+ * cdns_mhdp_dpcd_write - Writes data to a DPCD register.
+ *
+ * This function writes data to a specified DPCD register
+ * using the MHDP mailbox.
+ *
+ * @param base: Pointer to the CDNS MHDP base structure.
+ * @param addr: Address of the DPCD register to write to.
+ * @param value: Value to write to the register.
+ *
+ * Returns: 0 on success, negative error code on failure.
+ */
+int cdns_mhdp_dpcd_write(struct cdns_mhdp_base *base, u32 addr, u8 value)
+{
+	u8 msg[6], reg[5];
+	int ret;
+
+	put_unaligned_be16(1, msg);
+	put_unaligned_be24(addr, msg + 2);
+	msg[5] = value;
+
+	ret = cdns_mhdp_mailbox_send_recv(base, MB_MODULE_ID_DP_TX,
+					  DPTX_WRITE_DPCD,
+					  sizeof(msg), msg, sizeof(reg), reg);
+	if (ret) {
+		dev_err(base->dev, "dpcd write failed: %d\n", ret);
+		return ret;
+	}
+
+	if (addr != get_unaligned_be24(reg + 2)) {
+		dev_err(base->dev, "Invalid response: expected address 0x%06x, got 0x%06x\n",
+			addr, get_unaligned_be24(reg + 2));
+		return -EINVAL;
+	}
+
+	return 0;
+}
+EXPORT_SYMBOL_GPL(cdns_mhdp_dpcd_write);
+
+MODULE_DESCRIPTION("Cadence MHDP Helper driver");
+MODULE_AUTHOR("Sandor Yu <Sandor.yu@nxp.com>");
+MODULE_LICENSE("GPL");
diff --git a/include/soc/cadence/cdns-mhdp-helper.h b/include/soc/cadence/cdns-mhdp-helper.h
new file mode 100644
index 0000000000000..25b9737de615f
--- /dev/null
+++ b/include/soc/cadence/cdns-mhdp-helper.h
@@ -0,0 +1,129 @@
+/* SPDX-License-Identifier: GPL-2.0-only */
+/*
+ * Copyright (C) 2023-2024 NXP Semiconductor, Inc.
+ */
+#ifndef __CDNS_MHDP_HELPER_H__
+#define __CDNS_MHDP_HELPER_H__
+
+#include <linux/iopoll.h>
+#include <linux/unaligned.h>
+
+/* mailbox regs offset */
+#define CDNS_MAILBOX_FULL			0x00008
+#define CDNS_MAILBOX_EMPTY			0x0000c
+#define CDNS_MAILBOX_TX_DATA			0x00010
+#define CDNS_MAILBOX_RX_DATA			0x00014
+
+#define MAILBOX_RETRY_US			1000
+#define MAILBOX_TIMEOUT_US			2000000
+
+/* Module ID Code */
+#define MB_MODULE_ID_DP_TX			0x01
+#define MB_MODULE_ID_HDMI_TX			0x03
+#define MB_MODULE_ID_HDCP_TX			0x07
+#define MB_MODULE_ID_HDCP_RX			0x08
+#define MB_MODULE_ID_HDCP_GENERAL		0x09
+#define MB_MODULE_ID_GENERAL			0x0A
+
+/* General Commands */
+#define GENERAL_MAIN_CONTROL			0x01
+#define GENERAL_TEST_ECHO			0x02
+#define GENERAL_BUS_SETTINGS			0x03
+#define GENERAL_TEST_ACCESS			0x04
+#define GENERAL_REGISTER_WRITE			0x05
+#define GENERAL_WRITE_FIELD			0x06
+#define GENERAL_REGISTER_READ			0x07
+#define GENERAL_GET_HPD_STATE			0x11
+
+/* DPTX Commands */
+#define DPTX_SET_POWER_MNG			0x00
+#define DPTX_SET_HOST_CAPABILITIES		0x01
+#define DPTX_GET_EDID				0x02
+#define DPTX_READ_DPCD				0x03
+#define DPTX_WRITE_DPCD				0x04
+#define DPTX_ENABLE_EVENT			0x05
+#define DPTX_WRITE_REGISTER			0x06
+#define DPTX_READ_REGISTER			0x07
+#define DPTX_WRITE_FIELD			0x08
+#define DPTX_TRAINING_CONTROL			0x09
+#define DPTX_READ_EVENT				0x0a
+#define DPTX_READ_LINK_STAT			0x0b
+#define DPTX_SET_VIDEO				0x0c
+#define DPTX_SET_AUDIO				0x0d
+#define DPTX_GET_LAST_AUX_STAUS			0x0e
+#define DPTX_SET_LINK_BREAK_POINT		0x0f
+#define DPTX_FORCE_LANES			0x10
+#define DPTX_HPD_STATE				0x11
+#define DPTX_ADJUST_LT				0x12
+
+/* HDMI TX Commands */
+#define HDMI_TX_READ				0x00
+#define HDMI_TX_WRITE				0x01
+#define HDMI_TX_UPDATE_READ			0x02
+#define HDMI_TX_EDID				0x03
+#define HDMI_TX_EVENTS				0x04
+#define HDMI_TX_HPD_STATUS			0x05
+
+/* HDCP TX Commands */
+#define HDCP_TRAN_CONFIGURATION			0x00
+#define HDCP2X_TX_SET_PUBLIC_KEY_PARAMS		0x01
+#define HDCP2X_TX_SET_DEBUG_RANDOM_NUMBERS	0x02
+#define HDCP2X_TX_RESPOND_KM			0x03
+#define HDCP1_TX_SEND_KEYS			0x04
+#define HDCP1_TX_SEND_RANDOM_AN			0x05
+#define HDCP_TRAN_STATUS_CHANGE			0x06
+#define HDCP2X_TX_IS_KM_STORED			0x07
+#define HDCP2X_TX_STORE_KM			0x08
+#define HDCP_TRAN_IS_REC_ID_VALID		0x09
+#define HDCP_TRAN_RESPOND_RECEIVER_ID_VALID	0x09
+#define HDCP_TRAN_TEST_KEYS			0x0a
+#define HDCP2X_TX_SET_KM_KEY_PARAMS		0x0b
+#define HDCP_NUM_OF_SUPPORTED_MESSAGES		0x0c
+
+struct cdns_mhdp_base {
+	struct device *dev;
+	void __iomem *regs;
+	void __iomem *sapb_regs;
+};
+
+/* Mailbox helper functions */
+int cdns_mhdp_mailbox_send(struct cdns_mhdp_base *base,
+			   u8 module_id, u8 opcode,
+			   u16 size, u8 *message);
+int cdns_mhdp_mailbox_send_recv(struct cdns_mhdp_base *base,
+				u8 module_id, u8 opcode,
+				u16 msg_size, u8 *msg,
+				u16 resp_size, u8 *resp);
+int cdns_mhdp_mailbox_send_recv_multi(struct cdns_mhdp_base *base,
+				      u8 module_id, u8 opcode,
+				      u16 msg_size, u8 *msg,
+				      u8 opcode_resp,
+				      u16 resp1_size, u8 *resp1,
+				      u16 resp2_size, u8 *resp2);
+
+/* Secure mailbox helper functions */
+int cdns_mhdp_secure_mailbox_send(struct cdns_mhdp_base *base,
+				  u8 module_id, u8 opcode,
+				  u16 size, u8 *message);
+int cdns_mhdp_secure_mailbox_send_recv(struct cdns_mhdp_base *base,
+				       u8 module_id, u8 opcode,
+				       u16 msg_size, u8 *msg,
+				       u16 resp_size, u8 *resp);
+int cdns_mhdp_secure_mailbox_send_recv_multi(struct cdns_mhdp_base *base,
+					     u8 module_id, u8 opcode,
+					     u16 msg_size, u8 *msg,
+					     u8 opcode_resp,
+					     u16 resp1_size, u8 *resp1,
+					     u16 resp2_size, u8 *resp2);
+
+/* General commands helper functions */
+int cdns_mhdp_reg_read(struct cdns_mhdp_base *base, u32 addr, u32 *value);
+int cdns_mhdp_reg_write(struct cdns_mhdp_base *base, u32 addr, u32 val);
+
+/* DPTX commands helper functions */
+int cdns_mhdp_dp_reg_write_bit(struct cdns_mhdp_base *base, u16 addr,
+			       u8 start_bit, u8 bits_no, u32 val);
+int cdns_mhdp_dpcd_read(struct cdns_mhdp_base *base,
+			u32 addr, u8 *data, u16 len);
+int cdns_mhdp_dpcd_write(struct cdns_mhdp_base *base, u32 addr, u8 value);
+#endif /* __CDNS_MHDP_HELPER_H__ */

From patchwork Tue Dec 17 06:51:44 2024
Content-Type: text/plain; charset="utf-8"
MIME-Version: 1.0
Content-Transfer-Encoding: 7bit
Subject: [v20,2/9] drm: bridge: cadence: Update mhdp8546 mailbox access
 functions
From: Sandor Yu <Sandor.yu@nxp.com>
X-Patchwork-Id: 629289
Message-Id: 
 <74bc3f2ff56348afd9d773589236ddf06dc3d45c.1734340233.git.Sandor.yu@nxp.com>
To: dmitry.baryshkov@linaro.org, andrzej.hajda@intel.com,
 neil.armstrong@linaro.org, Laurent.pinchart@ideasonboard.com,
 jonas@kwiboo.se, jernej.skrabec@gmail.com, airlied@gmail.com,
 daniel@ffwll.ch, robh+dt@kernel.org, krzysztof.kozlowski+dt@linaro.org,
 shawnguo@kernel.org, s.hauer@pengutronix.de, festevam@gmail.com,
 vkoul@kernel.org, dri-devel@lists.freedesktop.org,
 devicetree@vger.kernel.org, linux-arm-kernel@lists.infradead.org,
 linux-kernel@vger.kernel.org, linux-phy@lists.infradead.org,
 mripard@kernel.org
Cc: kernel@pengutronix.de, linux-imx@nxp.com, Sandor.yu@nxp.com,
 oliver.brown@nxp.com, alexander.stein@ew.tq-group.com, sam@ravnborg.org
Date: Tue, 17 Dec 2024 14:51:44 +0800

Basic mailbox access functions are removed, they are replaced by
mailbox helper functions:
- cdns_mhdp_mailbox_send()
- cdns_mhdp_mailbox_send_recv()
- cdns_mhdp_mailbox_send_recv_multi()
- cdns_mhdp_secure_mailbox_send()
- cdns_mhdp_secure_mailbox_send_recv()
- cdns_mhdp_secure_mailbox_send_recv_multi()

All MHDP commands that need to be passed through the mailbox
have been rewritten using these new helper functions.

Signed-off-by: Sandor Yu <Sandor.yu@nxp.com>
Reviewed-by: Dmitry Baryshkov <dmitry.baryshkov@linaro.org>
---
v19->v20:
- remove mhdp helper functions from the patch.

v18->v19:
- Use guard(mutex)
- Add kerneldocs for all new APIs.
- Detail comments for mailbox access specific case.
- Remove cdns_mhdp_dp_reg_write() because it is not needed by driver now.

v17->v18:
- Create three ordinary mailbox access APIs
    cdns_mhdp_mailbox_send
    cdns_mhdp_mailbox_send_recv
    cdns_mhdp_mailbox_send_recv_multi
- Create three secure mailbox access APIs
    cdns_mhdp_secure_mailbox_send
    cdns_mhdp_secure_mailbox_send_recv
    cdns_mhdp_secure_mailbox_send_recv_multi
- MHDP8546 DP and HDCP commands that need access mailbox are rewrited
  with above 6 API functions.

v16->v17:
- Replaces the local mutex mbox_mutex with a global mutex mhdp_mailbox_mutex

v12->v16:
 *No change.

 drivers/gpu/drm/bridge/cadence/Kconfig        |   1 +
 .../drm/bridge/cadence/cdns-mhdp8546-core.c   | 487 +++---------------
 .../drm/bridge/cadence/cdns-mhdp8546-core.h   |  47 +-
 .../drm/bridge/cadence/cdns-mhdp8546-hdcp.c   | 212 +-------
 .../drm/bridge/cadence/cdns-mhdp8546-hdcp.h   |  18 +-
 5 files changed, 104 insertions(+), 661 deletions(-)

diff --git a/drivers/gpu/drm/bridge/cadence/Kconfig b/drivers/gpu/drm/bridge/cadence/Kconfig
index cced81633ddcd..dbb06533ccab2 100644
--- a/drivers/gpu/drm/bridge/cadence/Kconfig
+++ b/drivers/gpu/drm/bridge/cadence/Kconfig
@@ -28,6 +28,7 @@ config DRM_CDNS_MHDP8546
 	select DRM_DISPLAY_HELPER
 	select DRM_KMS_HELPER
 	select DRM_PANEL_BRIDGE
+	select CDNS_MHDP_HELPER
 	depends on OF
 	help
 	  Support Cadence DPI to DP bridge. This is an internal
diff --git a/drivers/gpu/drm/bridge/cadence/cdns-mhdp8546-core.c b/drivers/gpu/drm/bridge/cadence/cdns-mhdp8546-core.c
index d081850e3c03e..bd897c3ae7642 100644
--- a/drivers/gpu/drm/bridge/cadence/cdns-mhdp8546-core.c
+++ b/drivers/gpu/drm/bridge/cadence/cdns-mhdp8546-core.c
@@ -73,302 +73,18 @@ static void cdns_mhdp_bridge_hpd_disable(struct drm_bridge *bridge)
 	       mhdp->regs + CDNS_APB_INT_MASK);
 }
 
-static int cdns_mhdp_mailbox_read(struct cdns_mhdp_device *mhdp)
-{
-	int ret, empty;
-
-	WARN_ON(!mutex_is_locked(&mhdp->mbox_mutex));
-
-	ret = readx_poll_timeout(readl, mhdp->regs + CDNS_MAILBOX_EMPTY,
-				 empty, !empty, MAILBOX_RETRY_US,
-				 MAILBOX_TIMEOUT_US);
-	if (ret < 0)
-		return ret;
-
-	return readl(mhdp->regs + CDNS_MAILBOX_RX_DATA) & 0xff;
-}
-
-static int cdns_mhdp_mailbox_write(struct cdns_mhdp_device *mhdp, u8 val)
-{
-	int ret, full;
-
-	WARN_ON(!mutex_is_locked(&mhdp->mbox_mutex));
-
-	ret = readx_poll_timeout(readl, mhdp->regs + CDNS_MAILBOX_FULL,
-				 full, !full, MAILBOX_RETRY_US,
-				 MAILBOX_TIMEOUT_US);
-	if (ret < 0)
-		return ret;
-
-	writel(val, mhdp->regs + CDNS_MAILBOX_TX_DATA);
-
-	return 0;
-}
-
-static int cdns_mhdp_mailbox_recv_header(struct cdns_mhdp_device *mhdp,
-					 u8 module_id, u8 opcode,
-					 u16 req_size)
-{
-	u32 mbox_size, i;
-	u8 header[4];
-	int ret;
-
-	/* read the header of the message */
-	for (i = 0; i < sizeof(header); i++) {
-		ret = cdns_mhdp_mailbox_read(mhdp);
-		if (ret < 0)
-			return ret;
-
-		header[i] = ret;
-	}
-
-	mbox_size = get_unaligned_be16(header + 2);
-
-	if (opcode != header[0] || module_id != header[1] ||
-	    req_size != mbox_size) {
-		/*
-		 * If the message in mailbox is not what we want, we need to
-		 * clear the mailbox by reading its contents.
-		 */
-		for (i = 0; i < mbox_size; i++)
-			if (cdns_mhdp_mailbox_read(mhdp) < 0)
-				break;
-
-		return -EINVAL;
-	}
-
-	return 0;
-}
-
-static int cdns_mhdp_mailbox_recv_data(struct cdns_mhdp_device *mhdp,
-				       u8 *buff, u16 buff_size)
-{
-	u32 i;
-	int ret;
-
-	for (i = 0; i < buff_size; i++) {
-		ret = cdns_mhdp_mailbox_read(mhdp);
-		if (ret < 0)
-			return ret;
-
-		buff[i] = ret;
-	}
-
-	return 0;
-}
-
-static int cdns_mhdp_mailbox_send(struct cdns_mhdp_device *mhdp, u8 module_id,
-				  u8 opcode, u16 size, u8 *message)
-{
-	u8 header[4];
-	int ret, i;
-
-	header[0] = opcode;
-	header[1] = module_id;
-	put_unaligned_be16(size, header + 2);
-
-	for (i = 0; i < sizeof(header); i++) {
-		ret = cdns_mhdp_mailbox_write(mhdp, header[i]);
-		if (ret)
-			return ret;
-	}
-
-	for (i = 0; i < size; i++) {
-		ret = cdns_mhdp_mailbox_write(mhdp, message[i]);
-		if (ret)
-			return ret;
-	}
-
-	return 0;
-}
-
-static
-int cdns_mhdp_reg_read(struct cdns_mhdp_device *mhdp, u32 addr, u32 *value)
-{
-	u8 msg[4], resp[8];
-	int ret;
-
-	put_unaligned_be32(addr, msg);
-
-	mutex_lock(&mhdp->mbox_mutex);
-
-	ret = cdns_mhdp_mailbox_send(mhdp, MB_MODULE_ID_GENERAL,
-				     GENERAL_REGISTER_READ,
-				     sizeof(msg), msg);
-	if (ret)
-		goto out;
-
-	ret = cdns_mhdp_mailbox_recv_header(mhdp, MB_MODULE_ID_GENERAL,
-					    GENERAL_REGISTER_READ,
-					    sizeof(resp));
-	if (ret)
-		goto out;
-
-	ret = cdns_mhdp_mailbox_recv_data(mhdp, resp, sizeof(resp));
-	if (ret)
-		goto out;
-
-	/* Returned address value should be the same as requested */
-	if (memcmp(msg, resp, sizeof(msg))) {
-		ret = -EINVAL;
-		goto out;
-	}
-
-	*value = get_unaligned_be32(resp + 4);
-
-out:
-	mutex_unlock(&mhdp->mbox_mutex);
-	if (ret) {
-		dev_err(mhdp->dev, "Failed to read register\n");
-		*value = 0;
-	}
-
-	return ret;
-}
-
-static
-int cdns_mhdp_reg_write(struct cdns_mhdp_device *mhdp, u16 addr, u32 val)
-{
-	u8 msg[6];
-	int ret;
-
-	put_unaligned_be16(addr, msg);
-	put_unaligned_be32(val, msg + 2);
-
-	mutex_lock(&mhdp->mbox_mutex);
-
-	ret = cdns_mhdp_mailbox_send(mhdp, MB_MODULE_ID_DP_TX,
-				     DPTX_WRITE_REGISTER, sizeof(msg), msg);
-
-	mutex_unlock(&mhdp->mbox_mutex);
-
-	return ret;
-}
-
-static
-int cdns_mhdp_reg_write_bit(struct cdns_mhdp_device *mhdp, u16 addr,
-			    u8 start_bit, u8 bits_no, u32 val)
-{
-	u8 field[8];
-	int ret;
-
-	put_unaligned_be16(addr, field);
-	field[2] = start_bit;
-	field[3] = bits_no;
-	put_unaligned_be32(val, field + 4);
-
-	mutex_lock(&mhdp->mbox_mutex);
-
-	ret = cdns_mhdp_mailbox_send(mhdp, MB_MODULE_ID_DP_TX,
-				     DPTX_WRITE_FIELD, sizeof(field), field);
-
-	mutex_unlock(&mhdp->mbox_mutex);
-
-	return ret;
-}
-
-static
-int cdns_mhdp_dpcd_read(struct cdns_mhdp_device *mhdp,
-			u32 addr, u8 *data, u16 len)
-{
-	u8 msg[5], reg[5];
-	int ret;
-
-	put_unaligned_be16(len, msg);
-	put_unaligned_be24(addr, msg + 2);
-
-	mutex_lock(&mhdp->mbox_mutex);
-
-	ret = cdns_mhdp_mailbox_send(mhdp, MB_MODULE_ID_DP_TX,
-				     DPTX_READ_DPCD, sizeof(msg), msg);
-	if (ret)
-		goto out;
-
-	ret = cdns_mhdp_mailbox_recv_header(mhdp, MB_MODULE_ID_DP_TX,
-					    DPTX_READ_DPCD,
-					    sizeof(reg) + len);
-	if (ret)
-		goto out;
-
-	ret = cdns_mhdp_mailbox_recv_data(mhdp, reg, sizeof(reg));
-	if (ret)
-		goto out;
-
-	ret = cdns_mhdp_mailbox_recv_data(mhdp, data, len);
-
-out:
-	mutex_unlock(&mhdp->mbox_mutex);
-
-	return ret;
-}
-
-static
-int cdns_mhdp_dpcd_write(struct cdns_mhdp_device *mhdp, u32 addr, u8 value)
-{
-	u8 msg[6], reg[5];
-	int ret;
-
-	put_unaligned_be16(1, msg);
-	put_unaligned_be24(addr, msg + 2);
-	msg[5] = value;
-
-	mutex_lock(&mhdp->mbox_mutex);
-
-	ret = cdns_mhdp_mailbox_send(mhdp, MB_MODULE_ID_DP_TX,
-				     DPTX_WRITE_DPCD, sizeof(msg), msg);
-	if (ret)
-		goto out;
-
-	ret = cdns_mhdp_mailbox_recv_header(mhdp, MB_MODULE_ID_DP_TX,
-					    DPTX_WRITE_DPCD, sizeof(reg));
-	if (ret)
-		goto out;
-
-	ret = cdns_mhdp_mailbox_recv_data(mhdp, reg, sizeof(reg));
-	if (ret)
-		goto out;
-
-	if (addr != get_unaligned_be24(reg + 2))
-		ret = -EINVAL;
-
-out:
-	mutex_unlock(&mhdp->mbox_mutex);
-
-	if (ret)
-		dev_err(mhdp->dev, "dpcd write failed: %d\n", ret);
-	return ret;
-}
-
 static
 int cdns_mhdp_set_firmware_active(struct cdns_mhdp_device *mhdp, bool enable)
 {
-	u8 msg[5];
-	int ret, i;
-
-	msg[0] = GENERAL_MAIN_CONTROL;
-	msg[1] = MB_MODULE_ID_GENERAL;
-	msg[2] = 0;
-	msg[3] = 1;
-	msg[4] = enable ? FW_ACTIVE : FW_STANDBY;
-
-	mutex_lock(&mhdp->mbox_mutex);
-
-	for (i = 0; i < sizeof(msg); i++) {
-		ret = cdns_mhdp_mailbox_write(mhdp, msg[i]);
-		if (ret)
-			goto out;
-	}
-
-	/* read the firmware state */
-	ret = cdns_mhdp_mailbox_recv_data(mhdp, msg, sizeof(msg));
-	if (ret)
-		goto out;
-
-	ret = 0;
+	u8 status;
+	int ret;
 
-out:
-	mutex_unlock(&mhdp->mbox_mutex);
+	status = enable ? FW_ACTIVE : FW_STANDBY;
 
+	ret = cdns_mhdp_mailbox_send_recv(&mhdp->base, MB_MODULE_ID_GENERAL,
+					  GENERAL_MAIN_CONTROL,
+					  sizeof(status), &status,
+					  sizeof(status), &status);
 	if (ret < 0)
 		dev_err(mhdp->dev, "set firmware active failed\n");
 	return ret;
@@ -380,34 +96,18 @@ int cdns_mhdp_get_hpd_status(struct cdns_mhdp_device *mhdp)
 	u8 status;
 	int ret;
 
-	mutex_lock(&mhdp->mbox_mutex);
-
-	ret = cdns_mhdp_mailbox_send(mhdp, MB_MODULE_ID_DP_TX,
-				     DPTX_HPD_STATE, 0, NULL);
-	if (ret)
-		goto err_get_hpd;
-
-	ret = cdns_mhdp_mailbox_recv_header(mhdp, MB_MODULE_ID_DP_TX,
-					    DPTX_HPD_STATE,
-					    sizeof(status));
-	if (ret)
-		goto err_get_hpd;
+	ret = cdns_mhdp_mailbox_send_recv(&mhdp->base, MB_MODULE_ID_DP_TX,
+					  DPTX_HPD_STATE,
+					  0, NULL,
+					  sizeof(status), &status);
 
-	ret = cdns_mhdp_mailbox_recv_data(mhdp, &status, sizeof(status));
 	if (ret)
-		goto err_get_hpd;
-
-	mutex_unlock(&mhdp->mbox_mutex);
+		return ret;
 
 	dev_dbg(mhdp->dev, "%s: HPD %splugged\n", __func__,
 		status ? "" : "un");
 
 	return status;
-
-err_get_hpd:
-	mutex_unlock(&mhdp->mbox_mutex);
-
-	return ret;
 }
 
 static
@@ -418,28 +118,17 @@ int cdns_mhdp_get_edid_block(void *data, u8 *edid,
 	u8 msg[2], reg[2], i;
 	int ret;
 
-	mutex_lock(&mhdp->mbox_mutex);
-
 	for (i = 0; i < 4; i++) {
 		msg[0] = block / 2;
 		msg[1] = block % 2;
 
-		ret = cdns_mhdp_mailbox_send(mhdp, MB_MODULE_ID_DP_TX,
-					     DPTX_GET_EDID, sizeof(msg), msg);
-		if (ret)
-			continue;
-
-		ret = cdns_mhdp_mailbox_recv_header(mhdp, MB_MODULE_ID_DP_TX,
-						    DPTX_GET_EDID,
-						    sizeof(reg) + length);
-		if (ret)
-			continue;
-
-		ret = cdns_mhdp_mailbox_recv_data(mhdp, reg, sizeof(reg));
-		if (ret)
-			continue;
-
-		ret = cdns_mhdp_mailbox_recv_data(mhdp, edid, length);
+		ret = cdns_mhdp_mailbox_send_recv_multi(&mhdp->base,
+							MB_MODULE_ID_DP_TX,
+							DPTX_GET_EDID,
+							sizeof(msg), msg,
+							DPTX_GET_EDID,
+							sizeof(reg), reg,
+							length, edid);
 		if (ret)
 			continue;
 
@@ -447,8 +136,6 @@ int cdns_mhdp_get_edid_block(void *data, u8 *edid,
 			break;
 	}
 
-	mutex_unlock(&mhdp->mbox_mutex);
-
 	if (ret)
 		dev_err(mhdp->dev, "get block[%d] edid failed: %d\n",
 			block, ret);
@@ -462,21 +149,9 @@ int cdns_mhdp_read_hpd_event(struct cdns_mhdp_device *mhdp)
 	u8 event = 0;
 	int ret;
 
-	mutex_lock(&mhdp->mbox_mutex);
-
-	ret = cdns_mhdp_mailbox_send(mhdp, MB_MODULE_ID_DP_TX,
-				     DPTX_READ_EVENT, 0, NULL);
-	if (ret)
-		goto out;
-
-	ret = cdns_mhdp_mailbox_recv_header(mhdp, MB_MODULE_ID_DP_TX,
-					    DPTX_READ_EVENT, sizeof(event));
-	if (ret < 0)
-		goto out;
-
-	ret = cdns_mhdp_mailbox_recv_data(mhdp, &event, sizeof(event));
-out:
-	mutex_unlock(&mhdp->mbox_mutex);
+	ret = cdns_mhdp_mailbox_send_recv(&mhdp->base, MB_MODULE_ID_DP_TX,
+					  DPTX_READ_EVENT,
+					  0, NULL, sizeof(event), &event);
 
 	if (ret < 0)
 		return ret;
@@ -510,35 +185,23 @@ int cdns_mhdp_adjust_lt(struct cdns_mhdp_device *mhdp, unsigned int nlanes,
 	put_unaligned_be16(udelay, payload + 1);
 	memcpy(payload + 3, lanes_data, nlanes);
 
-	mutex_lock(&mhdp->mbox_mutex);
-
-	ret = cdns_mhdp_mailbox_send(mhdp, MB_MODULE_ID_DP_TX,
-				     DPTX_ADJUST_LT,
-				     sizeof(payload), payload);
-	if (ret)
-		goto out;
-
 	/* Yes, read the DPCD read command response */
-	ret = cdns_mhdp_mailbox_recv_header(mhdp, MB_MODULE_ID_DP_TX,
-					    DPTX_READ_DPCD,
-					    sizeof(hdr) + DP_LINK_STATUS_SIZE);
-	if (ret)
-		goto out;
-
-	ret = cdns_mhdp_mailbox_recv_data(mhdp, hdr, sizeof(hdr));
+	ret = cdns_mhdp_mailbox_send_recv_multi(&mhdp->base,
+						MB_MODULE_ID_DP_TX,
+						DPTX_ADJUST_LT,
+						sizeof(payload), payload,
+						DPTX_READ_DPCD,
+						sizeof(hdr), hdr,
+						DP_LINK_STATUS_SIZE,
+						link_status);
 	if (ret)
 		goto out;
 
 	addr = get_unaligned_be24(hdr + 2);
 	if (addr != DP_LANE0_1_STATUS)
-		goto out;
-
-	ret = cdns_mhdp_mailbox_recv_data(mhdp, link_status,
-					  DP_LINK_STATUS_SIZE);
+		ret = -EINVAL;
 
 out:
-	mutex_unlock(&mhdp->mbox_mutex);
-
 	if (ret)
 		dev_err(mhdp->dev, "Failed to adjust Link Training.\n");
 
@@ -847,7 +510,7 @@ static ssize_t cdns_mhdp_transfer(struct drm_dp_aux *aux,
 		unsigned int i;
 
 		for (i = 0; i < msg->size; ++i) {
-			ret = cdns_mhdp_dpcd_write(mhdp,
+			ret = cdns_mhdp_dpcd_write(&mhdp->base,
 						   msg->address + i, buf[i]);
 			if (!ret)
 				continue;
@@ -859,7 +522,7 @@ static ssize_t cdns_mhdp_transfer(struct drm_dp_aux *aux,
 			return ret;
 		}
 	} else {
-		ret = cdns_mhdp_dpcd_read(mhdp, msg->address,
+		ret = cdns_mhdp_dpcd_read(&mhdp->base, msg->address,
 					  msg->buffer, msg->size);
 		if (ret) {
 			dev_err(mhdp->dev,
@@ -887,12 +550,12 @@ static int cdns_mhdp_link_training_init(struct cdns_mhdp_device *mhdp)
 	if (!mhdp->host.scrambler)
 		reg32 |= CDNS_PHY_SCRAMBLER_BYPASS;
 
-	cdns_mhdp_reg_write(mhdp, CDNS_DPTX_PHY_CONFIG, reg32);
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DPTX_PHY_CONFIG, reg32);
 
-	cdns_mhdp_reg_write(mhdp, CDNS_DP_ENHNCD,
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DP_ENHNCD,
 			    mhdp->sink.enhanced & mhdp->host.enhanced);
 
-	cdns_mhdp_reg_write(mhdp, CDNS_DP_LANE_EN,
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DP_LANE_EN,
 			    CDNS_DP_LANE_EN_LANES(mhdp->link.num_lanes));
 
 	cdns_mhdp_link_configure(&mhdp->aux, &mhdp->link);
@@ -913,7 +576,7 @@ static int cdns_mhdp_link_training_init(struct cdns_mhdp_device *mhdp)
 		return ret;
 	}
 
-	cdns_mhdp_reg_write(mhdp, CDNS_DPTX_PHY_CONFIG,
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DPTX_PHY_CONFIG,
 			    CDNS_PHY_COMMON_CONFIG |
 			    CDNS_PHY_TRAINING_EN |
 			    CDNS_PHY_TRAINING_TYPE(1) |
@@ -1058,7 +721,7 @@ static bool cdns_mhdp_link_training_channel_eq(struct cdns_mhdp_device *mhdp,
 		CDNS_PHY_TRAINING_TYPE(eq_tps);
 	if (eq_tps != 4)
 		reg32 |= CDNS_PHY_SCRAMBLER_BYPASS;
-	cdns_mhdp_reg_write(mhdp, CDNS_DPTX_PHY_CONFIG, reg32);
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DPTX_PHY_CONFIG, reg32);
 
 	drm_dp_dpcd_writeb(&mhdp->aux, DP_TRAINING_PATTERN_SET,
 			   (eq_tps != 4) ? eq_tps | DP_LINK_SCRAMBLING_DISABLE :
@@ -1322,7 +985,7 @@ static int cdns_mhdp_link_training(struct cdns_mhdp_device *mhdp,
 			   mhdp->host.scrambler ? 0 :
 			   DP_LINK_SCRAMBLING_DISABLE);
 
-	ret = cdns_mhdp_reg_read(mhdp, CDNS_DP_FRAMER_GLOBAL_CONFIG, &reg32);
+	ret = cdns_mhdp_reg_read(&mhdp->base, CDNS_DP_FRAMER_GLOBAL_CONFIG, &reg32);
 	if (ret < 0) {
 		dev_err(mhdp->dev,
 			"Failed to read CDNS_DP_FRAMER_GLOBAL_CONFIG %d\n",
@@ -1333,13 +996,13 @@ static int cdns_mhdp_link_training(struct cdns_mhdp_device *mhdp,
 	reg32 |= CDNS_DP_NUM_LANES(mhdp->link.num_lanes);
 	reg32 |= CDNS_DP_WR_FAILING_EDGE_VSYNC;
 	reg32 |= CDNS_DP_FRAMER_EN;
-	cdns_mhdp_reg_write(mhdp, CDNS_DP_FRAMER_GLOBAL_CONFIG, reg32);
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DP_FRAMER_GLOBAL_CONFIG, reg32);
 
 	/* Reset PHY config */
 	reg32 = CDNS_PHY_COMMON_CONFIG | CDNS_PHY_TRAINING_TYPE(1);
 	if (!mhdp->host.scrambler)
 		reg32 |= CDNS_PHY_SCRAMBLER_BYPASS;
-	cdns_mhdp_reg_write(mhdp, CDNS_DPTX_PHY_CONFIG, reg32);
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DPTX_PHY_CONFIG, reg32);
 
 	return 0;
 err:
@@ -1347,7 +1010,7 @@ static int cdns_mhdp_link_training(struct cdns_mhdp_device *mhdp,
 	reg32 = CDNS_PHY_COMMON_CONFIG | CDNS_PHY_TRAINING_TYPE(1);
 	if (!mhdp->host.scrambler)
 		reg32 |= CDNS_PHY_SCRAMBLER_BYPASS;
-	cdns_mhdp_reg_write(mhdp, CDNS_DPTX_PHY_CONFIG, reg32);
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DPTX_PHY_CONFIG, reg32);
 
 	drm_dp_dpcd_writeb(&mhdp->aux, DP_TRAINING_PATTERN_SET,
 			   DP_TRAINING_PATTERN_DISABLE);
@@ -1461,7 +1124,7 @@ static int cdns_mhdp_link_up(struct cdns_mhdp_device *mhdp)
 	mhdp->link.num_lanes = cdns_mhdp_max_num_lanes(mhdp);
 
 	/* Disable framer for link training */
-	err = cdns_mhdp_reg_read(mhdp, CDNS_DP_FRAMER_GLOBAL_CONFIG, &resp);
+	err = cdns_mhdp_reg_read(&mhdp->base, CDNS_DP_FRAMER_GLOBAL_CONFIG, &resp);
 	if (err < 0) {
 		dev_err(mhdp->dev,
 			"Failed to read CDNS_DP_FRAMER_GLOBAL_CONFIG %d\n",
@@ -1470,7 +1133,7 @@ static int cdns_mhdp_link_up(struct cdns_mhdp_device *mhdp)
 	}
 
 	resp &= ~CDNS_DP_FRAMER_EN;
-	cdns_mhdp_reg_write(mhdp, CDNS_DP_FRAMER_GLOBAL_CONFIG, resp);
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DP_FRAMER_GLOBAL_CONFIG, resp);
 
 	/* Spread AMP if required, enable 8b/10b coding */
 	amp[0] = cdns_mhdp_get_ssc_supported(mhdp) ? DP_SPREAD_AMP_0_5 : 0;
@@ -1834,7 +1497,7 @@ static void cdns_mhdp_configure_video(struct cdns_mhdp_device *mhdp,
 	if (mode->flags & DRM_MODE_FLAG_INTERLACE)
 		bnd_hsync2vsync |= CDNS_IP_DET_INTERLACE_FORMAT;
 
-	cdns_mhdp_reg_write(mhdp, CDNS_BND_HSYNC2VSYNC(stream_id),
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_BND_HSYNC2VSYNC(stream_id),
 			    bnd_hsync2vsync);
 
 	hsync2vsync_pol_ctrl = 0;
@@ -1842,10 +1505,10 @@ static void cdns_mhdp_configure_video(struct cdns_mhdp_device *mhdp,
 		hsync2vsync_pol_ctrl |= CDNS_H2V_HSYNC_POL_ACTIVE_LOW;
 	if (mode->flags & DRM_MODE_FLAG_NVSYNC)
 		hsync2vsync_pol_ctrl |= CDNS_H2V_VSYNC_POL_ACTIVE_LOW;
-	cdns_mhdp_reg_write(mhdp, CDNS_HSYNC2VSYNC_POL_CTRL(stream_id),
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_HSYNC2VSYNC_POL_CTRL(stream_id),
 			    hsync2vsync_pol_ctrl);
 
-	cdns_mhdp_reg_write(mhdp, CDNS_DP_FRAMER_PXL_REPR(stream_id), pxl_repr);
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DP_FRAMER_PXL_REPR(stream_id), pxl_repr);
 
 	if (mode->flags & DRM_MODE_FLAG_INTERLACE)
 		dp_framer_sp |= CDNS_DP_FRAMER_INTERLACE;
@@ -1853,19 +1516,19 @@ static void cdns_mhdp_configure_video(struct cdns_mhdp_device *mhdp,
 		dp_framer_sp |= CDNS_DP_FRAMER_HSYNC_POL_LOW;
 	if (mode->flags & DRM_MODE_FLAG_NVSYNC)
 		dp_framer_sp |= CDNS_DP_FRAMER_VSYNC_POL_LOW;
-	cdns_mhdp_reg_write(mhdp, CDNS_DP_FRAMER_SP(stream_id), dp_framer_sp);
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DP_FRAMER_SP(stream_id), dp_framer_sp);
 
 	front_porch = mode->crtc_hsync_start - mode->crtc_hdisplay;
 	back_porch = mode->crtc_htotal - mode->crtc_hsync_end;
-	cdns_mhdp_reg_write(mhdp, CDNS_DP_FRONT_BACK_PORCH(stream_id),
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DP_FRONT_BACK_PORCH(stream_id),
 			    CDNS_DP_FRONT_PORCH(front_porch) |
 			    CDNS_DP_BACK_PORCH(back_porch));
 
-	cdns_mhdp_reg_write(mhdp, CDNS_DP_BYTE_COUNT(stream_id),
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DP_BYTE_COUNT(stream_id),
 			    mode->crtc_hdisplay * bpp / 8);
 
 	msa_h0 = mode->crtc_htotal - mode->crtc_hsync_start;
-	cdns_mhdp_reg_write(mhdp, CDNS_DP_MSA_HORIZONTAL_0(stream_id),
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DP_MSA_HORIZONTAL_0(stream_id),
 			    CDNS_DP_MSAH0_H_TOTAL(mode->crtc_htotal) |
 			    CDNS_DP_MSAH0_HSYNC_START(msa_h0));
 
@@ -1874,11 +1537,11 @@ static void cdns_mhdp_configure_video(struct cdns_mhdp_device *mhdp,
 			   CDNS_DP_MSAH1_HDISP_WIDTH(mode->crtc_hdisplay);
 	if (mode->flags & DRM_MODE_FLAG_NHSYNC)
 		msa_horizontal_1 |= CDNS_DP_MSAH1_HSYNC_POL_LOW;
-	cdns_mhdp_reg_write(mhdp, CDNS_DP_MSA_HORIZONTAL_1(stream_id),
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DP_MSA_HORIZONTAL_1(stream_id),
 			    msa_horizontal_1);
 
 	msa_v0 = mode->crtc_vtotal - mode->crtc_vsync_start;
-	cdns_mhdp_reg_write(mhdp, CDNS_DP_MSA_VERTICAL_0(stream_id),
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DP_MSA_VERTICAL_0(stream_id),
 			    CDNS_DP_MSAV0_V_TOTAL(mode->crtc_vtotal) |
 			    CDNS_DP_MSAV0_VSYNC_START(msa_v0));
 
@@ -1887,7 +1550,7 @@ static void cdns_mhdp_configure_video(struct cdns_mhdp_device *mhdp,
 			 CDNS_DP_MSAV1_VDISP_WIDTH(mode->crtc_vdisplay);
 	if (mode->flags & DRM_MODE_FLAG_NVSYNC)
 		msa_vertical_1 |= CDNS_DP_MSAV1_VSYNC_POL_LOW;
-	cdns_mhdp_reg_write(mhdp, CDNS_DP_MSA_VERTICAL_1(stream_id),
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DP_MSA_VERTICAL_1(stream_id),
 			    msa_vertical_1);
 
 	if ((mode->flags & DRM_MODE_FLAG_INTERLACE) &&
@@ -1899,14 +1562,14 @@ static void cdns_mhdp_configure_video(struct cdns_mhdp_device *mhdp,
 	if (pxlfmt == DRM_COLOR_FORMAT_YCBCR420)
 		misc1 = CDNS_DP_TEST_VSC_SDP;
 
-	cdns_mhdp_reg_write(mhdp, CDNS_DP_MSA_MISC(stream_id),
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DP_MSA_MISC(stream_id),
 			    misc0 | (misc1 << 8));
 
-	cdns_mhdp_reg_write(mhdp, CDNS_DP_HORIZONTAL(stream_id),
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DP_HORIZONTAL(stream_id),
 			    CDNS_DP_H_HSYNC_WIDTH(hsync) |
 			    CDNS_DP_H_H_TOTAL(mode->crtc_hdisplay));
 
-	cdns_mhdp_reg_write(mhdp, CDNS_DP_VERTICAL_0(stream_id),
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DP_VERTICAL_0(stream_id),
 			    CDNS_DP_V0_VHEIGHT(mode->crtc_vdisplay) |
 			    CDNS_DP_V0_VSTART(msa_v0));
 
@@ -1915,13 +1578,13 @@ static void cdns_mhdp_configure_video(struct cdns_mhdp_device *mhdp,
 	    mode->crtc_vtotal % 2 == 0)
 		dp_vertical_1 |= CDNS_DP_V1_VTOTAL_EVEN;
 
-	cdns_mhdp_reg_write(mhdp, CDNS_DP_VERTICAL_1(stream_id), dp_vertical_1);
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DP_VERTICAL_1(stream_id), dp_vertical_1);
 
-	cdns_mhdp_reg_write_bit(mhdp, CDNS_DP_VB_ID(stream_id), 2, 1,
-				(mode->flags & DRM_MODE_FLAG_INTERLACE) ?
-				CDNS_DP_VB_ID_INTERLACED : 0);
+	cdns_mhdp_dp_reg_write_bit(&mhdp->base, CDNS_DP_VB_ID(stream_id), 2, 1,
+				   (mode->flags & DRM_MODE_FLAG_INTERLACE) ?
+				   CDNS_DP_VB_ID_INTERLACED : 0);
 
-	ret = cdns_mhdp_reg_read(mhdp, CDNS_DP_FRAMER_GLOBAL_CONFIG, &framer);
+	ret = cdns_mhdp_reg_read(&mhdp->base, CDNS_DP_FRAMER_GLOBAL_CONFIG, &framer);
 	if (ret < 0) {
 		dev_err(mhdp->dev,
 			"Failed to read CDNS_DP_FRAMER_GLOBAL_CONFIG %d\n",
@@ -1930,7 +1593,7 @@ static void cdns_mhdp_configure_video(struct cdns_mhdp_device *mhdp,
 	}
 	framer |= CDNS_DP_FRAMER_EN;
 	framer &= ~CDNS_DP_NO_VIDEO_MODE;
-	cdns_mhdp_reg_write(mhdp, CDNS_DP_FRAMER_GLOBAL_CONFIG, framer);
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DP_FRAMER_GLOBAL_CONFIG, framer);
 }
 
 static void cdns_mhdp_sst_enable(struct cdns_mhdp_device *mhdp,
@@ -1963,15 +1626,15 @@ static void cdns_mhdp_sst_enable(struct cdns_mhdp_device *mhdp,
 
 	mhdp->stream_id = 0;
 
-	cdns_mhdp_reg_write(mhdp, CDNS_DP_FRAMER_TU,
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DP_FRAMER_TU,
 			    CDNS_DP_FRAMER_TU_VS(vs) |
 			    CDNS_DP_FRAMER_TU_SIZE(tu_size) |
 			    CDNS_DP_FRAMER_TU_CNT_RST_EN);
 
-	cdns_mhdp_reg_write(mhdp, CDNS_DP_LINE_THRESH(0),
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DP_LINE_THRESH(0),
 			    line_thresh & GENMASK(5, 0));
 
-	cdns_mhdp_reg_write(mhdp, CDNS_DP_STREAM_CONFIG_2(0),
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DP_STREAM_CONFIG_2(0),
 			    CDNS_DP_SC2_TU_VS_DIFF((tu_size - vs > 3) ?
 						   0 : tu_size - vs));
 
@@ -2006,13 +1669,13 @@ static void cdns_mhdp_atomic_enable(struct drm_bridge *bridge,
 		mhdp->info->ops->enable(mhdp);
 
 	/* Enable VIF clock for stream 0 */
-	ret = cdns_mhdp_reg_read(mhdp, CDNS_DPTX_CAR, &resp);
+	ret = cdns_mhdp_reg_read(&mhdp->base, CDNS_DPTX_CAR, &resp);
 	if (ret < 0) {
 		dev_err(mhdp->dev, "Failed to read CDNS_DPTX_CAR %d\n", ret);
 		goto out;
 	}
 
-	cdns_mhdp_reg_write(mhdp, CDNS_DPTX_CAR,
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DPTX_CAR,
 			    resp | CDNS_VIF_CLK_EN | CDNS_VIF_CLK_RSTN);
 
 	connector = drm_atomic_get_new_connector_for_encoder(state,
@@ -2083,16 +1746,16 @@ static void cdns_mhdp_atomic_disable(struct drm_bridge *bridge,
 		cdns_mhdp_hdcp_disable(mhdp);
 
 	mhdp->bridge_enabled = false;
-	cdns_mhdp_reg_read(mhdp, CDNS_DP_FRAMER_GLOBAL_CONFIG, &resp);
+	cdns_mhdp_reg_read(&mhdp->base, CDNS_DP_FRAMER_GLOBAL_CONFIG, &resp);
 	resp &= ~CDNS_DP_FRAMER_EN;
 	resp |= CDNS_DP_NO_VIDEO_MODE;
-	cdns_mhdp_reg_write(mhdp, CDNS_DP_FRAMER_GLOBAL_CONFIG, resp);
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DP_FRAMER_GLOBAL_CONFIG, resp);
 
 	cdns_mhdp_link_down(mhdp);
 
 	/* Disable VIF clock for stream 0 */
-	cdns_mhdp_reg_read(mhdp, CDNS_DPTX_CAR, &resp);
-	cdns_mhdp_reg_write(mhdp, CDNS_DPTX_CAR,
+	cdns_mhdp_reg_read(&mhdp->base, CDNS_DPTX_CAR, &resp);
+	cdns_mhdp_reg_write(&mhdp->base, CDNS_DPTX_CAR,
 			    resp & ~(CDNS_VIF_CLK_EN | CDNS_VIF_CLK_RSTN));
 
 	if (mhdp->info && mhdp->info->ops && mhdp->info->ops->disable)
@@ -2471,7 +2134,6 @@ static int cdns_mhdp_probe(struct platform_device *pdev)
 
 	mhdp->clk = clk;
 	mhdp->dev = dev;
-	mutex_init(&mhdp->mbox_mutex);
 	mutex_init(&mhdp->link_mutex);
 	spin_lock_init(&mhdp->start_lock);
 
@@ -2502,6 +2164,11 @@ static int cdns_mhdp_probe(struct platform_device *pdev)
 
 	platform_set_drvdata(pdev, mhdp);
 
+	/* init base struct for access mailbox  */
+	mhdp->base.dev = mhdp->dev;
+	mhdp->base.regs = mhdp->regs;
+	mhdp->base.sapb_regs = mhdp->sapb_regs;
+
 	mhdp->info = of_device_get_match_data(dev);
 
 	clk_prepare_enable(clk);
diff --git a/drivers/gpu/drm/bridge/cadence/cdns-mhdp8546-core.h b/drivers/gpu/drm/bridge/cadence/cdns-mhdp8546-core.h
index bad2fc0c73066..535300d040dea 100644
--- a/drivers/gpu/drm/bridge/cadence/cdns-mhdp8546-core.h
+++ b/drivers/gpu/drm/bridge/cadence/cdns-mhdp8546-core.h
@@ -18,6 +18,7 @@
 #include <drm/display/drm_dp_helper.h>
 #include <drm/drm_bridge.h>
 #include <drm/drm_connector.h>
+#include <soc/cadence/cdns-mhdp-helper.h>
 
 struct clk;
 struct device;
@@ -27,10 +28,6 @@ struct phy;
 #define CDNS_APB_CTRL				0x00000
 #define CDNS_CPU_STALL				BIT(3)
 
-#define CDNS_MAILBOX_FULL			0x00008
-#define CDNS_MAILBOX_EMPTY			0x0000c
-#define CDNS_MAILBOX_TX_DATA			0x00010
-#define CDNS_MAILBOX_RX_DATA			0x00014
 #define CDNS_KEEP_ALIVE				0x00018
 #define CDNS_KEEP_ALIVE_MASK			GENMASK(7, 0)
 
@@ -198,45 +195,10 @@ struct phy;
 #define CDNS_DP_BYTE_COUNT(s)			(CDNS_DPTX_STREAM(s) + 0x7c)
 #define CDNS_DP_BYTE_COUNT_BYTES_IN_CHUNK_SHIFT	16
 
-/* mailbox */
-#define MAILBOX_RETRY_US			1000
-#define MAILBOX_TIMEOUT_US			2000000
-
-#define MB_OPCODE_ID				0
-#define MB_MODULE_ID				1
-#define MB_SIZE_MSB_ID				2
-#define MB_SIZE_LSB_ID				3
-#define MB_DATA_ID				4
-
-#define MB_MODULE_ID_DP_TX			0x01
-#define MB_MODULE_ID_HDCP_TX			0x07
-#define MB_MODULE_ID_HDCP_RX			0x08
-#define MB_MODULE_ID_HDCP_GENERAL		0x09
-#define MB_MODULE_ID_GENERAL			0x0a
-
-/* firmware and opcodes */
+/* firmware */
 #define FW_NAME					"cadence/mhdp8546.bin"
 #define CDNS_MHDP_IMEM				0x10000
 
-#define GENERAL_MAIN_CONTROL			0x01
-#define GENERAL_TEST_ECHO			0x02
-#define GENERAL_BUS_SETTINGS			0x03
-#define GENERAL_TEST_ACCESS			0x04
-#define GENERAL_REGISTER_READ			0x07
-
-#define DPTX_SET_POWER_MNG			0x00
-#define DPTX_GET_EDID				0x02
-#define DPTX_READ_DPCD				0x03
-#define DPTX_WRITE_DPCD				0x04
-#define DPTX_ENABLE_EVENT			0x05
-#define DPTX_WRITE_REGISTER			0x06
-#define DPTX_READ_REGISTER			0x07
-#define DPTX_WRITE_FIELD			0x08
-#define DPTX_READ_EVENT				0x0a
-#define DPTX_GET_LAST_AUX_STAUS			0x0e
-#define DPTX_HPD_STATE				0x11
-#define DPTX_ADJUST_LT				0x12
-
 #define FW_STANDBY				0
 #define FW_ACTIVE				1
 
@@ -352,6 +314,8 @@ struct cdns_mhdp_hdcp {
 };
 
 struct cdns_mhdp_device {
+	struct cdns_mhdp_base base;
+
 	void __iomem *regs;
 	void __iomem *sapb_regs;
 	void __iomem *j721e_regs;
@@ -362,9 +326,6 @@ struct cdns_mhdp_device {
 
 	const struct cdns_mhdp_platform_info *info;
 
-	/* This is to protect mailbox communications with the firmware */
-	struct mutex mbox_mutex;
-
 	/*
 	 * "link_mutex" protects the access to all the link parameters
 	 * including the link training process. Link training will be
diff --git a/drivers/gpu/drm/bridge/cadence/cdns-mhdp8546-hdcp.c b/drivers/gpu/drm/bridge/cadence/cdns-mhdp8546-hdcp.c
index 42248f179b69d..3944642f2ebbc 100644
--- a/drivers/gpu/drm/bridge/cadence/cdns-mhdp8546-hdcp.c
+++ b/drivers/gpu/drm/bridge/cadence/cdns-mhdp8546-hdcp.c
@@ -15,144 +15,20 @@
 
 #include "cdns-mhdp8546-hdcp.h"
 
-static int cdns_mhdp_secure_mailbox_read(struct cdns_mhdp_device *mhdp)
-{
-	int ret, empty;
-
-	WARN_ON(!mutex_is_locked(&mhdp->mbox_mutex));
-
-	ret = readx_poll_timeout(readl, mhdp->sapb_regs + CDNS_MAILBOX_EMPTY,
-				 empty, !empty, MAILBOX_RETRY_US,
-				 MAILBOX_TIMEOUT_US);
-	if (ret < 0)
-		return ret;
-
-	return readl(mhdp->sapb_regs + CDNS_MAILBOX_RX_DATA) & 0xff;
-}
-
-static int cdns_mhdp_secure_mailbox_write(struct cdns_mhdp_device *mhdp,
-					  u8 val)
-{
-	int ret, full;
-
-	WARN_ON(!mutex_is_locked(&mhdp->mbox_mutex));
-
-	ret = readx_poll_timeout(readl, mhdp->sapb_regs + CDNS_MAILBOX_FULL,
-				 full, !full, MAILBOX_RETRY_US,
-				 MAILBOX_TIMEOUT_US);
-	if (ret < 0)
-		return ret;
-
-	writel(val, mhdp->sapb_regs + CDNS_MAILBOX_TX_DATA);
-
-	return 0;
-}
-
-static int cdns_mhdp_secure_mailbox_recv_header(struct cdns_mhdp_device *mhdp,
-						u8 module_id,
-						u8 opcode,
-						u16 req_size)
-{
-	u32 mbox_size, i;
-	u8 header[4];
-	int ret;
-
-	/* read the header of the message */
-	for (i = 0; i < sizeof(header); i++) {
-		ret = cdns_mhdp_secure_mailbox_read(mhdp);
-		if (ret < 0)
-			return ret;
-
-		header[i] = ret;
-	}
-
-	mbox_size = get_unaligned_be16(header + 2);
-
-	if (opcode != header[0] || module_id != header[1] ||
-	    (opcode != HDCP_TRAN_IS_REC_ID_VALID && req_size != mbox_size)) {
-		for (i = 0; i < mbox_size; i++)
-			if (cdns_mhdp_secure_mailbox_read(mhdp) < 0)
-				break;
-		return -EINVAL;
-	}
-
-	return 0;
-}
-
-static int cdns_mhdp_secure_mailbox_recv_data(struct cdns_mhdp_device *mhdp,
-					      u8 *buff, u16 buff_size)
-{
-	int ret;
-	u32 i;
-
-	for (i = 0; i < buff_size; i++) {
-		ret = cdns_mhdp_secure_mailbox_read(mhdp);
-		if (ret < 0)
-			return ret;
-
-		buff[i] = ret;
-	}
-
-	return 0;
-}
-
-static int cdns_mhdp_secure_mailbox_send(struct cdns_mhdp_device *mhdp,
-					 u8 module_id,
-					 u8 opcode,
-					 u16 size,
-					 u8 *message)
-{
-	u8 header[4];
-	int ret;
-	u32 i;
-
-	header[0] = opcode;
-	header[1] = module_id;
-	put_unaligned_be16(size, header + 2);
-
-	for (i = 0; i < sizeof(header); i++) {
-		ret = cdns_mhdp_secure_mailbox_write(mhdp, header[i]);
-		if (ret)
-			return ret;
-	}
-
-	for (i = 0; i < size; i++) {
-		ret = cdns_mhdp_secure_mailbox_write(mhdp, message[i]);
-		if (ret)
-			return ret;
-	}
-
-	return 0;
-}
-
 static int cdns_mhdp_hdcp_get_status(struct cdns_mhdp_device *mhdp,
 				     u16 *hdcp_port_status)
 {
 	u8 hdcp_status[HDCP_STATUS_SIZE];
 	int ret;
 
-	mutex_lock(&mhdp->mbox_mutex);
-	ret = cdns_mhdp_secure_mailbox_send(mhdp, MB_MODULE_ID_HDCP_TX,
-					    HDCP_TRAN_STATUS_CHANGE, 0, NULL);
-	if (ret)
-		goto err_get_hdcp_status;
-
-	ret = cdns_mhdp_secure_mailbox_recv_header(mhdp, MB_MODULE_ID_HDCP_TX,
-						   HDCP_TRAN_STATUS_CHANGE,
-						   sizeof(hdcp_status));
-	if (ret)
-		goto err_get_hdcp_status;
-
-	ret = cdns_mhdp_secure_mailbox_recv_data(mhdp, hdcp_status,
-						 sizeof(hdcp_status));
+	ret = cdns_mhdp_secure_mailbox_send_recv(&mhdp->base, MB_MODULE_ID_HDCP_TX,
+						 HDCP_TRAN_STATUS_CHANGE, 0, NULL,
+						 sizeof(hdcp_status), hdcp_status);
 	if (ret)
-		goto err_get_hdcp_status;
+		return ret;
 
 	*hdcp_port_status = ((u16)(hdcp_status[0] << 8) | hdcp_status[1]);
 
-err_get_hdcp_status:
-	mutex_unlock(&mhdp->mbox_mutex);
-
 	return ret;
 }
 
@@ -170,98 +46,52 @@ static u8 cdns_mhdp_hdcp_handle_status(struct cdns_mhdp_device *mhdp,
 static int cdns_mhdp_hdcp_rx_id_valid_response(struct cdns_mhdp_device *mhdp,
 					       u8 valid)
 {
-	int ret;
-
-	mutex_lock(&mhdp->mbox_mutex);
-	ret = cdns_mhdp_secure_mailbox_send(mhdp, MB_MODULE_ID_HDCP_TX,
+	return cdns_mhdp_secure_mailbox_send(&mhdp->base, MB_MODULE_ID_HDCP_TX,
 					    HDCP_TRAN_RESPOND_RECEIVER_ID_VALID,
 					    1, &valid);
-	mutex_unlock(&mhdp->mbox_mutex);
-
-	return ret;
 }
 
 static int cdns_mhdp_hdcp_rx_id_valid(struct cdns_mhdp_device *mhdp,
 				      u8 *recv_num, u8 *hdcp_rx_id)
 {
 	u8 rec_id_hdr[2];
-	u8 status;
 	int ret;
 
-	mutex_lock(&mhdp->mbox_mutex);
-	ret = cdns_mhdp_secure_mailbox_send(mhdp, MB_MODULE_ID_HDCP_TX,
-					    HDCP_TRAN_IS_REC_ID_VALID, 0, NULL);
-	if (ret)
-		goto err_rx_id_valid;
-
-	ret = cdns_mhdp_secure_mailbox_recv_header(mhdp, MB_MODULE_ID_HDCP_TX,
-						   HDCP_TRAN_IS_REC_ID_VALID,
-						   sizeof(status));
-	if (ret)
-		goto err_rx_id_valid;
-
-	ret = cdns_mhdp_secure_mailbox_recv_data(mhdp, rec_id_hdr, 2);
+	ret = cdns_mhdp_secure_mailbox_send_recv_multi(&mhdp->base,
+						       MB_MODULE_ID_HDCP_TX,
+						       HDCP_TRAN_IS_REC_ID_VALID,
+						       0, NULL,
+						       HDCP_TRAN_IS_REC_ID_VALID,
+						       sizeof(rec_id_hdr), rec_id_hdr,
+						       0, hdcp_rx_id);
 	if (ret)
-		goto err_rx_id_valid;
+		return ret;
 
 	*recv_num = rec_id_hdr[0];
 
-	ret = cdns_mhdp_secure_mailbox_recv_data(mhdp, hdcp_rx_id, 5 * *recv_num);
-
-err_rx_id_valid:
-	mutex_unlock(&mhdp->mbox_mutex);
-
-	return ret;
+	return 0;
 }
 
 static int cdns_mhdp_hdcp_km_stored_resp(struct cdns_mhdp_device *mhdp,
 					 u32 size, u8 *km)
 {
-	int ret;
-
-	mutex_lock(&mhdp->mbox_mutex);
-	ret = cdns_mhdp_secure_mailbox_send(mhdp, MB_MODULE_ID_HDCP_TX,
-					    HDCP2X_TX_RESPOND_KM, size, km);
-	mutex_unlock(&mhdp->mbox_mutex);
-
-	return ret;
+	return cdns_mhdp_secure_mailbox_send(&mhdp->base, MB_MODULE_ID_HDCP_TX,
+					     HDCP2X_TX_RESPOND_KM, size, km);
 }
 
 static int cdns_mhdp_hdcp_tx_is_km_stored(struct cdns_mhdp_device *mhdp,
 					  u8 *resp, u32 size)
 {
-	int ret;
-
-	mutex_lock(&mhdp->mbox_mutex);
-	ret = cdns_mhdp_secure_mailbox_send(mhdp, MB_MODULE_ID_HDCP_TX,
-					    HDCP2X_TX_IS_KM_STORED, 0, NULL);
-	if (ret)
-		goto err_is_km_stored;
-
-	ret = cdns_mhdp_secure_mailbox_recv_header(mhdp, MB_MODULE_ID_HDCP_TX,
-						   HDCP2X_TX_IS_KM_STORED,
-						   size);
-	if (ret)
-		goto err_is_km_stored;
-
-	ret = cdns_mhdp_secure_mailbox_recv_data(mhdp, resp, size);
-err_is_km_stored:
-	mutex_unlock(&mhdp->mbox_mutex);
-
-	return ret;
+	return cdns_mhdp_secure_mailbox_send_recv(&mhdp->base, MB_MODULE_ID_HDCP_TX,
+						 HDCP2X_TX_IS_KM_STORED,
+						 0, NULL, size, resp);
 }
 
 static int cdns_mhdp_hdcp_tx_config(struct cdns_mhdp_device *mhdp,
 				    u8 hdcp_cfg)
 {
-	int ret;
-
-	mutex_lock(&mhdp->mbox_mutex);
-	ret = cdns_mhdp_secure_mailbox_send(mhdp, MB_MODULE_ID_HDCP_TX,
-					    HDCP_TRAN_CONFIGURATION, 1, &hdcp_cfg);
-	mutex_unlock(&mhdp->mbox_mutex);
-
-	return ret;
+	return cdns_mhdp_secure_mailbox_send(&mhdp->base, MB_MODULE_ID_HDCP_TX,
+					     HDCP_TRAN_CONFIGURATION, 1, &hdcp_cfg);
 }
 
 static int cdns_mhdp_hdcp_set_config(struct cdns_mhdp_device *mhdp,
diff --git a/drivers/gpu/drm/bridge/cadence/cdns-mhdp8546-hdcp.h b/drivers/gpu/drm/bridge/cadence/cdns-mhdp8546-hdcp.h
index 3b6ec9c3a8d8b..1e68530e72229 100644
--- a/drivers/gpu/drm/bridge/cadence/cdns-mhdp8546-hdcp.h
+++ b/drivers/gpu/drm/bridge/cadence/cdns-mhdp8546-hdcp.h
@@ -9,6 +9,7 @@
 #ifndef CDNS_MHDP8546_HDCP_H
 #define CDNS_MHDP8546_HDCP_H
 
+#include <soc/cadence/cdns-mhdp-helper.h>
 #include "cdns-mhdp8546-core.h"
 
 #define HDCP_MAX_RECEIVERS 32
@@ -32,23 +33,6 @@ enum {
 	HDCP_SET_SEED,
 };
 
-enum {
-	HDCP_TRAN_CONFIGURATION,
-	HDCP2X_TX_SET_PUBLIC_KEY_PARAMS,
-	HDCP2X_TX_SET_DEBUG_RANDOM_NUMBERS,
-	HDCP2X_TX_RESPOND_KM,
-	HDCP1_TX_SEND_KEYS,
-	HDCP1_TX_SEND_RANDOM_AN,
-	HDCP_TRAN_STATUS_CHANGE,
-	HDCP2X_TX_IS_KM_STORED,
-	HDCP2X_TX_STORE_KM,
-	HDCP_TRAN_IS_REC_ID_VALID,
-	HDCP_TRAN_RESPOND_RECEIVER_ID_VALID,
-	HDCP_TRAN_TEST_KEYS,
-	HDCP2X_TX_SET_KM_KEY_PARAMS,
-	HDCP_NUM_OF_SUPPORTED_MESSAGES
-};
-
 enum {
 	HDCP_CONTENT_TYPE_0,
 	HDCP_CONTENT_TYPE_1,

From patchwork Tue Dec 17 06:51:46 2024
Content-Type: text/plain; charset="utf-8"
MIME-Version: 1.0
Content-Transfer-Encoding: 7bit
Subject: [v20,4/9] dt-bindings: display: bridge: Add Cadence MHDP8501
From: Sandor Yu <Sandor.yu@nxp.com>
X-Patchwork-Id: 629291
Message-Id: 
 <f2b7beebeb99ca69021ca24744e29af3454f5620.1734340233.git.Sandor.yu@nxp.com>
To: dmitry.baryshkov@linaro.org, andrzej.hajda@intel.com,
 neil.armstrong@linaro.org, Laurent.pinchart@ideasonboard.com,
 jonas@kwiboo.se, jernej.skrabec@gmail.com, airlied@gmail.com,
 daniel@ffwll.ch, robh+dt@kernel.org, krzysztof.kozlowski+dt@linaro.org,
 shawnguo@kernel.org, s.hauer@pengutronix.de, festevam@gmail.com,
 vkoul@kernel.org, dri-devel@lists.freedesktop.org,
 devicetree@vger.kernel.org, linux-arm-kernel@lists.infradead.org,
 linux-kernel@vger.kernel.org, linux-phy@lists.infradead.org,
 mripard@kernel.org
Cc: kernel@pengutronix.de, linux-imx@nxp.com, Sandor.yu@nxp.com,
 oliver.brown@nxp.com, alexander.stein@ew.tq-group.com, sam@ravnborg.org
Date: Tue, 17 Dec 2024 14:51:46 +0800

Add bindings for Cadence MHDP8501 DisplayPort/HDMI bridge.

Signed-off-by: Sandor Yu <Sandor.yu@nxp.com>
Reviewed-by: Krzysztof Kozlowski <krzysztof.kozlowski@linaro.org>
---
v19->v20:
- remove data type link of data-lanes.

v18->v19:
- move data-lanes property to endpoint of port@1

v17->v18:
- remove lane-mapping and replace it with data-lanes
- remove r-b tag as property changed.

v16->v17:
- Add lane-mapping property

v9->v16:
 *No change

 .../display/bridge/cdns,mhdp8501.yaml         | 121 ++++++++++++++++++
 1 file changed, 121 insertions(+)
 create mode 100644 Documentation/devicetree/bindings/display/bridge/cdns,mhdp8501.yaml

diff --git a/Documentation/devicetree/bindings/display/bridge/cdns,mhdp8501.yaml b/Documentation/devicetree/bindings/display/bridge/cdns,mhdp8501.yaml
new file mode 100644
index 0000000000000..2417f4038b437
--- /dev/null
+++ b/Documentation/devicetree/bindings/display/bridge/cdns,mhdp8501.yaml
@@ -0,0 +1,121 @@
+# SPDX-License-Identifier: (GPL-2.0 OR BSD-2-Clause)
+%YAML 1.2
+---
+$id: http://devicetree.org/schemas/display/bridge/cdns,mhdp8501.yaml#
+$schema: http://devicetree.org/meta-schemas/core.yaml#
+
+title: Cadence MHDP8501 DP/HDMI bridge
+
+maintainers:
+  - Sandor Yu <Sandor.yu@nxp.com>
+
+description:
+  Cadence MHDP8501 DisplayPort/HDMI interface.
+
+properties:
+  compatible:
+    enum:
+      - fsl,imx8mq-mhdp8501
+
+  reg:
+    maxItems: 1
+
+  clocks:
+    maxItems: 1
+    description: MHDP8501 DP/HDMI APB clock.
+
+  phys:
+    maxItems: 1
+    description:
+      phandle to the DP/HDMI PHY
+
+  interrupts:
+    items:
+      - description: Hotplug cable plugin.
+      - description: Hotplug cable plugout.
+
+  interrupt-names:
+    items:
+      - const: plug_in
+      - const: plug_out
+
+  ports:
+    $ref: /schemas/graph.yaml#/properties/ports
+
+    properties:
+      port@0:
+        $ref: /schemas/graph.yaml#/properties/port
+        description:
+          Input port from display controller output.
+
+      port@1:
+        $ref: /schemas/graph.yaml#/$defs/port-base
+        unevaluatedProperties: false
+        description:
+          Output port to DisplayPort or HDMI connector.
+
+        properties:
+          endpoint:
+            $ref: /schemas/media/video-interfaces.yaml#
+            unevaluatedProperties: false
+
+            properties:
+              data-lanes:
+                description: Lane reordering for HDMI or DisplayPort interface.
+                minItems: 4
+                maxItems: 4
+
+            required:
+              - data-lanes
+
+    required:
+      - port@0
+      - port@1
+
+required:
+  - compatible
+  - reg
+  - clocks
+  - interrupts
+  - interrupt-names
+  - phys
+  - ports
+
+additionalProperties: false
+
+examples:
+  - |
+    #include <dt-bindings/clock/imx8mq-clock.h>
+    #include <dt-bindings/interrupt-controller/arm-gic.h>
+
+    mhdp: display-bridge@32c00000 {
+        compatible = "fsl,imx8mq-mhdp8501";
+        reg = <0x32c00000 0x100000>;
+        interrupts = <GIC_SPI 16 IRQ_TYPE_LEVEL_HIGH>,
+                     <GIC_SPI 25 IRQ_TYPE_LEVEL_HIGH>;
+        interrupt-names = "plug_in", "plug_out";
+        clocks = <&clk IMX8MQ_CLK_DISP_APB_ROOT>;
+        phys = <&mdhp_phy>;
+
+        ports {
+            #address-cells = <1>;
+            #size-cells = <0>;
+
+            port@0 {
+                reg = <0>;
+
+                mhdp_in: endpoint {
+                    remote-endpoint = <&dcss_out>;
+                };
+            };
+
+            port@1 {
+                reg = <1>;
+
+                mhdp_out: endpoint {
+                    remote-endpoint = <&dp_connector>;
+                    data-lanes = <2 1 0 3>;
+                };
+            };
+        };
+    };

From patchwork Tue Dec 17 06:51:47 2024
Content-Type: text/plain; charset="utf-8"
MIME-Version: 1.0
Content-Transfer-Encoding: 7bit
Subject: [v20,5/9] drm: bridge: Cadence: Add MHDP8501 DP/HDMI driver
From: Sandor Yu <Sandor.yu@nxp.com>
X-Patchwork-Id: 629292
Message-Id: 
 <fbd12029fab1f60e2ba4fad75ef650298a59cb15.1734340233.git.Sandor.yu@nxp.com>
To: dmitry.baryshkov@linaro.org, andrzej.hajda@intel.com,
 neil.armstrong@linaro.org, Laurent.pinchart@ideasonboard.com,
 jonas@kwiboo.se, jernej.skrabec@gmail.com, airlied@gmail.com,
 daniel@ffwll.ch, robh+dt@kernel.org, krzysztof.kozlowski+dt@linaro.org,
 shawnguo@kernel.org, s.hauer@pengutronix.de, festevam@gmail.com,
 vkoul@kernel.org, dri-devel@lists.freedesktop.org,
 devicetree@vger.kernel.org, linux-arm-kernel@lists.infradead.org,
 linux-kernel@vger.kernel.org, linux-phy@lists.infradead.org,
 mripard@kernel.org
Cc: kernel@pengutronix.de, linux-imx@nxp.com, Sandor.yu@nxp.com,
 oliver.brown@nxp.com, alexander.stein@ew.tq-group.com, sam@ravnborg.org
Date: Tue, 17 Dec 2024 14:51:47 +0800

Add a new DRM DisplayPort and HDMI bridge driver for Candence MHDP8501
used in i.MX8MQ SOC. MHDP8501 could support HDMI or DisplayPort
standards according embedded Firmware running in the uCPU.

For iMX8MQ SOC, the DisplayPort/HDMI FW was loaded and activated by
SOC's ROM code. Bootload binary included respective specific firmware
is required.

Driver will check display connector type and
then load the corresponding driver.

Signed-off-by: Sandor Yu <Sandor.yu@nxp.com>
---
v19->v20:
- Dump mhdp FW version by debugfs
- Combine HDMI and DP cable detect functions into one function
- Combine HDMI and DP cable bridge_mode_valid() functions into one function
- Rename cdns_hdmi_reset_link() to cdns_hdmi_handle_hotplug()
- Add comments for EDID in cdns_hdmi_handle_hotplug() and cdns_dp_check_link_state()
- Add atomic_get_input_bus_fmts() and bridge_atomic_check() for DP driver
- Remove bpc and color_fmt init in atomic_enable() function.
- More detail comments for DDC adapter only support SCDC_I2C_SLAVE_ADDRESS
  read and write in HDMI driver.


v18->v19:
- Get endpoint for data-lanes as it had move to endpoint of port@1
- Update clock management as devm_clk_get_enabled() introduced.
- Fix clear_infoframe() function is not work issue.
- Manage PHY power state via phy_power_on() and phy_power_off().

v17->v18:
- MHDP8501 HDMI and DP commands that need access mailbox are rewrited
  with new API functions created in patch #1.
- replace lane-mapping with data-lanes, use the value from data-lanes
  to reorder HDMI and DP lane mapping.
- create I2C adapter for HDMI SCDC, remove cdns_hdmi_scdc_write() function.
- Rewrite cdns_hdmi_sink_config() function, use HDMI SCDC helper function
  drm_scdc_set_high_tmds_clock_ratio() and drm_scdc_set_scrambling()
  to config HDMI sink TMDS.
- Remove struct video_info from HDMI driver.
- Remove tmds_char_rate_valid() be called in bridge_mode_valid(),
  community had patch in reviewing to implement the function.
- Remove warning message print when get unknown HPD cable status.
- Add more detail comments for HDP plugin and plugout interrupt.
- use dev_dbg to repleace DRM_INFO when cable HPD status changed.
- Remove t-b tag as above code change.

 drivers/gpu/drm/bridge/cadence/Kconfig        |  16 +
 drivers/gpu/drm/bridge/cadence/Makefile       |   2 +
 .../drm/bridge/cadence/cdns-mhdp8501-core.c   | 379 +++++++++
 .../drm/bridge/cadence/cdns-mhdp8501-core.h   | 380 +++++++++
 .../gpu/drm/bridge/cadence/cdns-mhdp8501-dp.c | 694 ++++++++++++++++
 .../drm/bridge/cadence/cdns-mhdp8501-hdmi.c   | 745 ++++++++++++++++++
 6 files changed, 2216 insertions(+)
 create mode 100644 drivers/gpu/drm/bridge/cadence/cdns-mhdp8501-core.c
 create mode 100644 drivers/gpu/drm/bridge/cadence/cdns-mhdp8501-core.h
 create mode 100644 drivers/gpu/drm/bridge/cadence/cdns-mhdp8501-dp.c
 create mode 100644 drivers/gpu/drm/bridge/cadence/cdns-mhdp8501-hdmi.c

diff --git a/drivers/gpu/drm/bridge/cadence/Kconfig b/drivers/gpu/drm/bridge/cadence/Kconfig
index dbb06533ccab2..bd979f3e6df48 100644
--- a/drivers/gpu/drm/bridge/cadence/Kconfig
+++ b/drivers/gpu/drm/bridge/cadence/Kconfig
@@ -48,3 +48,19 @@ config DRM_CDNS_MHDP8546_J721E
 	  initializes the J721E Display Port and sets up the
 	  clock and data muxes.
 endif
+
+config DRM_CDNS_MHDP8501
+	tristate "Cadence MHDP8501 DP/HDMI bridge"
+	select DRM_KMS_HELPER
+	select DRM_PANEL_BRIDGE
+	select DRM_DISPLAY_DP_HELPER
+	select DRM_DISPLAY_HELPER
+	select DRM_CDNS_AUDIO
+	select CDNS_MHDP_HELPER
+	depends on OF
+	help
+	  Support Cadence MHDP8501 DisplayPort/HDMI bridge.
+	  Cadence MHDP8501 support one or more protocols,
+	  including DisplayPort and HDMI.
+	  To use the DP and HDMI drivers, their respective
+	  specific firmware is required.
diff --git a/drivers/gpu/drm/bridge/cadence/Makefile b/drivers/gpu/drm/bridge/cadence/Makefile
index c95fd5b81d137..ea327287d1c14 100644
--- a/drivers/gpu/drm/bridge/cadence/Makefile
+++ b/drivers/gpu/drm/bridge/cadence/Makefile
@@ -5,3 +5,5 @@ cdns-dsi-$(CONFIG_DRM_CDNS_DSI_J721E) += cdns-dsi-j721e.o
 obj-$(CONFIG_DRM_CDNS_MHDP8546) += cdns-mhdp8546.o
 cdns-mhdp8546-y := cdns-mhdp8546-core.o cdns-mhdp8546-hdcp.o
 cdns-mhdp8546-$(CONFIG_DRM_CDNS_MHDP8546_J721E) += cdns-mhdp8546-j721e.o
+obj-$(CONFIG_DRM_CDNS_MHDP8501) += cdns-mhdp8501.o
+cdns-mhdp8501-y := cdns-mhdp8501-core.o cdns-mhdp8501-dp.o cdns-mhdp8501-hdmi.o
diff --git a/drivers/gpu/drm/bridge/cadence/cdns-mhdp8501-core.c b/drivers/gpu/drm/bridge/cadence/cdns-mhdp8501-core.c
new file mode 100644
index 0000000000000..98116ef012fa3
--- /dev/null
+++ b/drivers/gpu/drm/bridge/cadence/cdns-mhdp8501-core.c
@@ -0,0 +1,379 @@
+// SPDX-License-Identifier: GPL-2.0-only
+/*
+ * Cadence Display Port Interface (DP) driver
+ *
+ * Copyright (C) 2023-2024 NXP Semiconductor, Inc.
+ *
+ */
+#include <drm/drm_of.h>
+#include <drm/drm_print.h>
+#include <linux/clk.h>
+#include <linux/irq.h>
+#include <linux/mutex.h>
+#include <linux/of_device.h>
+#include <linux/platform_device.h>
+#include <linux/phy/phy.h>
+
+#include "cdns-mhdp8501-core.h"
+
+static ssize_t firmware_version_show(struct device *dev,
+				     struct device_attribute *attr, char *buf);
+static struct device_attribute firmware_version = __ATTR_RO(firmware_version);
+
+ssize_t firmware_version_show(struct device *dev,
+			      struct device_attribute *attr, char *buf)
+{
+	struct cdns_mhdp8501_device *mhdp = dev_get_drvdata(dev);
+
+	u32 version = readl(mhdp->base.regs + VER_L) | readl(mhdp->base.regs + VER_H) << 8;
+	u32 lib_version = readl(mhdp->base.regs + VER_LIB_L_ADDR) |
+			  readl(mhdp->base.regs + VER_LIB_H_ADDR) << 8;
+
+	return sprintf(buf, "FW version %d, Lib version %d\n", version, lib_version);
+}
+
+static void cdns_mhdp8501_create_device_files(struct cdns_mhdp8501_device *mhdp)
+{
+	if (device_create_file(mhdp->dev, &firmware_version)) {
+		DRM_ERROR("Unable to create firmware_version sysfs\n");
+		device_remove_file(mhdp->dev, &firmware_version);
+	}
+}
+
+static void cdns_mhdp8501_remove_device_files(struct cdns_mhdp8501_device *mhdp)
+{
+	device_remove_file(mhdp->dev, &firmware_version);
+}
+
+static int cdns_mhdp8501_read_hpd(struct cdns_mhdp8501_device *mhdp)
+{
+	u8 status;
+	int ret;
+
+	ret = cdns_mhdp_mailbox_send_recv(&mhdp->base, MB_MODULE_ID_GENERAL,
+					  GENERAL_GET_HPD_STATE,
+					  0, NULL, sizeof(status), &status);
+	if (ret) {
+		dev_err(mhdp->dev, "read hpd failed: %d\n", ret);
+		return ret;
+	}
+
+	return status;
+}
+
+enum drm_connector_status cdns_mhdp8501_detect(struct drm_bridge *bridge)
+{
+	struct cdns_mhdp8501_device *mhdp = bridge->driver_private;
+
+	u8 hpd = 0xf;
+
+	hpd = cdns_mhdp8501_read_hpd(mhdp);
+	if (hpd == 1)
+		return connector_status_connected;
+	else if (hpd == 0)
+		return connector_status_disconnected;
+
+	return connector_status_unknown;
+}
+
+enum drm_mode_status
+cdns_mhdp8501_mode_valid(struct drm_bridge *bridge,
+			 const struct drm_display_info *info,
+			 const struct drm_display_mode *mode)
+{
+	/* We don't support double-clocked */
+	if (mode->flags & DRM_MODE_FLAG_DBLCLK)
+		return MODE_BAD;
+
+	/* MAX support pixel clock rate 594MHz */
+	if (mode->clock > 594000)
+		return MODE_CLOCK_HIGH;
+
+	if (mode->hdisplay > 3840)
+		return MODE_BAD_HVALUE;
+
+	if (mode->vdisplay > 2160)
+		return MODE_BAD_VVALUE;
+
+	return MODE_OK;
+}
+
+static void hotplug_work_func(struct work_struct *work)
+{
+	struct cdns_mhdp8501_device *mhdp = container_of(work,
+						     struct cdns_mhdp8501_device,
+						     hotplug_work.work);
+	enum drm_connector_status status = cdns_mhdp8501_detect(&mhdp->bridge);
+
+	drm_bridge_hpd_notify(&mhdp->bridge, status);
+
+	/*
+	 * iMX8MQ has two HPD interrupts: one for plugout and one for plugin.
+	 * These interrupts cannot be masked and cleaned, so we must enable one
+	 * and disable the other to avoid continuous interrupt generation.
+	 */
+	if (status == connector_status_connected) {
+		/* Cable connected  */
+		dev_dbg(mhdp->dev, "HDMI/DP Cable Plug In\n");
+		enable_irq(mhdp->irq[IRQ_OUT]);
+
+		/* Reset HDMI/DP link with sink */
+		if (mhdp->connector_type == DRM_MODE_CONNECTOR_HDMIA)
+			cdns_hdmi_handle_hotplug(mhdp);
+		else
+			cdns_dp_check_link_state(mhdp);
+
+	} else if (status == connector_status_disconnected) {
+		/* Cable Disconnected  */
+		dev_dbg(mhdp->dev, "HDMI/DP Cable Plug Out\n");
+		enable_irq(mhdp->irq[IRQ_IN]);
+	}
+}
+
+static irqreturn_t cdns_mhdp8501_irq_thread(int irq, void *data)
+{
+	struct cdns_mhdp8501_device *mhdp = data;
+
+	disable_irq_nosync(irq);
+
+	mod_delayed_work(system_wq, &mhdp->hotplug_work,
+			 msecs_to_jiffies(HOTPLUG_DEBOUNCE_MS));
+
+	return IRQ_HANDLED;
+}
+
+#define DATA_LANES_COUNT	4
+static int cdns_mhdp8501_dt_parse(struct cdns_mhdp8501_device *mhdp,
+				  struct platform_device *pdev)
+{
+	struct device *dev = &pdev->dev;
+	struct device_node *np = dev->of_node;
+	struct device_node *remote, *endpoint;
+	u32 data_lanes[DATA_LANES_COUNT];
+	u32 lane_value;
+	int ret, i;
+
+	remote = of_graph_get_remote_node(np, 1, 0);
+	if (!remote) {
+		dev_err(dev, "fail to get remote node\n");
+		of_node_put(remote);
+		return -EINVAL;
+	}
+
+	/* get connector type */
+	if (of_device_is_compatible(remote, "hdmi-connector")) {
+		mhdp->connector_type = DRM_MODE_CONNECTOR_HDMIA;
+
+	} else if (of_device_is_compatible(remote, "dp-connector")) {
+		mhdp->connector_type = DRM_MODE_CONNECTOR_DisplayPort;
+
+	} else {
+		dev_err(dev, "Unknown connector type\n");
+		of_node_put(remote);
+		return -EINVAL;
+	}
+
+	of_node_put(remote);
+
+	endpoint = of_graph_get_endpoint_by_regs(np, 1, -1);
+
+	/* Get the data lanes ordering */
+	ret = of_property_count_u32_elems(endpoint, "data-lanes");
+	if (ret < 0)
+		return  -EINVAL;
+	if (ret != DATA_LANES_COUNT) {
+		dev_err(dev, "expected 4 data lanes\n");
+		return  -EINVAL;
+	}
+
+	ret = of_property_read_u32_array(endpoint, "data-lanes",
+					 data_lanes, DATA_LANES_COUNT);
+	if (ret)
+		return  -EINVAL;
+
+	mhdp->lane_mapping  = 0;
+	for (i = 0; i < DATA_LANES_COUNT; i++) {
+		lane_value = (data_lanes[i] >= 0 && data_lanes[i] <= 3) ? data_lanes[i] : 0;
+		mhdp->lane_mapping |= lane_value << (i * 2);
+	}
+
+	return true;
+}
+
+static int cdns_mhdp8501_add_bridge(struct cdns_mhdp8501_device *mhdp)
+{
+	mhdp->bridge.type = mhdp->connector_type;
+	mhdp->bridge.driver_private = mhdp;
+	mhdp->bridge.of_node = mhdp->dev->of_node;
+	mhdp->bridge.vendor = "NXP";
+	mhdp->bridge.product = "i.MX8";
+	mhdp->bridge.ops = DRM_BRIDGE_OP_DETECT | DRM_BRIDGE_OP_EDID |
+			   DRM_BRIDGE_OP_HPD;
+
+	if (mhdp->connector_type == DRM_MODE_CONNECTOR_HDMIA) {
+		mhdp->bridge.funcs = &cdns_hdmi_bridge_funcs;
+		mhdp->bridge.ops |= DRM_BRIDGE_OP_HDMI;
+		mhdp->bridge.ddc = cdns_hdmi_i2c_adapter(mhdp);
+	} else if (mhdp->connector_type == DRM_MODE_CONNECTOR_DisplayPort) {
+		mhdp->bridge.funcs = &cdns_dp_bridge_funcs;
+	} else {
+		dev_err(mhdp->dev, "Unsupported connector type!\n");
+		return -EINVAL;
+	}
+
+	drm_bridge_add(&mhdp->bridge);
+
+	return 0;
+}
+
+static int cdns_mhdp8501_probe(struct platform_device *pdev)
+{
+	struct device *dev = &pdev->dev;
+	struct cdns_mhdp8501_device *mhdp;
+	struct resource *res;
+	enum phy_mode phy_mode;
+	u32 reg;
+	int ret;
+
+	mhdp = devm_kzalloc(dev, sizeof(*mhdp), GFP_KERNEL);
+	if (!mhdp)
+		return -ENOMEM;
+
+	mhdp->dev = dev;
+
+	INIT_DELAYED_WORK(&mhdp->hotplug_work, hotplug_work_func);
+
+	res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+	if (!res)
+		return -ENODEV;
+
+	mhdp->regs = devm_ioremap(dev, res->start, resource_size(res));
+	if (IS_ERR(mhdp->regs))
+		return PTR_ERR(mhdp->regs);
+
+	cdns_mhdp8501_create_device_files(mhdp);
+
+	ret = cdns_mhdp8501_dt_parse(mhdp, pdev);
+	if (ret < 0)
+		return -EINVAL;
+
+	mhdp->phy = devm_of_phy_get_by_index(dev, pdev->dev.of_node, 0);
+	if (IS_ERR(mhdp->phy))
+		return dev_err_probe(dev, PTR_ERR(mhdp->phy), "no PHY configured\n");
+
+	mhdp->irq[IRQ_IN] = platform_get_irq_byname(pdev, "plug_in");
+	if (mhdp->irq[IRQ_IN] < 0)
+		return dev_err_probe(dev, mhdp->irq[IRQ_IN], "No plug_in irq number\n");
+
+	mhdp->irq[IRQ_OUT] = platform_get_irq_byname(pdev, "plug_out");
+	if (mhdp->irq[IRQ_OUT] < 0)
+		return dev_err_probe(dev, mhdp->irq[IRQ_OUT], "No plug_out irq number\n");
+
+	irq_set_status_flags(mhdp->irq[IRQ_IN], IRQ_NOAUTOEN);
+	ret = devm_request_threaded_irq(dev, mhdp->irq[IRQ_IN],
+					NULL, cdns_mhdp8501_irq_thread,
+					IRQF_ONESHOT, dev_name(dev), mhdp);
+	if (ret < 0) {
+		dev_err(dev, "can't claim irq %d\n", mhdp->irq[IRQ_IN]);
+		return -EINVAL;
+	}
+
+	irq_set_status_flags(mhdp->irq[IRQ_OUT], IRQ_NOAUTOEN);
+	ret = devm_request_threaded_irq(dev, mhdp->irq[IRQ_OUT],
+					NULL, cdns_mhdp8501_irq_thread,
+					IRQF_ONESHOT, dev_name(dev), mhdp);
+	if (ret < 0) {
+		dev_err(dev, "can't claim irq %d\n", mhdp->irq[IRQ_OUT]);
+		return -EINVAL;
+	}
+
+	/* cdns_mhdp8501_dt_parse() ensures connector_type is valid */
+	if (mhdp->connector_type == DRM_MODE_CONNECTOR_DisplayPort)
+		phy_mode = PHY_MODE_DP;
+	else if (mhdp->connector_type == DRM_MODE_CONNECTOR_HDMIA)
+		phy_mode = PHY_MODE_HDMI;
+
+	dev_set_drvdata(dev, mhdp);
+
+	/* init base struct for access mhdp mailbox */
+	mhdp->base.dev = mhdp->dev;
+	mhdp->base.regs = mhdp->regs;
+
+	if (mhdp->connector_type == DRM_MODE_CONNECTOR_DisplayPort) {
+		drm_dp_aux_init(&mhdp->dp.aux);
+		mhdp->dp.aux.name = "mhdp8501_dp_aux";
+		mhdp->dp.aux.dev = dev;
+		mhdp->dp.aux.transfer = cdns_dp_aux_transfer;
+	}
+
+	/* Enable APB clock */
+	mhdp->apb_clk = devm_clk_get_enabled(dev, NULL);
+	if (IS_ERR(mhdp->apb_clk))
+		return dev_err_probe(dev, PTR_ERR(mhdp->apb_clk),
+				     "couldn't get apb clk\n");
+	/*
+	 * Wait for the KEEP_ALIVE "message" on the first 8 bits.
+	 * Updated each sched "tick" (~2ms)
+	 */
+	ret = readl_poll_timeout(mhdp->regs + KEEP_ALIVE, reg,
+				 reg & CDNS_KEEP_ALIVE_MASK, 500,
+				 CDNS_KEEP_ALIVE_TIMEOUT);
+	if (ret) {
+		dev_err(dev, "device didn't give any life sign: reg %d\n", reg);
+		return ret;
+	}
+
+	ret = phy_init(mhdp->phy);
+	if (ret) {
+		dev_err(dev, "Failed to initialize PHY: %d\n", ret);
+		return ret;
+	}
+
+	ret = phy_set_mode(mhdp->phy, phy_mode);
+	if (ret) {
+		dev_err(dev, "Failed to configure PHY: %d\n", ret);
+		return ret;
+	}
+
+	/* Enable cable hotplug detect */
+	if (cdns_mhdp8501_read_hpd(mhdp))
+		enable_irq(mhdp->irq[IRQ_OUT]);
+	else
+		enable_irq(mhdp->irq[IRQ_IN]);
+
+	return cdns_mhdp8501_add_bridge(mhdp);
+}
+
+static void cdns_mhdp8501_remove(struct platform_device *pdev)
+{
+	struct cdns_mhdp8501_device *mhdp = platform_get_drvdata(pdev);
+
+	cdns_mhdp8501_remove_device_files(mhdp);
+
+	if (mhdp->connector_type == DRM_MODE_CONNECTOR_DisplayPort)
+		cdns_dp_aux_destroy(mhdp);
+
+	drm_bridge_remove(&mhdp->bridge);
+}
+
+static const struct of_device_id cdns_mhdp8501_dt_ids[] = {
+	{ .compatible = "fsl,imx8mq-mhdp8501",
+	},
+	{ },
+};
+MODULE_DEVICE_TABLE(of, cdns_mhdp8501_dt_ids);
+
+static struct platform_driver cdns_mhdp8501_driver = {
+	.probe = cdns_mhdp8501_probe,
+	.remove = cdns_mhdp8501_remove,
+	.driver = {
+		.name = "cdns-mhdp8501",
+		.of_match_table = cdns_mhdp8501_dt_ids,
+	},
+};
+
+module_platform_driver(cdns_mhdp8501_driver);
+
+MODULE_AUTHOR("Sandor Yu <sandor.yu@nxp.com>");
+MODULE_DESCRIPTION("Cadence MHDP8501 bridge driver");
+MODULE_LICENSE("GPL");
diff --git a/drivers/gpu/drm/bridge/cadence/cdns-mhdp8501-core.h b/drivers/gpu/drm/bridge/cadence/cdns-mhdp8501-core.h
new file mode 100644
index 0000000000000..8fc463098ab84
--- /dev/null
+++ b/drivers/gpu/drm/bridge/cadence/cdns-mhdp8501-core.h
@@ -0,0 +1,380 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Cadence MHDP 8501 Common head file
+ *
+ * Copyright (C) 2019-2024 NXP Semiconductor, Inc.
+ *
+ */
+
+#ifndef _CDNS_MHDP8501_CORE_H_
+#define _CDNS_MHDP8501_CORE_H_
+
+#include <drm/drm_bridge.h>
+#include <drm/drm_connector.h>
+#include <drm/display/drm_dp_helper.h>
+#include <linux/bitops.h>
+#include <linux/i2c.h>
+#include <soc/cadence/cdns-mhdp-helper.h>
+
+#define ADDR_IMEM			0x10000
+#define ADDR_DMEM			0x20000
+
+/* APB CFG addr */
+#define APB_CTRL			0
+#define XT_INT_CTRL			0x04
+#define MAILBOX_FULL_ADDR		0x08
+#define MAILBOX_EMPTY_ADDR		0x0c
+#define MAILBOX0_WR_DATA		0x10
+#define MAILBOX0_RD_DATA		0x14
+#define KEEP_ALIVE			0x18
+#define VER_L				0x1c
+#define VER_H				0x20
+#define VER_LIB_L_ADDR			0x24
+#define VER_LIB_H_ADDR			0x28
+#define SW_DEBUG_L			0x2c
+#define SW_DEBUG_H			0x30
+#define MAILBOX_INT_MASK		0x34
+#define MAILBOX_INT_STATUS		0x38
+#define SW_CLK_L			0x3c
+#define SW_CLK_H			0x40
+#define SW_EVENTS0			0x44
+#define SW_EVENTS1			0x48
+#define SW_EVENTS2			0x4c
+#define SW_EVENTS3			0x50
+#define XT_OCD_CTRL			0x60
+#define APB_INT_MASK			0x6c
+#define APB_STATUS_MASK			0x70
+
+/* Source phy comp */
+#define PHY_DATA_SEL			0x0818
+#define LANES_CONFIG			0x0814
+
+/* Source CAR Addr */
+#define SOURCE_HDTX_CAR			0x0900
+#define SOURCE_DPTX_CAR			0x0904
+#define SOURCE_PHY_CAR			0x0908
+#define SOURCE_CEC_CAR			0x090c
+#define SOURCE_CBUS_CAR			0x0910
+#define SOURCE_PKT_CAR			0x0918
+#define SOURCE_AIF_CAR			0x091c
+#define SOURCE_CIPHER_CAR		0x0920
+#define SOURCE_CRYPTO_CAR		0x0924
+
+/* clock meters addr */
+#define CM_CTRL				0x0a00
+#define CM_I2S_CTRL			0x0a04
+#define CM_SPDIF_CTRL			0x0a08
+#define CM_VID_CTRL			0x0a0c
+#define CM_LANE_CTRL			0x0a10
+#define I2S_NM_STABLE			0x0a14
+#define I2S_NCTS_STABLE			0x0a18
+#define SPDIF_NM_STABLE			0x0a1c
+#define SPDIF_NCTS_STABLE		0x0a20
+#define NMVID_MEAS_STABLE		0x0a24
+#define I2S_MEAS			0x0a40
+#define SPDIF_MEAS			0x0a80
+#define NMVID_MEAS			0x0ac0
+
+/* source vif addr */
+#define BND_HSYNC2VSYNC			0x0b00
+#define HSYNC2VSYNC_F1_L1		0x0b04
+#define HSYNC2VSYNC_STATUS		0x0b0c
+#define HSYNC2VSYNC_POL_CTRL		0x0b10
+
+/* MHDP TX_top_comp */
+#define SCHEDULER_H_SIZE		0x1000
+#define SCHEDULER_V_SIZE		0x1004
+#define HDTX_SIGNAL_FRONT_WIDTH		0x100c
+#define HDTX_SIGNAL_SYNC_WIDTH		0x1010
+#define HDTX_SIGNAL_BACK_WIDTH		0x1014
+#define HDTX_CONTROLLER			0x1018
+#define HDTX_HPD			0x1020
+#define HDTX_CLOCK_REG_0		0x1024
+#define HDTX_CLOCK_REG_1		0x1028
+
+/* DPTX hpd addr */
+#define HPD_IRQ_DET_MIN_TIMER		0x2100
+#define HPD_IRQ_DET_MAX_TIMER		0x2104
+#define HPD_UNPLGED_DET_MIN_TIMER	0x2108
+#define HPD_STABLE_TIMER		0x210c
+#define HPD_FILTER_TIMER		0x2110
+#define HPD_EVENT_MASK			0x211c
+#define HPD_EVENT_DET			0x2120
+
+/* DPTX framer addr */
+#define DP_FRAMER_GLOBAL_CONFIG		0x2200
+#define DP_SW_RESET			0x2204
+#define DP_FRAMER_TU			0x2208
+#define DP_FRAMER_PXL_REPR		0x220c
+#define DP_FRAMER_SP			0x2210
+#define AUDIO_PACK_CONTROL		0x2214
+#define DP_VC_TABLE(x)			(0x2218 + ((x) << 2))
+#define DP_VB_ID			0x2258
+#define DP_MTPH_LVP_CONTROL		0x225c
+#define DP_MTPH_SYMBOL_VALUES		0x2260
+#define DP_MTPH_ECF_CONTROL		0x2264
+#define DP_MTPH_ACT_CONTROL		0x2268
+#define DP_MTPH_STATUS			0x226c
+#define DP_INTERRUPT_SOURCE		0x2270
+#define DP_INTERRUPT_MASK		0x2274
+#define DP_FRONT_BACK_PORCH		0x2278
+#define DP_BYTE_COUNT			0x227c
+
+/* DPTX stream addr */
+#define MSA_HORIZONTAL_0		0x2280
+#define MSA_HORIZONTAL_1		0x2284
+#define MSA_VERTICAL_0			0x2288
+#define MSA_VERTICAL_1			0x228c
+#define MSA_MISC			0x2290
+#define STREAM_CONFIG			0x2294
+#define AUDIO_PACK_STATUS		0x2298
+#define VIF_STATUS			0x229c
+#define PCK_STUFF_STATUS_0		0x22a0
+#define PCK_STUFF_STATUS_1		0x22a4
+#define INFO_PACK_STATUS		0x22a8
+#define RATE_GOVERNOR_STATUS		0x22ac
+#define DP_HORIZONTAL			0x22b0
+#define DP_VERTICAL_0			0x22b4
+#define DP_VERTICAL_1			0x22b8
+#define DP_BLOCK_SDP			0x22bc
+
+/* DPTX glbl addr */
+#define DPTX_LANE_EN			0x2300
+#define DPTX_ENHNCD			0x2304
+#define DPTX_INT_MASK			0x2308
+#define DPTX_INT_STATUS			0x230c
+
+/* DP AUX Addr */
+#define DP_AUX_HOST_CONTROL		0x2800
+#define DP_AUX_INTERRUPT_SOURCE		0x2804
+#define DP_AUX_INTERRUPT_MASK		0x2808
+#define DP_AUX_SWAP_INVERSION_CONTROL	0x280c
+#define DP_AUX_SEND_NACK_TRANSACTION	0x2810
+#define DP_AUX_CLEAR_RX			0x2814
+#define DP_AUX_CLEAR_TX			0x2818
+#define DP_AUX_TIMER_STOP		0x281c
+#define DP_AUX_TIMER_CLEAR		0x2820
+#define DP_AUX_RESET_SW			0x2824
+#define DP_AUX_DIVIDE_2M		0x2828
+#define DP_AUX_TX_PREACHARGE_LENGTH	0x282c
+#define DP_AUX_FREQUENCY_1M_MAX		0x2830
+#define DP_AUX_FREQUENCY_1M_MIN		0x2834
+#define DP_AUX_RX_PRE_MIN		0x2838
+#define DP_AUX_RX_PRE_MAX		0x283c
+#define DP_AUX_TIMER_PRESET		0x2840
+#define DP_AUX_NACK_FORMAT		0x2844
+#define DP_AUX_TX_DATA			0x2848
+#define DP_AUX_RX_DATA			0x284c
+#define DP_AUX_TX_STATUS		0x2850
+#define DP_AUX_RX_STATUS		0x2854
+#define DP_AUX_RX_CYCLE_COUNTER		0x2858
+#define DP_AUX_MAIN_STATES		0x285c
+#define DP_AUX_MAIN_TIMER		0x2860
+#define DP_AUX_AFE_OUT			0x2864
+
+/* source pif addr */
+#define SOURCE_PIF_WR_ADDR		0x30800
+#define SOURCE_PIF_WR_REQ		0x30804
+#define SOURCE_PIF_RD_ADDR		0x30808
+#define SOURCE_PIF_RD_REQ		0x3080c
+#define SOURCE_PIF_DATA_WR		0x30810
+#define SOURCE_PIF_DATA_RD		0x30814
+#define SOURCE_PIF_FIFO1_FLUSH		0x30818
+#define SOURCE_PIF_FIFO2_FLUSH		0x3081c
+#define SOURCE_PIF_STATUS		0x30820
+#define SOURCE_PIF_INTERRUPT_SOURCE	0x30824
+#define SOURCE_PIF_INTERRUPT_MASK	0x30828
+#define SOURCE_PIF_PKT_ALLOC_REG	0x3082c
+#define SOURCE_PIF_PKT_ALLOC_WR_EN	0x30830
+#define SOURCE_PIF_SW_RESET		0x30834
+
+#define LINK_TRAINING_NOT_ACTIV		0
+#define LINK_TRAINING_RUN		1
+#define LINK_TRAINING_RESTART		2
+
+#define CONTROL_VIDEO_IDLE		0
+#define CONTROL_VIDEO_VALID		1
+
+#define INTERLACE_FMT_DET		BIT(12)
+#define VIF_BYPASS_INTERLACE		BIT(13)
+#define TU_CNT_RST_EN			BIT(15)
+#define INTERLACE_DTCT_WIN		0x20
+
+#define DP_FRAMER_SP_INTERLACE_EN	BIT(2)
+#define DP_FRAMER_SP_HSP		BIT(1)
+#define DP_FRAMER_SP_VSP		BIT(0)
+
+/* Capability */
+#define AUX_HOST_INVERT			3
+#define FAST_LT_SUPPORT			1
+#define FAST_LT_NOT_SUPPORT		0
+#define LANE_MAPPING_FLIPPED		0xe4
+#define ENHANCED			1
+#define SCRAMBLER_EN			BIT(4)
+
+#define FULL_LT_STARTED			BIT(0)
+#define FASE_LT_STARTED			BIT(1)
+#define CLK_RECOVERY_FINISHED		BIT(2)
+#define EQ_PHASE_FINISHED		BIT(3)
+#define FASE_LT_START_FINISHED		BIT(4)
+#define CLK_RECOVERY_FAILED		BIT(5)
+#define EQ_PHASE_FAILED			BIT(6)
+#define FASE_LT_FAILED			BIT(7)
+
+#define TU_SIZE				30
+#define CDNS_DP_MAX_LINK_RATE		540000
+
+#define F_HDMI2_CTRL_IL_MODE(x)		(((x) & ((1 << 1) - 1)) << 19)
+#define F_HDMI2_PREAMBLE_EN(x)		(((x) & ((1 << 1) - 1)) << 18)
+#define F_HDMI_ENCODING(x)		(((x) & ((1 << 2) - 1)) << 16)
+#define F_DATA_EN(x)			(((x) & ((1 << 1) - 1)) << 15)
+#define F_CLEAR_AVMUTE(x)		(((x) & ((1 << 1) - 1)) << 14)
+#define F_SET_AVMUTE(x)			(((x) & ((1 << 1) - 1)) << 13)
+#define F_GCP_EN(x)			(((x) & ((1 << 1) - 1)) << 12)
+#define F_BCH_EN(x)			(((x) & ((1 << 1) - 1)) << 11)
+#define F_PIC_3D(x)			(((x) & ((1 << 4) - 1)) << 7)
+#define F_VIF_DATA_WIDTH(x)		(((x) & ((1 << 2) - 1)) << 2)
+#define F_HDMI_MODE(x)			(((x) & ((1 << 2) - 1)) << 0)
+
+#define F_SOURCE_PHY_MHDP_SEL(x)	(((x) & ((1 << 2) - 1)) << 3)
+
+#define F_HPD_GLITCH_WIDTH(x)		(((x) & ((1 << 8) - 1)) << 12)
+#define F_PACKET_TYPE(x)		(((x) & ((1 << 8) - 1)) << 8)
+#define F_HPD_VALID_WIDTH(x)		(((x) & ((1 << 12) - 1)) << 0)
+
+#define F_SOURCE_PHY_LANE3_SWAP(x)	(((x) & ((1 << 2) - 1)) << 6)
+#define F_SOURCE_PHY_LANE2_SWAP(x)	(((x) & ((1 << 2) - 1)) << 4)
+#define F_SOURCE_PHY_LANE1_SWAP(x)	(((x) & ((1 << 2) - 1)) << 2)
+#define F_SOURCE_PHY_LANE0_SWAP(x)	(((x) & ((1 << 2) - 1)) << 0)
+
+#define F_ACTIVE_IDLE_TYPE(x)		(((x) & ((1 << 1) - 1)) << 17)
+#define F_TYPE_VALID(x)			(((x) & ((1 << 1) - 1)) << 16)
+#define F_PKT_ALLOC_ADDRESS(x)		(((x) & ((1 << 4) - 1)) << 0)
+
+#define F_FIFO1_FLUSH(x)		(((x) & ((1 << 1) - 1)) << 0)
+#define F_PKT_ALLOC_WR_EN(x)		(((x) & ((1 << 1) - 1)) << 0)
+#define F_DATA_WR(x)			(x)
+#define F_WR_ADDR(x)			(((x) & ((1 << 4) - 1)) << 0)
+#define F_HOST_WR(x)			(((x) & ((1 << 1) - 1)) << 0)
+
+/* Reference cycles when using lane clock as reference */
+#define LANE_REF_CYC			0x8000
+
+/* HPD Debounce */
+#define HOTPLUG_DEBOUNCE_MS		200
+
+/* HPD IRQ Index */
+#define IRQ_IN    0
+#define IRQ_OUT   1
+#define IRQ_NUM   2
+
+/* FW check alive timeout */
+#define CDNS_KEEP_ALIVE_TIMEOUT		2000
+#define CDNS_KEEP_ALIVE_MASK		GENMASK(7, 0)
+
+enum voltage_swing_level {
+	VOLTAGE_LEVEL_0,
+	VOLTAGE_LEVEL_1,
+	VOLTAGE_LEVEL_2,
+	VOLTAGE_LEVEL_3,
+};
+
+enum pre_emphasis_level {
+	PRE_EMPHASIS_LEVEL_0,
+	PRE_EMPHASIS_LEVEL_1,
+	PRE_EMPHASIS_LEVEL_2,
+	PRE_EMPHASIS_LEVEL_3,
+};
+
+enum pattern_set {
+	PTS1 = BIT(0),
+	PTS2 = BIT(1),
+	PTS3 = BIT(2),
+	PTS4 = BIT(3),
+	DP_NONE	= BIT(4)
+};
+
+enum vic_color_depth {
+	BCS_6 = 0x1,
+	BCS_8 = 0x2,
+	BCS_10 = 0x4,
+	BCS_12 = 0x8,
+	BCS_16 = 0x10,
+};
+
+enum vic_bt_type {
+	BT_601 = 0x0,
+	BT_709 = 0x1,
+};
+
+enum {
+	MODE_DVI,
+	MODE_HDMI_1_4,
+	MODE_HDMI_2_0,
+};
+
+struct video_info {
+	int bpc;
+	int color_fmt;
+};
+
+struct cdns_hdmi_i2c {
+	struct i2c_adapter	adap;
+
+	struct mutex		lock;	/* used to serialize data transfers */
+	struct completion	cmp;
+	u8			stat;
+
+	u8			slave_reg;
+	bool			is_regaddr;
+	bool			is_segment;
+};
+
+struct cdns_mhdp8501_device {
+	struct cdns_mhdp_base base;
+
+	struct device *dev;
+	void __iomem *regs;
+	struct drm_connector *curr_conn;
+	struct drm_bridge bridge;
+	struct clk *apb_clk;
+	struct phy *phy;
+
+	struct video_info video_info;
+
+	int irq[IRQ_NUM];
+	struct delayed_work hotplug_work;
+	int connector_type;
+	u32 lane_mapping;
+
+	union {
+		struct _dp_data {
+			u32 rate;
+			u8 num_lanes;
+			struct drm_dp_aux aux;
+			u8 dpcd[DP_RECEIVER_CAP_SIZE];
+		} dp;
+		struct _hdmi_data {
+			u32 hdmi_type;
+			struct cdns_hdmi_i2c *i2c;
+		} hdmi;
+	};
+};
+
+extern const struct drm_bridge_funcs cdns_dp_bridge_funcs;
+extern const struct drm_bridge_funcs cdns_hdmi_bridge_funcs;
+
+enum drm_connector_status
+cdns_mhdp8501_detect(struct drm_bridge *bridge);
+enum drm_mode_status
+cdns_mhdp8501_mode_valid(struct drm_bridge *bridge,
+			 const struct drm_display_info *info,
+			 const struct drm_display_mode *mode);
+
+ssize_t cdns_dp_aux_transfer(struct drm_dp_aux *aux, struct drm_dp_aux_msg *msg);
+int cdns_dp_aux_destroy(struct cdns_mhdp8501_device *mhdp);
+void cdns_dp_check_link_state(struct cdns_mhdp8501_device *mhdp);
+
+void cdns_hdmi_handle_hotplug(struct cdns_mhdp8501_device *mhdp);
+struct i2c_adapter *cdns_hdmi_i2c_adapter(struct cdns_mhdp8501_device *mhdp);
+#endif
diff --git a/drivers/gpu/drm/bridge/cadence/cdns-mhdp8501-dp.c b/drivers/gpu/drm/bridge/cadence/cdns-mhdp8501-dp.c
new file mode 100644
index 0000000000000..157b4d44b9e2b
--- /dev/null
+++ b/drivers/gpu/drm/bridge/cadence/cdns-mhdp8501-dp.c
@@ -0,0 +1,694 @@
+// SPDX-License-Identifier: GPL-2.0-only
+/*
+ * Cadence MHDP8501 DisplayPort(DP) bridge driver
+ *
+ * Copyright (C) 2019-2024 NXP Semiconductor, Inc.
+ *
+ */
+#include <drm/drm_atomic_helper.h>
+#include <drm/drm_edid.h>
+#include <drm/drm_print.h>
+#include <linux/media-bus-format.h>
+#include <linux/phy/phy.h>
+#include <linux/phy/phy-dp.h>
+
+#include "cdns-mhdp8501-core.h"
+
+#define LINK_TRAINING_TIMEOUT_MS	500
+#define LINK_TRAINING_RETRY_MS		20
+
+ssize_t cdns_dp_aux_transfer(struct drm_dp_aux *aux,
+			     struct drm_dp_aux_msg *msg)
+{
+	struct cdns_mhdp8501_device *mhdp = dev_get_drvdata(aux->dev);
+	bool native = msg->request & (DP_AUX_NATIVE_WRITE & DP_AUX_NATIVE_READ);
+	int ret;
+
+	/* Ignore address only message */
+	if (!msg->size || !msg->buffer) {
+		msg->reply = native ?
+			DP_AUX_NATIVE_REPLY_ACK : DP_AUX_I2C_REPLY_ACK;
+		return msg->size;
+	}
+
+	if (!native) {
+		dev_err(mhdp->dev, "%s: only native messages supported\n", __func__);
+		return -EINVAL;
+	}
+
+	/* msg sanity check */
+	if (msg->size > DP_AUX_MAX_PAYLOAD_BYTES) {
+		dev_err(mhdp->dev, "%s: invalid msg: size(%zu), request(%x)\n",
+			__func__, msg->size, (unsigned int)msg->request);
+		return -EINVAL;
+	}
+
+	if (msg->request == DP_AUX_NATIVE_WRITE) {
+		const u8 *buf = msg->buffer;
+		int i;
+
+		for (i = 0; i < msg->size; ++i) {
+			ret = cdns_mhdp_dpcd_write(&mhdp->base,
+						   msg->address + i, buf[i]);
+			if (ret < 0) {
+				dev_err(mhdp->dev, "Failed to write DPCD\n");
+				return ret;
+			}
+		}
+		msg->reply = DP_AUX_NATIVE_REPLY_ACK;
+		return msg->size;
+	}
+
+	if (msg->request == DP_AUX_NATIVE_READ) {
+		ret = cdns_mhdp_dpcd_read(&mhdp->base, msg->address,
+					  msg->buffer, msg->size);
+		if (ret < 0)
+			return ret;
+		msg->reply = DP_AUX_NATIVE_REPLY_ACK;
+		return msg->size;
+	}
+	return 0;
+}
+
+int cdns_dp_aux_destroy(struct cdns_mhdp8501_device *mhdp)
+{
+	drm_dp_aux_unregister(&mhdp->dp.aux);
+
+	return 0;
+}
+
+static int cdns_dp_get_msa_misc(struct video_info *video)
+{
+	u32 msa_misc;
+	u8 color_space = 0;
+	u8 bpc = 0;
+
+	switch (video->color_fmt) {
+	/* set YUV default color space conversion to BT601 */
+	case DRM_COLOR_FORMAT_YCBCR444:
+		color_space = 6 + BT_601 * 8;
+		break;
+	case DRM_COLOR_FORMAT_YCBCR422:
+		color_space = 5 + BT_601 * 8;
+		break;
+	case DRM_COLOR_FORMAT_YCBCR420:
+		color_space = 5;
+		break;
+	case DRM_COLOR_FORMAT_RGB444:
+	default:
+		color_space = 0;
+		break;
+	};
+
+	switch (video->bpc) {
+	case 6:
+		bpc = 0;
+		break;
+	case 10:
+		bpc = 2;
+		break;
+	case 12:
+		bpc = 3;
+		break;
+	case 16:
+		bpc = 4;
+		break;
+	case 8:
+	default:
+		bpc = 1;
+		break;
+	};
+
+	msa_misc = (bpc << 5) | (color_space << 1);
+
+	return msa_misc;
+}
+
+static int cdns_dp_config_video(struct cdns_mhdp8501_device *mhdp,
+				const struct drm_display_mode *mode)
+{
+	struct video_info *video = &mhdp->video_info;
+	bool h_sync_polarity, v_sync_polarity;
+	u64 symbol;
+	u32 val, link_rate, rem;
+	u8 bit_per_pix, tu_size_reg = TU_SIZE;
+	int ret;
+
+	bit_per_pix = (video->color_fmt == DRM_COLOR_FORMAT_YCBCR422) ?
+		      (video->bpc * 2) : (video->bpc * 3);
+
+	link_rate = mhdp->dp.rate / 1000;
+
+	ret = cdns_mhdp_reg_write(&mhdp->base, BND_HSYNC2VSYNC, VIF_BYPASS_INTERLACE);
+	if (ret)
+		goto err_config_video;
+
+	ret = cdns_mhdp_reg_write(&mhdp->base, HSYNC2VSYNC_POL_CTRL, 0);
+	if (ret)
+		goto err_config_video;
+
+	/*
+	 * get a best tu_size and valid symbol:
+	 * 1. chose Lclk freq(162Mhz, 270Mhz, 540Mhz), set TU to 32
+	 * 2. calculate VS(valid symbol) = TU * Pclk * Bpp / (Lclk * Lanes)
+	 * 3. if VS > *.85 or VS < *.1 or VS < 2 or TU < VS + 4, then set
+	 *    TU += 2 and repeat 2nd step.
+	 */
+	do {
+		tu_size_reg += 2;
+		symbol = tu_size_reg * mode->clock * bit_per_pix;
+		do_div(symbol, mhdp->dp.num_lanes * link_rate * 8);
+		rem = do_div(symbol, 1000);
+		if (tu_size_reg > 64) {
+			ret = -EINVAL;
+			dev_err(mhdp->dev, "tu error, clk:%d, lanes:%d, rate:%d\n",
+				mode->clock, mhdp->dp.num_lanes, link_rate);
+			goto err_config_video;
+		}
+	} while ((symbol <= 1) || (tu_size_reg - symbol < 4) ||
+		 (rem > 850) || (rem < 100));
+
+	val = symbol + (tu_size_reg << 8);
+	val |= TU_CNT_RST_EN;
+	ret = cdns_mhdp_reg_write(&mhdp->base, DP_FRAMER_TU, val);
+	if (ret)
+		goto err_config_video;
+
+	/* set the FIFO Buffer size */
+	val = div_u64(mode->clock * (symbol + 1), 1000) + link_rate;
+	val /= (mhdp->dp.num_lanes * link_rate);
+	val = div_u64(8 * (symbol + 1), bit_per_pix) - val;
+	val += 2;
+	ret = cdns_mhdp_reg_write(&mhdp->base, DP_VC_TABLE(15), val);
+
+	switch (video->bpc) {
+	case 6:
+		val = BCS_6;
+		break;
+	case 10:
+		val = BCS_10;
+		break;
+	case 12:
+		val = BCS_12;
+		break;
+	case 16:
+		val = BCS_16;
+		break;
+	case 8:
+	default:
+		val = BCS_8;
+		break;
+	};
+
+	val += video->color_fmt << 8;
+	ret = cdns_mhdp_reg_write(&mhdp->base, DP_FRAMER_PXL_REPR, val);
+	if (ret)
+		goto err_config_video;
+
+	v_sync_polarity = !!(mode->flags & DRM_MODE_FLAG_NVSYNC);
+	h_sync_polarity = !!(mode->flags & DRM_MODE_FLAG_NHSYNC);
+
+	val = h_sync_polarity ? DP_FRAMER_SP_HSP : 0;
+	val |= v_sync_polarity ? DP_FRAMER_SP_VSP : 0;
+	ret = cdns_mhdp_reg_write(&mhdp->base, DP_FRAMER_SP, val);
+	if (ret)
+		goto err_config_video;
+
+	val = (mode->hsync_start - mode->hdisplay) << 16;
+	val |= mode->htotal - mode->hsync_end;
+	ret = cdns_mhdp_reg_write(&mhdp->base, DP_FRONT_BACK_PORCH, val);
+	if (ret)
+		goto err_config_video;
+
+	val = mode->hdisplay * bit_per_pix / 8;
+	ret = cdns_mhdp_reg_write(&mhdp->base, DP_BYTE_COUNT, val);
+	if (ret)
+		goto err_config_video;
+
+	val = mode->htotal | ((mode->htotal - mode->hsync_start) << 16);
+	ret = cdns_mhdp_reg_write(&mhdp->base, MSA_HORIZONTAL_0, val);
+	if (ret)
+		goto err_config_video;
+
+	val = mode->hsync_end - mode->hsync_start;
+	val |= (mode->hdisplay << 16) | (h_sync_polarity << 15);
+	ret = cdns_mhdp_reg_write(&mhdp->base, MSA_HORIZONTAL_1, val);
+	if (ret)
+		goto err_config_video;
+
+	val = mode->vtotal;
+	val |= (mode->vtotal - mode->vsync_start) << 16;
+	ret = cdns_mhdp_reg_write(&mhdp->base, MSA_VERTICAL_0, val);
+	if (ret)
+		goto err_config_video;
+
+	val = mode->vsync_end - mode->vsync_start;
+	val |= (mode->vdisplay << 16) | (v_sync_polarity << 15);
+	ret = cdns_mhdp_reg_write(&mhdp->base, MSA_VERTICAL_1, val);
+	if (ret)
+		goto err_config_video;
+
+	val = cdns_dp_get_msa_misc(video);
+	ret = cdns_mhdp_reg_write(&mhdp->base, MSA_MISC, val);
+	if (ret)
+		goto err_config_video;
+
+	ret = cdns_mhdp_reg_write(&mhdp->base, STREAM_CONFIG, 1);
+	if (ret)
+		goto err_config_video;
+
+	val = mode->hsync_end - mode->hsync_start;
+	val |= mode->hdisplay << 16;
+	ret = cdns_mhdp_reg_write(&mhdp->base, DP_HORIZONTAL, val);
+	if (ret)
+		goto err_config_video;
+
+	val = mode->vdisplay;
+	val |= (mode->vtotal - mode->vsync_start) << 16;
+	ret = cdns_mhdp_reg_write(&mhdp->base, DP_VERTICAL_0, val);
+	if (ret)
+		goto err_config_video;
+
+	val = mode->vtotal;
+	ret = cdns_mhdp_reg_write(&mhdp->base, DP_VERTICAL_1, val);
+	if (ret)
+		goto err_config_video;
+
+	ret = cdns_mhdp_dp_reg_write_bit(&mhdp->base, DP_VB_ID, 2, 1, 0);
+
+err_config_video:
+	if (ret)
+		dev_err(mhdp->dev, "config video failed: %d\n", ret);
+	return ret;
+}
+
+static void cdns_dp_pixel_clk_reset(struct cdns_mhdp8501_device *mhdp)
+{
+	u32 val;
+
+	/* reset pixel clk */
+	cdns_mhdp_reg_read(&mhdp->base, SOURCE_HDTX_CAR, &val);
+	cdns_mhdp_reg_write(&mhdp->base, SOURCE_HDTX_CAR, val & 0xFD);
+	cdns_mhdp_reg_write(&mhdp->base, SOURCE_HDTX_CAR, val);
+}
+
+static int cdns_dp_set_video_status(struct cdns_mhdp8501_device *mhdp, int active)
+{
+	u8 msg;
+	int ret;
+
+	msg = !!active;
+
+	ret = cdns_mhdp_mailbox_send(&mhdp->base, MB_MODULE_ID_DP_TX,
+				     DPTX_SET_VIDEO, sizeof(msg), &msg);
+	if (ret)
+		dev_err(mhdp->dev, "set video status failed: %d\n", ret);
+
+	return ret;
+}
+
+static int cdns_dp_training_start(struct cdns_mhdp8501_device *mhdp)
+{
+	unsigned long timeout;
+	u8 msg, event[2];
+	int ret;
+
+	msg = LINK_TRAINING_RUN;
+
+	/* start training */
+	ret = cdns_mhdp_mailbox_send(&mhdp->base, MB_MODULE_ID_DP_TX,
+				     DPTX_TRAINING_CONTROL, sizeof(msg), &msg);
+	if (ret)
+		return ret;
+
+	timeout = jiffies + msecs_to_jiffies(LINK_TRAINING_TIMEOUT_MS);
+	while (time_before(jiffies, timeout)) {
+		msleep(LINK_TRAINING_RETRY_MS);
+		ret = cdns_mhdp_mailbox_send_recv(&mhdp->base, MB_MODULE_ID_DP_TX,
+						  DPTX_READ_EVENT,
+						  0, NULL, sizeof(event), event);
+		if (ret)
+			return ret;
+
+		if (event[1] & CLK_RECOVERY_FAILED)
+			dev_err(mhdp->dev, "clock recovery failed\n");
+		else if (event[1] & EQ_PHASE_FINISHED)
+			return 0;
+	}
+
+	return -ETIMEDOUT;
+}
+
+static int cdns_dp_get_training_status(struct cdns_mhdp8501_device *mhdp)
+{
+	u8 status[13];
+	int ret;
+
+	ret = cdns_mhdp_mailbox_send_recv(&mhdp->base, MB_MODULE_ID_DP_TX,
+					  DPTX_READ_LINK_STAT,
+					  0, NULL, sizeof(status), status);
+	if (ret)
+		return ret;
+
+	mhdp->dp.rate = drm_dp_bw_code_to_link_rate(status[0]);
+	mhdp->dp.num_lanes = status[1];
+
+	return ret;
+}
+
+static int cdns_dp_train_link(struct cdns_mhdp8501_device *mhdp)
+{
+	int ret;
+
+	ret = cdns_dp_training_start(mhdp);
+	if (ret) {
+		dev_err(mhdp->dev, "Failed to start training %d\n", ret);
+		return ret;
+	}
+
+	ret = cdns_dp_get_training_status(mhdp);
+	if (ret) {
+		dev_err(mhdp->dev, "Failed to get training stat %d\n", ret);
+		return ret;
+	}
+
+	dev_dbg(mhdp->dev, "rate:0x%x, lanes:%d\n", mhdp->dp.rate,
+		mhdp->dp.num_lanes);
+	return ret;
+}
+
+static int cdns_dp_set_host_cap(struct cdns_mhdp8501_device *mhdp)
+{
+	u8 msg[8];
+	int ret;
+
+	msg[0] = drm_dp_link_rate_to_bw_code(mhdp->dp.rate);
+	msg[1] = mhdp->dp.num_lanes | SCRAMBLER_EN;
+	msg[2] = VOLTAGE_LEVEL_2;
+	msg[3] = PRE_EMPHASIS_LEVEL_3;
+	msg[4] = PTS1 | PTS2 | PTS3 | PTS4;
+	msg[5] = FAST_LT_NOT_SUPPORT;
+	msg[6] = mhdp->lane_mapping;
+	msg[7] = ENHANCED;
+
+	ret = cdns_mhdp_mailbox_send(&mhdp->base, MB_MODULE_ID_DP_TX,
+				     DPTX_SET_HOST_CAPABILITIES,
+				     sizeof(msg), msg);
+	if (ret)
+		dev_err(mhdp->dev, "set host cap failed: %d\n", ret);
+
+	return ret;
+}
+
+static int cdns_dp_get_edid_block(void *data, u8 *edid,
+				  unsigned int block, size_t length)
+{
+	struct cdns_mhdp8501_device *mhdp = data;
+	u8 msg[2], reg[2], i;
+	int ret;
+
+	for (i = 0; i < 4; i++) {
+		msg[0] = block / 2;
+		msg[1] = block % 2;
+
+		ret = cdns_mhdp_mailbox_send_recv_multi(&mhdp->base,
+							MB_MODULE_ID_DP_TX,
+							DPTX_GET_EDID,
+							sizeof(msg), msg,
+							DPTX_GET_EDID,
+							sizeof(reg), reg,
+							length, edid);
+		if (ret)
+			continue;
+
+		if (reg[0] == length && reg[1] == block / 2)
+			break;
+	}
+
+	if (ret)
+		dev_err(mhdp->dev, "get block[%d] edid failed: %d\n",
+			block, ret);
+
+	return ret;
+}
+
+static void cdns_dp_mode_set(struct cdns_mhdp8501_device *mhdp,
+			     const struct drm_display_mode *mode)
+{
+	union phy_configure_opts phy_cfg;
+	int ret;
+
+	cdns_dp_pixel_clk_reset(mhdp);
+
+	/* Get DP Caps  */
+	ret = drm_dp_dpcd_read(&mhdp->dp.aux, DP_DPCD_REV, mhdp->dp.dpcd,
+			       DP_RECEIVER_CAP_SIZE);
+	if (ret < 0) {
+		dev_err(mhdp->dev, "Failed to get caps %d\n", ret);
+		return;
+	}
+
+	mhdp->dp.rate = drm_dp_max_link_rate(mhdp->dp.dpcd);
+	mhdp->dp.num_lanes = drm_dp_max_lane_count(mhdp->dp.dpcd);
+
+	/* check the max link rate */
+	if (mhdp->dp.rate > CDNS_DP_MAX_LINK_RATE)
+		mhdp->dp.rate = CDNS_DP_MAX_LINK_RATE;
+
+	phy_cfg.dp.lanes = mhdp->dp.num_lanes;
+	phy_cfg.dp.link_rate = mhdp->dp.rate;
+	phy_cfg.dp.set_lanes = false;
+	phy_cfg.dp.set_rate = false;
+	phy_cfg.dp.set_voltages = false;
+
+	ret = phy_configure(mhdp->phy, &phy_cfg);
+	if (ret) {
+		dev_err(mhdp->dev, "%s: phy_configure() failed: %d\n",
+			__func__, ret);
+		return;
+	}
+
+	/* Video off */
+	ret = cdns_dp_set_video_status(mhdp, CONTROL_VIDEO_IDLE);
+	if (ret) {
+		dev_err(mhdp->dev, "Failed to valid video %d\n", ret);
+		return;
+	}
+
+	/* Line swapping */
+	cdns_mhdp_reg_write(&mhdp->base, LANES_CONFIG, 0x00400000 | mhdp->lane_mapping);
+
+	/* Set DP host capability */
+	ret = cdns_dp_set_host_cap(mhdp);
+	if (ret) {
+		dev_err(mhdp->dev, "Failed to set host cap %d\n", ret);
+		return;
+	}
+
+	ret = cdns_mhdp_reg_write(&mhdp->base, DP_AUX_SWAP_INVERSION_CONTROL,
+				  AUX_HOST_INVERT);
+	if (ret) {
+		dev_err(mhdp->dev, "Failed to set host invert %d\n", ret);
+		return;
+	}
+
+	ret = cdns_dp_config_video(mhdp, mode);
+	if (ret)
+		dev_err(mhdp->dev, "Failed to config video %d\n", ret);
+}
+
+static bool
+cdns_dp_needs_link_retrain(struct cdns_mhdp8501_device *mhdp)
+{
+	u8 link_status[DP_LINK_STATUS_SIZE];
+
+	if (drm_dp_dpcd_read_phy_link_status(&mhdp->dp.aux, DP_PHY_DPRX,
+					     link_status) < 0)
+		return false;
+
+	/* Retrain if link not ok */
+	return !drm_dp_channel_eq_ok(link_status, mhdp->dp.num_lanes);
+}
+
+void cdns_dp_check_link_state(struct cdns_mhdp8501_device *mhdp)
+{
+	struct drm_connector *connector = mhdp->curr_conn;
+	const struct drm_edid *drm_edid;
+	struct drm_connector_state *conn_state;
+	struct drm_crtc_state *crtc_state;
+	struct drm_crtc *crtc;
+
+	if (!connector)
+		return;
+
+	/*
+	 * EDID data needs updating after each cable plugin
+	 * due to potential display monitor changes
+	 */
+	drm_edid = drm_edid_read_custom(connector, cdns_dp_get_edid_block, mhdp);
+	drm_edid_connector_update(connector, drm_edid);
+
+	if (!drm_edid)
+		return;
+
+	drm_edid_free(drm_edid);
+
+	conn_state = connector->state;
+	crtc = conn_state->crtc;
+	if (!crtc)
+		return;
+
+	crtc_state = crtc->state;
+	if (!crtc_state->active)
+		return;
+
+	if (!cdns_dp_needs_link_retrain(mhdp))
+		return;
+
+	/* DP link retrain */
+	if (cdns_dp_train_link(mhdp))
+		dev_err(mhdp->dev, "Failed link train\n");
+}
+
+static int cdns_dp_bridge_attach(struct drm_bridge *bridge,
+				 struct drm_encoder *encoder,
+				 enum drm_bridge_attach_flags flags)
+{
+	struct cdns_mhdp8501_device *mhdp = bridge->driver_private;
+
+	if (!(flags & DRM_BRIDGE_ATTACH_NO_CONNECTOR)) {
+		dev_err(mhdp->dev, "do not support creating a drm_connector\n");
+		return -EINVAL;
+	}
+
+	mhdp->dp.aux.drm_dev = bridge->dev;
+
+	return drm_dp_aux_register(&mhdp->dp.aux);
+}
+
+static const struct drm_edid
+*cdns_dp_bridge_edid_read(struct drm_bridge *bridge,
+			  struct drm_connector *connector)
+{
+	struct cdns_mhdp8501_device *mhdp = bridge->driver_private;
+
+	return drm_edid_read_custom(connector, cdns_dp_get_edid_block, mhdp);
+}
+
+/* Currently supported format */
+static const u32 mhdp8501_input_fmts[] = {
+	MEDIA_BUS_FMT_RGB888_1X24,
+	MEDIA_BUS_FMT_RGB101010_1X30,
+};
+
+static u32 *cdns_dp_bridge_atomic_get_input_bus_fmts(struct drm_bridge *bridge,
+						     struct drm_bridge_state *bridge_state,
+						     struct drm_crtc_state *crtc_state,
+						     struct drm_connector_state *conn_state,
+						     u32 output_fmt,
+						     unsigned int *num_input_fmts)
+{
+	u32 *input_fmts;
+
+	*num_input_fmts = 0;
+
+	input_fmts = kcalloc(ARRAY_SIZE(mhdp8501_input_fmts),
+			     sizeof(*input_fmts),
+			     GFP_KERNEL);
+	if (!input_fmts)
+		return NULL;
+
+	*num_input_fmts = ARRAY_SIZE(mhdp8501_input_fmts);
+	memcpy(input_fmts, mhdp8501_input_fmts, sizeof(mhdp8501_input_fmts));
+
+	return input_fmts;
+}
+
+static int cdns_dp_bridge_atomic_check(struct drm_bridge *bridge,
+				       struct drm_bridge_state *bridge_state,
+				       struct drm_crtc_state *crtc_state,
+				       struct drm_connector_state *conn_state)
+{
+	struct cdns_mhdp8501_device *mhdp = bridge->driver_private;
+	struct video_info *video = &mhdp->video_info;
+
+	if (bridge_state->input_bus_cfg.format == MEDIA_BUS_FMT_RGB888_1X24) {
+		video->bpc = 8;
+		video->color_fmt = DRM_COLOR_FORMAT_RGB444;
+	} else if (bridge_state->input_bus_cfg.format == MEDIA_BUS_FMT_RGB101010_1X30) {
+		video->bpc = 10;
+		video->color_fmt = DRM_COLOR_FORMAT_RGB444;
+	} else {
+		return -EINVAL;
+	}
+
+	return 0;
+}
+
+static void cdns_dp_bridge_atomic_disable(struct drm_bridge *bridge,
+					  struct drm_atomic_state *state)
+{
+	struct cdns_mhdp8501_device *mhdp = bridge->driver_private;
+
+	cdns_dp_set_video_status(mhdp, CONTROL_VIDEO_IDLE);
+	mhdp->curr_conn = NULL;
+
+	phy_power_off(mhdp->phy);
+}
+
+static void cdns_dp_bridge_atomic_enable(struct drm_bridge *bridge,
+					 struct drm_atomic_state *state)
+{
+	struct cdns_mhdp8501_device *mhdp = bridge->driver_private;
+	struct drm_connector *connector;
+	struct drm_crtc_state *crtc_state;
+	struct drm_connector_state *conn_state;
+	int ret;
+
+	connector = drm_atomic_get_new_connector_for_encoder(state,
+							     bridge->encoder);
+	if (WARN_ON(!connector))
+		return;
+
+	mhdp->curr_conn = connector;
+
+	conn_state = drm_atomic_get_new_connector_state(state, connector);
+	if (WARN_ON(!conn_state))
+		return;
+
+	crtc_state = drm_atomic_get_new_crtc_state(state, conn_state->crtc);
+	if (WARN_ON(!crtc_state))
+		return;
+
+	cdns_dp_mode_set(mhdp, &crtc_state->adjusted_mode);
+
+	/* Power up PHY before link training */
+	phy_power_on(mhdp->phy);
+
+	/* Link training */
+	ret = cdns_dp_train_link(mhdp);
+	if (ret) {
+		dev_err(mhdp->dev, "Failed link train %d\n", ret);
+		return;
+	}
+
+	ret = cdns_dp_set_video_status(mhdp, CONTROL_VIDEO_VALID);
+	if (ret) {
+		dev_err(mhdp->dev, "Failed to valid video %d\n", ret);
+		return;
+	}
+}
+
+const struct drm_bridge_funcs cdns_dp_bridge_funcs = {
+	.attach = cdns_dp_bridge_attach,
+	.detect = cdns_mhdp8501_detect,
+	.edid_read = cdns_dp_bridge_edid_read,
+	.mode_valid = cdns_mhdp8501_mode_valid,
+	.atomic_enable = cdns_dp_bridge_atomic_enable,
+	.atomic_disable = cdns_dp_bridge_atomic_disable,
+	.atomic_get_input_bus_fmts = cdns_dp_bridge_atomic_get_input_bus_fmts,
+	.atomic_check = cdns_dp_bridge_atomic_check,
+	.atomic_duplicate_state = drm_atomic_helper_bridge_duplicate_state,
+	.atomic_destroy_state = drm_atomic_helper_bridge_destroy_state,
+	.atomic_reset = drm_atomic_helper_bridge_reset,
+};
diff --git a/drivers/gpu/drm/bridge/cadence/cdns-mhdp8501-hdmi.c b/drivers/gpu/drm/bridge/cadence/cdns-mhdp8501-hdmi.c
new file mode 100644
index 0000000000000..9556d0929e21d
--- /dev/null
+++ b/drivers/gpu/drm/bridge/cadence/cdns-mhdp8501-hdmi.c
@@ -0,0 +1,745 @@
+// SPDX-License-Identifier: GPL-2.0-only
+/*
+ * Cadence MHDP8501 HDMI bridge driver
+ *
+ * Copyright (C) 2019-2024 NXP Semiconductor, Inc.
+ *
+ */
+#include <drm/display/drm_hdmi_helper.h>
+#include <drm/display/drm_hdmi_state_helper.h>
+#include <drm/display/drm_scdc_helper.h>
+#include <drm/drm_atomic_helper.h>
+#include <drm/drm_edid.h>
+#include <drm/drm_print.h>
+#include <linux/phy/phy.h>
+#include <linux/phy/phy-hdmi.h>
+
+#include "cdns-mhdp8501-core.h"
+
+/**
+ * cdns_hdmi_config_infoframe() - fill the HDMI infoframe
+ * @mhdp: phandle to mhdp device.
+ * @entry_id: The packet memory address in which the data is written.
+ * @len: length of infoframe.
+ * @buf: point to InfoFrame Packet.
+ * @type: Packet Type of InfoFrame in HDMI Specification.
+ *
+ */
+
+static void cdns_hdmi_clear_infoframe(struct cdns_mhdp8501_device *mhdp,
+				      u8 entry_id, u8 type)
+{
+	u32 val;
+
+	/* invalidate entry */
+	val = F_ACTIVE_IDLE_TYPE(1) | F_PKT_ALLOC_ADDRESS(entry_id) |
+	      F_PACKET_TYPE(type);
+	writel(val, mhdp->regs + SOURCE_PIF_PKT_ALLOC_REG);
+	writel(F_PKT_ALLOC_WR_EN(1), mhdp->regs + SOURCE_PIF_PKT_ALLOC_WR_EN);
+}
+
+static void cdns_hdmi_config_infoframe(struct cdns_mhdp8501_device *mhdp,
+				       u8 entry_id, u8 len,
+				       const u8 *buf, u8 type)
+{
+	u8 packet[32], packet_len = 32;
+	u32 packet32, len32;
+	u32 val, i;
+
+	/*
+	 * only support 32 bytes now
+	 * packet[0] = 0
+	 * packet[1-3] = HB[0-2]  InfoFrame Packet Header
+	 * packet[4-31 = PB[0-27] InfoFrame Packet Contents
+	 */
+	if (len >= (packet_len - 1))
+		return;
+	packet[0] = 0;
+	memcpy(packet + 1, buf, len);
+
+	cdns_hdmi_clear_infoframe(mhdp, entry_id, type);
+
+	/* flush fifo 1 */
+	writel(F_FIFO1_FLUSH(1), mhdp->regs + SOURCE_PIF_FIFO1_FLUSH);
+
+	/* write packet into memory */
+	len32 = packet_len / 4;
+	for (i = 0; i < len32; i++) {
+		packet32 = get_unaligned_le32(packet + 4 * i);
+		writel(F_DATA_WR(packet32), mhdp->regs + SOURCE_PIF_DATA_WR);
+	}
+
+	/* write entry id */
+	writel(F_WR_ADDR(entry_id), mhdp->regs + SOURCE_PIF_WR_ADDR);
+
+	/* write request */
+	writel(F_HOST_WR(1), mhdp->regs + SOURCE_PIF_WR_REQ);
+
+	/* update entry */
+	val = F_ACTIVE_IDLE_TYPE(1) | F_TYPE_VALID(1) |
+	      F_PACKET_TYPE(type) | F_PKT_ALLOC_ADDRESS(entry_id);
+	writel(val, mhdp->regs + SOURCE_PIF_PKT_ALLOC_REG);
+
+	writel(F_PKT_ALLOC_WR_EN(1), mhdp->regs + SOURCE_PIF_PKT_ALLOC_WR_EN);
+}
+
+static int cdns_hdmi_get_edid_block(void *data, u8 *edid,
+				    u32 block, size_t length)
+{
+	struct cdns_mhdp8501_device *mhdp = data;
+	u8 msg[2], reg[5], i;
+	int ret;
+
+	for (i = 0; i < 4; i++) {
+		msg[0] = block / 2;
+		msg[1] = block % 2;
+
+		ret = cdns_mhdp_mailbox_send_recv_multi(&mhdp->base,
+							MB_MODULE_ID_HDMI_TX,
+							HDMI_TX_EDID,
+							sizeof(msg), msg,
+							HDMI_TX_EDID,
+							sizeof(reg), reg,
+							length, edid);
+
+		if (ret)
+			continue;
+
+		if ((reg[3] << 8 | reg[4]) == length)
+			break;
+	}
+
+	if (ret)
+		dev_err(mhdp->dev, "get block[%d] edid failed: %d\n", block, ret);
+	return ret;
+}
+
+static int cdns_hdmi_set_hdmi_mode_type(struct cdns_mhdp8501_device *mhdp)
+{
+	struct drm_connector_state *conn_state = mhdp->curr_conn->state;
+	u32 protocol = mhdp->hdmi.hdmi_type;
+	u32 val;
+
+	if (protocol == MODE_HDMI_2_0 &&
+	    conn_state->hdmi.tmds_char_rate >= 340000000) {
+		cdns_mhdp_reg_write(&mhdp->base, HDTX_CLOCK_REG_0, 0);
+		cdns_mhdp_reg_write(&mhdp->base, HDTX_CLOCK_REG_1, 0xFFFFF);
+	}
+
+	cdns_mhdp_reg_read(&mhdp->base, HDTX_CONTROLLER, &val);
+
+	/* set HDMI mode and preemble mode data enable */
+	val |= F_HDMI_MODE(protocol) | F_HDMI2_PREAMBLE_EN(1) |
+	       F_HDMI2_CTRL_IL_MODE(1);
+	return cdns_mhdp_reg_write(&mhdp->base, HDTX_CONTROLLER, val);
+}
+
+static int cdns_hdmi_ctrl_init(struct cdns_mhdp8501_device *mhdp)
+{
+	u32 val;
+	int ret;
+
+	/* Set PHY to HDMI data */
+	ret = cdns_mhdp_reg_write(&mhdp->base, PHY_DATA_SEL, F_SOURCE_PHY_MHDP_SEL(1));
+	if (ret < 0)
+		return ret;
+
+	ret = cdns_mhdp_reg_write(&mhdp->base, HDTX_HPD,
+				  F_HPD_VALID_WIDTH(4) | F_HPD_GLITCH_WIDTH(0));
+	if (ret < 0)
+		return ret;
+
+	/* open CARS */
+	ret = cdns_mhdp_reg_write(&mhdp->base, SOURCE_PHY_CAR, 0xF);
+	if (ret < 0)
+		return ret;
+	ret = cdns_mhdp_reg_write(&mhdp->base, SOURCE_HDTX_CAR, 0xFF);
+	if (ret < 0)
+		return ret;
+	ret = cdns_mhdp_reg_write(&mhdp->base, SOURCE_PKT_CAR, 0xF);
+	if (ret < 0)
+		return ret;
+	ret = cdns_mhdp_reg_write(&mhdp->base, SOURCE_AIF_CAR, 0xF);
+	if (ret < 0)
+		return ret;
+	ret = cdns_mhdp_reg_write(&mhdp->base, SOURCE_CIPHER_CAR, 0xF);
+	if (ret < 0)
+		return ret;
+	ret = cdns_mhdp_reg_write(&mhdp->base, SOURCE_CRYPTO_CAR, 0xF);
+	if (ret < 0)
+		return ret;
+	ret = cdns_mhdp_reg_write(&mhdp->base, SOURCE_CEC_CAR, 3);
+	if (ret < 0)
+		return ret;
+
+	ret = cdns_mhdp_reg_write(&mhdp->base, HDTX_CLOCK_REG_0, 0x7c1f);
+	if (ret < 0)
+		return ret;
+	ret = cdns_mhdp_reg_write(&mhdp->base, HDTX_CLOCK_REG_1, 0x7c1f);
+	if (ret < 0)
+		return ret;
+
+	/* init HDMI Controller */
+	val = F_BCH_EN(1) | F_PIC_3D(0xF) | F_CLEAR_AVMUTE(1);
+	ret = cdns_mhdp_reg_write(&mhdp->base, HDTX_CONTROLLER, val);
+	if (ret < 0)
+		return ret;
+
+	return cdns_hdmi_set_hdmi_mode_type(mhdp);
+}
+
+static int cdns_hdmi_mode_config(struct cdns_mhdp8501_device *mhdp,
+				 struct drm_display_mode *mode,
+				 struct drm_connector_hdmi_state *hdmi)
+{
+	u32 vsync_lines = mode->vsync_end - mode->vsync_start;
+	u32 eof_lines = mode->vsync_start - mode->vdisplay;
+	u32 sof_lines = mode->vtotal - mode->vsync_end;
+	u32 hblank = mode->htotal - mode->hdisplay;
+	u32 hactive = mode->hdisplay;
+	u32 vblank = mode->vtotal - mode->vdisplay;
+	u32 vactive = mode->vdisplay;
+	u32 hfront = mode->hsync_start - mode->hdisplay;
+	u32 hback = mode->htotal - mode->hsync_end;
+	u32 vfront = eof_lines;
+	u32 hsync = hblank - hfront - hback;
+	u32 vsync = vsync_lines;
+	u32 vback = sof_lines;
+	u32 v_h_polarity = ((mode->flags & DRM_MODE_FLAG_NHSYNC) ? 0 : 1) +
+			   ((mode->flags & DRM_MODE_FLAG_NVSYNC) ? 0 : 2);
+	int ret;
+	u32 val;
+
+	ret = cdns_mhdp_reg_write(&mhdp->base, SCHEDULER_H_SIZE, (hactive << 16) + hblank);
+	if (ret < 0)
+		return ret;
+
+	ret = cdns_mhdp_reg_write(&mhdp->base, SCHEDULER_V_SIZE, (vactive << 16) + vblank);
+	if (ret < 0)
+		return ret;
+
+	ret = cdns_mhdp_reg_write(&mhdp->base, HDTX_SIGNAL_FRONT_WIDTH, (vfront << 16) + hfront);
+	if (ret < 0)
+		return ret;
+
+	ret = cdns_mhdp_reg_write(&mhdp->base, HDTX_SIGNAL_SYNC_WIDTH, (vsync << 16) + hsync);
+	if (ret < 0)
+		return ret;
+
+	ret = cdns_mhdp_reg_write(&mhdp->base, HDTX_SIGNAL_BACK_WIDTH, (vback << 16) + hback);
+	if (ret < 0)
+		return ret;
+
+	ret = cdns_mhdp_reg_write(&mhdp->base, HSYNC2VSYNC_POL_CTRL, v_h_polarity);
+	if (ret < 0)
+		return ret;
+
+	/* Reset Data Enable */
+	cdns_mhdp_reg_read(&mhdp->base, HDTX_CONTROLLER, &val);
+	val &= ~F_DATA_EN(1);
+	ret = cdns_mhdp_reg_write(&mhdp->base, HDTX_CONTROLLER, val);
+	if (ret < 0)
+		return ret;
+
+	/* Set bpc */
+	val &= ~F_VIF_DATA_WIDTH(3);
+	switch (hdmi->output_bpc) {
+	case 10:
+		val |= F_VIF_DATA_WIDTH(1);
+		break;
+	case 12:
+		val |= F_VIF_DATA_WIDTH(2);
+		break;
+	case 16:
+		val |= F_VIF_DATA_WIDTH(3);
+		break;
+	case 8:
+	default:
+		val |= F_VIF_DATA_WIDTH(0);
+		break;
+	}
+
+	/* select color encoding */
+	val &= ~F_HDMI_ENCODING(3);
+	switch (hdmi->output_format) {
+	case HDMI_COLORSPACE_YUV444:
+		val |= F_HDMI_ENCODING(2);
+		break;
+	case HDMI_COLORSPACE_YUV422:
+		val |= F_HDMI_ENCODING(1);
+		break;
+	case HDMI_COLORSPACE_YUV420:
+		val |= F_HDMI_ENCODING(3);
+		break;
+	case HDMI_COLORSPACE_RGB:
+	default:
+		val |= F_HDMI_ENCODING(0);
+		break;
+	}
+
+	ret = cdns_mhdp_reg_write(&mhdp->base, HDTX_CONTROLLER, val);
+	if (ret < 0)
+		return ret;
+
+	/* set data enable */
+	val |= F_DATA_EN(1);
+	return cdns_mhdp_reg_write(&mhdp->base, HDTX_CONTROLLER, val);
+}
+
+static int cdns_hdmi_disable_gcp(struct cdns_mhdp8501_device *mhdp)
+{
+	u32 val;
+
+	cdns_mhdp_reg_read(&mhdp->base, HDTX_CONTROLLER, &val);
+	val &= ~F_GCP_EN(1);
+
+	return cdns_mhdp_reg_write(&mhdp->base, HDTX_CONTROLLER, val);
+}
+
+static int cdns_hdmi_enable_gcp(struct cdns_mhdp8501_device *mhdp)
+{
+	u32 val;
+
+	cdns_mhdp_reg_read(&mhdp->base, HDTX_CONTROLLER, &val);
+	val |= F_GCP_EN(1);
+
+	return cdns_mhdp_reg_write(&mhdp->base, HDTX_CONTROLLER, val);
+}
+
+#define HDMI_14_MAX_TMDS_CLK   (340 * 1000 * 1000)
+static void cdns_hdmi_sink_config(struct cdns_mhdp8501_device *mhdp,
+				  unsigned long long tmds_char_rate)
+{
+	struct drm_connector *connector = mhdp->curr_conn;
+	struct drm_display_info *display = &connector->display_info;
+	struct drm_scdc *scdc = &display->hdmi.scdc;
+	bool hdmi_scrambling = false;
+	bool hdmi_high_tmds_clock_ratio = false;
+
+	/* check sink type (HDMI or DVI) */
+	if (!display->is_hdmi) {
+		mhdp->hdmi.hdmi_type = MODE_DVI;
+		return;
+	}
+
+	/* Default work in HDMI1.4 */
+	mhdp->hdmi.hdmi_type = MODE_HDMI_1_4;
+
+	/* check sink support SCDC or not */
+	if (!scdc->supported) {
+		dev_dbg(mhdp->dev, "Sink Not Support SCDC\n");
+		return;
+	}
+
+	if (tmds_char_rate > HDMI_14_MAX_TMDS_CLK) {
+		hdmi_scrambling = true;
+		hdmi_high_tmds_clock_ratio = true;
+		mhdp->hdmi.hdmi_type = MODE_HDMI_2_0;
+	} else if (scdc->scrambling.low_rates) {
+		hdmi_scrambling = true;
+		mhdp->hdmi.hdmi_type = MODE_HDMI_2_0;
+	}
+
+	/* Set TMDS bit clock ratio to 1/40 or 1/10, and enable/disable scrambling */
+	drm_scdc_set_high_tmds_clock_ratio(connector, hdmi_high_tmds_clock_ratio);
+	drm_scdc_set_scrambling(connector, hdmi_scrambling);
+}
+
+static int cdns_hdmi_bridge_attach(struct drm_bridge *bridge,
+				   struct drm_encoder *encoder,
+				   enum drm_bridge_attach_flags flags)
+{
+	struct cdns_mhdp8501_device *mhdp = bridge->driver_private;
+
+	if (!(flags & DRM_BRIDGE_ATTACH_NO_CONNECTOR)) {
+		dev_err(mhdp->dev, "do not support creating a drm_connector\n");
+		return -EINVAL;
+	}
+
+	return 0;
+}
+
+static int reset_pipe(struct drm_crtc *crtc)
+{
+	struct drm_atomic_state *state;
+	struct drm_crtc_state *crtc_state;
+	struct drm_modeset_acquire_ctx ctx;
+	int ret;
+
+	state = drm_atomic_state_alloc(crtc->dev);
+	if (!state)
+		return -ENOMEM;
+
+	drm_modeset_acquire_init(&ctx, 0);
+
+	state->acquire_ctx = &ctx;
+
+	crtc_state = drm_atomic_get_crtc_state(state, crtc);
+	if (IS_ERR(crtc_state)) {
+		ret = PTR_ERR(crtc_state);
+		goto out;
+	}
+
+	crtc_state->connectors_changed = true;
+
+	ret = drm_atomic_commit(state);
+out:
+	drm_atomic_state_put(state);
+	drm_modeset_drop_locks(&ctx);
+	drm_modeset_acquire_fini(&ctx);
+
+	return ret;
+}
+
+void cdns_hdmi_handle_hotplug(struct cdns_mhdp8501_device *mhdp)
+{
+	struct drm_connector *connector = mhdp->curr_conn;
+	const struct drm_edid *drm_edid;
+	struct drm_connector_state *conn_state;
+	struct drm_crtc_state *crtc_state;
+	struct drm_crtc *crtc;
+
+	if (!connector)
+		return;
+
+	/*
+	 * EDID data needs updating after each cable plugin
+	 * due to potential display monitor changes
+	 */
+	drm_edid = drm_edid_read_custom(connector, cdns_hdmi_get_edid_block, mhdp);
+	drm_edid_connector_update(connector, drm_edid);
+
+	if (!drm_edid)
+		return;
+
+	drm_edid_free(drm_edid);
+
+	conn_state = connector->state;
+	crtc = conn_state->crtc;
+	if (!crtc)
+		return;
+
+	crtc_state = crtc->state;
+	if (!crtc_state->active)
+		return;
+
+	/*
+	 * HDMI 2.0 says that one should not send scrambled data
+	 * prior to configuring the sink scrambling, and that
+	 * TMDS clock/data transmission should be suspended when
+	 * changing the TMDS clock rate in the sink. So let's
+	 * just do a full modeset here, even though some sinks
+	 * would be perfectly happy if were to just reconfigure
+	 * the SCDC settings on the fly.
+	 */
+	reset_pipe(crtc);
+}
+
+static int cdns_hdmi_i2c_write(struct cdns_mhdp8501_device *mhdp,
+			       struct i2c_msg *msgs)
+{
+	u8 msg[5], reg[5];
+	int ret;
+
+	msg[0] = msgs->addr;
+	msg[1] = msgs->buf[0];
+	msg[2] = 0;
+	msg[3] = 1;
+	msg[4] = msgs->buf[1];
+
+	ret = cdns_mhdp_mailbox_send_recv(&mhdp->base,
+					  MB_MODULE_ID_HDMI_TX, HDMI_TX_WRITE,
+					  sizeof(msg), msg, sizeof(reg), reg);
+	if (ret) {
+		dev_err(mhdp->dev, "I2C write failed: %d\n", ret);
+		return ret;
+	}
+
+	if (reg[0] != 0)
+		return -EINVAL;
+
+	return 0;
+}
+
+static int cdns_hdmi_i2c_read(struct cdns_mhdp8501_device *mhdp,
+			      struct i2c_msg *msgs, int num)
+{
+	u8 msg[4], reg[5];
+	u8 addr, offset, *buf, len;
+	int ret, i;
+
+	for (i = 0; i < num; i++) {
+		if (msgs[i].flags & I2C_M_RD) {
+			addr = msgs[i].addr;
+			buf = msgs[i].buf;
+			len = msgs[i].len;
+		} else {
+			offset = msgs[i].buf[0];
+		}
+	}
+
+	msg[0] = addr;
+	msg[1] = offset;
+	put_unaligned_be16(len, msg + 2);
+
+	ret = cdns_mhdp_mailbox_send_recv_multi(&mhdp->base,
+						MB_MODULE_ID_HDMI_TX, HDMI_TX_READ,
+						sizeof(msg), msg,
+						HDMI_TX_READ,
+						sizeof(reg), reg,
+						len, buf);
+	if (ret) {
+		dev_err(mhdp->dev, "I2c Read failed: %d\n", ret);
+		return ret;
+	}
+
+	return 0;
+}
+
+#define  SCDC_I2C_SLAVE_ADDRESS	0x54
+static int cdns_hdmi_i2c_xfer(struct i2c_adapter *adap,
+			      struct i2c_msg *msgs, int num)
+{
+	struct cdns_mhdp8501_device *mhdp = i2c_get_adapdata(adap);
+	struct cdns_hdmi_i2c *i2c = mhdp->hdmi.i2c;
+	int i, ret = 0;
+
+	/*
+	 * MHDP FW provides mailbox APIs for SCDC registers access, but lacks direct I2C APIs.
+	 * While individual I2C registers can be read/written using HDMI general register APIs,
+	 * block reads (e.g., EDID) are not supported, making it a limited I2C interface.
+	 */
+	for (i = 0; i < num; i++) {
+		if (msgs[i].addr != SCDC_I2C_SLAVE_ADDRESS) {
+			dev_err(mhdp->dev, "ADDR=%0x is not supported\n", msgs[i].addr);
+			return -EINVAL;
+		}
+	}
+
+	mutex_lock(&i2c->lock);
+
+	if (num == 1)
+		ret = cdns_hdmi_i2c_write(mhdp, msgs);
+	else
+		ret = cdns_hdmi_i2c_read(mhdp, msgs, num);
+
+	if (!ret)
+		ret = num;
+
+	mutex_unlock(&i2c->lock);
+
+	return ret;
+}
+
+static u32 cdns_hdmi_i2c_func(struct i2c_adapter *adapter)
+{
+	return I2C_FUNC_I2C | I2C_FUNC_SMBUS_EMUL;
+}
+
+static const struct i2c_algorithm cdns_hdmi_algorithm = {
+	.master_xfer	= cdns_hdmi_i2c_xfer,
+	.functionality	= cdns_hdmi_i2c_func,
+};
+
+struct i2c_adapter *cdns_hdmi_i2c_adapter(struct cdns_mhdp8501_device *mhdp)
+{
+	struct i2c_adapter *adap;
+	struct cdns_hdmi_i2c *i2c;
+	int ret;
+
+	i2c = devm_kzalloc(mhdp->dev, sizeof(*i2c), GFP_KERNEL);
+	if (!i2c)
+		return ERR_PTR(-ENOMEM);
+
+	mutex_init(&i2c->lock);
+
+	adap = &i2c->adap;
+	adap->owner = THIS_MODULE;
+	adap->dev.parent = mhdp->dev;
+	adap->algo = &cdns_hdmi_algorithm;
+	strscpy(adap->name, "MHDP HDMI", sizeof(adap->name));
+	i2c_set_adapdata(adap, mhdp);
+
+	ret = i2c_add_adapter(adap);
+	if (ret) {
+		dev_warn(mhdp->dev, "cannot add %s I2C adapter\n", adap->name);
+		devm_kfree(mhdp->dev, i2c);
+		return ERR_PTR(ret);
+	}
+
+	mhdp->hdmi.i2c = i2c;
+
+	return adap;
+}
+
+static enum drm_mode_status
+cdns_hdmi_tmds_char_rate_valid(const struct drm_bridge *bridge,
+			       const struct drm_display_mode *mode,
+			       unsigned long long tmds_rate)
+{
+	struct cdns_mhdp8501_device *mhdp = bridge->driver_private;
+	union phy_configure_opts phy_cfg;
+	int ret;
+
+	phy_cfg.hdmi.tmds_char_rate = tmds_rate;
+
+	ret = phy_validate(mhdp->phy, PHY_MODE_HDMI, 0, &phy_cfg);
+	if (ret < 0)
+		return MODE_CLOCK_RANGE;
+
+	return MODE_OK;
+}
+
+static const struct drm_edid
+*cdns_hdmi_bridge_edid_read(struct drm_bridge *bridge,
+			    struct drm_connector *connector)
+{
+	struct cdns_mhdp8501_device *mhdp = bridge->driver_private;
+
+	return drm_edid_read_custom(connector, cdns_hdmi_get_edid_block, mhdp);
+}
+
+static void cdns_hdmi_bridge_atomic_disable(struct drm_bridge *bridge,
+					    struct drm_atomic_state *state)
+{
+	struct cdns_mhdp8501_device *mhdp = bridge->driver_private;
+
+	mhdp->curr_conn = NULL;
+
+	phy_power_off(mhdp->phy);
+}
+
+static void cdns_hdmi_bridge_atomic_enable(struct drm_bridge *bridge,
+					   struct drm_atomic_state *state)
+{
+	struct cdns_mhdp8501_device *mhdp = bridge->driver_private;
+	struct drm_connector *connector;
+	struct drm_crtc_state *crtc_state;
+	struct drm_connector_state *conn_state;
+	struct drm_connector_hdmi_state *hdmi;
+	union phy_configure_opts phy_cfg;
+	int ret;
+
+	connector = drm_atomic_get_new_connector_for_encoder(state,
+							     bridge->encoder);
+	if (WARN_ON(!connector))
+		return;
+
+	mhdp->curr_conn = connector;
+
+	conn_state = drm_atomic_get_new_connector_state(state, connector);
+	if (WARN_ON(!conn_state))
+		return;
+
+	crtc_state = drm_atomic_get_new_crtc_state(state, conn_state->crtc);
+	if (WARN_ON(!crtc_state))
+		return;
+
+	drm_atomic_helper_connector_hdmi_update_infoframes(connector, state);
+
+	/* Line swapping */
+	cdns_mhdp_reg_write(&mhdp->base, LANES_CONFIG, 0x00400000 | mhdp->lane_mapping);
+
+	hdmi = &conn_state->hdmi;
+	if (WARN_ON(!hdmi))
+		return;
+
+	phy_cfg.hdmi.tmds_char_rate = hdmi->tmds_char_rate;
+	ret = phy_configure(mhdp->phy, &phy_cfg);
+	if (ret) {
+		dev_err(mhdp->dev, "%s: phy_configure() failed: %d\n",
+			__func__, ret);
+		return;
+	}
+
+	phy_power_on(mhdp->phy);
+
+	cdns_hdmi_sink_config(mhdp, hdmi->tmds_char_rate);
+
+	ret = cdns_hdmi_ctrl_init(mhdp);
+	if (ret < 0) {
+		dev_err(mhdp->dev, "hdmi ctrl init failed = %d\n",  ret);
+		return;
+	}
+
+	/* Config GCP */
+	if (hdmi->output_bpc == 8)
+		cdns_hdmi_disable_gcp(mhdp);
+	else
+		cdns_hdmi_enable_gcp(mhdp);
+
+	ret = cdns_hdmi_mode_config(mhdp, &crtc_state->adjusted_mode, hdmi);
+	if (ret < 0) {
+		dev_err(mhdp->dev, "CDN_API_HDMITX_SetVic_blocking ret = %d\n", ret);
+		return;
+	}
+}
+
+static int cdns_hdmi_bridge_clear_infoframe(struct drm_bridge *bridge,
+					    enum hdmi_infoframe_type type)
+{
+	struct cdns_mhdp8501_device *mhdp = bridge->driver_private;
+
+	switch (type) {
+	case HDMI_INFOFRAME_TYPE_AVI:
+		cdns_hdmi_clear_infoframe(mhdp, 0, HDMI_INFOFRAME_TYPE_AVI);
+		break;
+	case HDMI_INFOFRAME_TYPE_SPD:
+		cdns_hdmi_clear_infoframe(mhdp, 1, HDMI_INFOFRAME_TYPE_SPD);
+		break;
+	case HDMI_INFOFRAME_TYPE_VENDOR:
+		cdns_hdmi_clear_infoframe(mhdp, 2, HDMI_INFOFRAME_TYPE_VENDOR);
+		break;
+	default:
+		dev_dbg(mhdp->dev, "Unsupported infoframe type %x\n", type);
+	}
+
+	return 0;
+}
+
+static int cdns_hdmi_bridge_write_infoframe(struct drm_bridge *bridge,
+					    enum hdmi_infoframe_type type,
+					    const u8 *buffer, size_t len)
+{
+	struct cdns_mhdp8501_device *mhdp = bridge->driver_private;
+
+	switch (type) {
+	case HDMI_INFOFRAME_TYPE_AVI:
+		cdns_hdmi_config_infoframe(mhdp, 0, len, buffer, HDMI_INFOFRAME_TYPE_AVI);
+		break;
+	case HDMI_INFOFRAME_TYPE_SPD:
+		cdns_hdmi_config_infoframe(mhdp, 1, len, buffer, HDMI_INFOFRAME_TYPE_SPD);
+		break;
+	case HDMI_INFOFRAME_TYPE_VENDOR:
+		cdns_hdmi_config_infoframe(mhdp, 2, len, buffer, HDMI_INFOFRAME_TYPE_VENDOR);
+		break;
+	default:
+		dev_dbg(mhdp->dev, "Unsupported infoframe type %x\n", type);
+	}
+
+	return 0;
+}
+
+static int cdns_hdmi_bridge_atomic_check(struct drm_bridge *bridge,
+					 struct drm_bridge_state *bridge_state,
+					 struct drm_crtc_state *crtc_state,
+					 struct drm_connector_state *conn_state)
+{
+	return drm_atomic_helper_connector_hdmi_check(conn_state->connector, conn_state->state);
+}
+
+const struct drm_bridge_funcs cdns_hdmi_bridge_funcs = {
+	.attach = cdns_hdmi_bridge_attach,
+	.detect = cdns_mhdp8501_detect,
+	.edid_read = cdns_hdmi_bridge_edid_read,
+	.mode_valid = cdns_mhdp8501_mode_valid,
+	.atomic_enable = cdns_hdmi_bridge_atomic_enable,
+	.atomic_disable = cdns_hdmi_bridge_atomic_disable,
+	.atomic_check = cdns_hdmi_bridge_atomic_check,
+	.atomic_duplicate_state = drm_atomic_helper_bridge_duplicate_state,
+	.atomic_destroy_state = drm_atomic_helper_bridge_destroy_state,
+	.atomic_reset = drm_atomic_helper_bridge_reset,
+	.hdmi_clear_infoframe = cdns_hdmi_bridge_clear_infoframe,
+	.hdmi_write_infoframe = cdns_hdmi_bridge_write_infoframe,
+	.hdmi_tmds_char_rate_valid = cdns_hdmi_tmds_char_rate_valid,
+};

From patchwork Tue Dec 17 06:51:48 2024
Content-Type: text/plain; charset="utf-8"
MIME-Version: 1.0
Content-Transfer-Encoding: 7bit
Subject: [v20,6/9] dt-bindings: phy: Add Freescale iMX8MQ DP and HDMI PHY
From: Sandor Yu <Sandor.yu@nxp.com>
X-Patchwork-Id: 629293
Message-Id: 
 <1f01892a4e462d451a21ddcb4b114283d998cd1b.1734340233.git.Sandor.yu@nxp.com>
To: dmitry.baryshkov@linaro.org, andrzej.hajda@intel.com,
 neil.armstrong@linaro.org, Laurent.pinchart@ideasonboard.com,
 jonas@kwiboo.se, jernej.skrabec@gmail.com, airlied@gmail.com,
 daniel@ffwll.ch, robh+dt@kernel.org, krzysztof.kozlowski+dt@linaro.org,
 shawnguo@kernel.org, s.hauer@pengutronix.de, festevam@gmail.com,
 vkoul@kernel.org, dri-devel@lists.freedesktop.org,
 devicetree@vger.kernel.org, linux-arm-kernel@lists.infradead.org,
 linux-kernel@vger.kernel.org, linux-phy@lists.infradead.org,
 mripard@kernel.org
Cc: kernel@pengutronix.de, linux-imx@nxp.com, Sandor.yu@nxp.com,
 oliver.brown@nxp.com, alexander.stein@ew.tq-group.com, sam@ravnborg.org,
 Rob Herring <robh@kernel.org>
Date: Tue, 17 Dec 2024 14:51:48 +0800

Add bindings for Freescale iMX8MQ DP and HDMI PHY.

Signed-off-by: Sandor Yu <Sandor.yu@nxp.com>
Reviewed-by: Rob Herring <robh@kernel.org>
---
v9->v20:
 *No change.

 .../bindings/phy/fsl,imx8mq-dp-hdmi-phy.yaml  | 51 +++++++++++++++++++
 1 file changed, 51 insertions(+)
 create mode 100644 Documentation/devicetree/bindings/phy/fsl,imx8mq-dp-hdmi-phy.yaml

diff --git a/Documentation/devicetree/bindings/phy/fsl,imx8mq-dp-hdmi-phy.yaml b/Documentation/devicetree/bindings/phy/fsl,imx8mq-dp-hdmi-phy.yaml
new file mode 100644
index 0000000000000..c17a645e71bad
--- /dev/null
+++ b/Documentation/devicetree/bindings/phy/fsl,imx8mq-dp-hdmi-phy.yaml
@@ -0,0 +1,51 @@
+# SPDX-License-Identifier: (GPL-2.0 OR BSD-2-Clause)
+%YAML 1.2
+---
+$id: http://devicetree.org/schemas/phy/fsl,imx8mq-dp-hdmi-phy.yaml#
+$schema: http://devicetree.org/meta-schemas/core.yaml#
+
+title: Cadence HDP-TX DP/HDMI PHY for Freescale i.MX8MQ SoC
+
+maintainers:
+  - Sandor Yu <sandor.yu@nxp.com>
+
+properties:
+  compatible:
+    const: fsl,imx8mq-hdptx-phy
+
+  reg:
+    maxItems: 1
+
+  clocks:
+    items:
+      - description: PHY reference clock.
+      - description: APB clock.
+
+  clock-names:
+    items:
+      - const: ref
+      - const: apb
+
+  "#phy-cells":
+    const: 0
+
+required:
+  - compatible
+  - reg
+  - clocks
+  - clock-names
+  - "#phy-cells"
+
+additionalProperties: false
+
+examples:
+  - |
+    #include <dt-bindings/clock/imx8mq-clock.h>
+    #include <dt-bindings/phy/phy.h>
+    dp_phy: phy@32c00000 {
+        compatible = "fsl,imx8mq-hdptx-phy";
+        reg = <0x32c00000 0x100000>;
+        #phy-cells = <0>;
+        clocks = <&hdmi_phy_27m>, <&clk IMX8MQ_CLK_DISP_APB_ROOT>;
+        clock-names = "ref", "apb";
+    };

From patchwork Tue Dec 17 06:51:49 2024
Content-Type: text/plain; charset="utf-8"
MIME-Version: 1.0
Content-Transfer-Encoding: 7bit
Subject: [v20,7/9] phy: freescale: Add DisplayPort/HDMI Combo-PHY driver for
 i.MX8MQ
From: Sandor Yu <Sandor.yu@nxp.com>
X-Patchwork-Id: 629294
Message-Id: 
 <f85a57a2657ffe0e7334b7a7982ebcb3c4889eec.1734340233.git.Sandor.yu@nxp.com>
To: dmitry.baryshkov@linaro.org, andrzej.hajda@intel.com,
 neil.armstrong@linaro.org, Laurent.pinchart@ideasonboard.com,
 jonas@kwiboo.se, jernej.skrabec@gmail.com, airlied@gmail.com,
 daniel@ffwll.ch, robh+dt@kernel.org, krzysztof.kozlowski+dt@linaro.org,
 shawnguo@kernel.org, s.hauer@pengutronix.de, festevam@gmail.com,
 vkoul@kernel.org, dri-devel@lists.freedesktop.org,
 devicetree@vger.kernel.org, linux-arm-kernel@lists.infradead.org,
 linux-kernel@vger.kernel.org, linux-phy@lists.infradead.org,
 mripard@kernel.org
Cc: kernel@pengutronix.de, linux-imx@nxp.com, Sandor.yu@nxp.com,
 oliver.brown@nxp.com, alexander.stein@ew.tq-group.com, sam@ravnborg.org
Date: Tue, 17 Dec 2024 14:51:49 +0800

Add Cadence HDP-TX DisplayPort and HDMI PHY driver for i.MX8MQ.

Cadence HDP-TX PHY could be put in either DP mode or
HDMI mode base on the configuration chosen.
DisplayPort or HDMI PHY mode is configured in the driver.

Signed-off-by: Sandor Yu <Sandor.yu@nxp.com>
Signed-off-by: Alexander Stein <alexander.stein@ew.tq-group.com>
---
v19->v20:
- implify DP configuration handling by directly copying
  the configuration options to the driver's internal structure.
- return the error code directly instead of logging an error message in `hdptx_clk_enable`
- Remove redundant ref_clk_rate check

v18->v19:
- Simplify the PLL tables by removing unused and constant data
- Remove PHY power management, controller driver will handle them.
- Remove enum dp_link_rate
- Introduce read_pll_timeout.
- Update clock management as devm_clk_get_enabled() introduced.
- Remove cdns_hdptx_phy_init() and cdns_hdptx_phy_remove().

v17->v18:
- fix build error as code rebase to latest kernel version.

 drivers/phy/freescale/Kconfig                |   10 +
 drivers/phy/freescale/Makefile               |    1 +
 drivers/phy/freescale/phy-fsl-imx8mq-hdptx.c | 1231 ++++++++++++++++++
 3 files changed, 1242 insertions(+)
 create mode 100644 drivers/phy/freescale/phy-fsl-imx8mq-hdptx.c

diff --git a/drivers/phy/freescale/Kconfig b/drivers/phy/freescale/Kconfig
index dcd9acff6d01a..2b1210367b31c 100644
--- a/drivers/phy/freescale/Kconfig
+++ b/drivers/phy/freescale/Kconfig
@@ -35,6 +35,16 @@ config PHY_FSL_IMX8M_PCIE
 	  Enable this to add support for the PCIE PHY as found on
 	  i.MX8M family of SOCs.
 
+config PHY_FSL_IMX8MQ_HDPTX
+	tristate "Freescale i.MX8MQ DP/HDMI PHY support"
+	depends on OF && HAS_IOMEM
+	depends on COMMON_CLK
+	select GENERIC_PHY
+	select CDNS_MHDP_HELPER
+	help
+	  Enable this to support the Cadence HDPTX DP/HDMI PHY driver
+	  on i.MX8MQ SOC.
+
 config PHY_FSL_IMX8QM_HSIO
 	tristate "Freescale i.MX8QM HSIO PHY"
 	depends on OF && HAS_IOMEM
diff --git a/drivers/phy/freescale/Makefile b/drivers/phy/freescale/Makefile
index 658eac7d0a622..a946b87905498 100644
--- a/drivers/phy/freescale/Makefile
+++ b/drivers/phy/freescale/Makefile
@@ -1,4 +1,5 @@
 # SPDX-License-Identifier: GPL-2.0-only
+obj-$(CONFIG_PHY_FSL_IMX8MQ_HDPTX)	+= phy-fsl-imx8mq-hdptx.o
 obj-$(CONFIG_PHY_FSL_IMX8MQ_USB)	+= phy-fsl-imx8mq-usb.o
 obj-$(CONFIG_PHY_MIXEL_LVDS_PHY)	+= phy-fsl-imx8qm-lvds-phy.o
 obj-$(CONFIG_PHY_MIXEL_MIPI_DPHY)	+= phy-fsl-imx8-mipi-dphy.o
diff --git a/drivers/phy/freescale/phy-fsl-imx8mq-hdptx.c b/drivers/phy/freescale/phy-fsl-imx8mq-hdptx.c
new file mode 100644
index 0000000000000..230b7148639b2
--- /dev/null
+++ b/drivers/phy/freescale/phy-fsl-imx8mq-hdptx.c
@@ -0,0 +1,1231 @@
+// SPDX-License-Identifier: GPL-2.0-only
+/*
+ * Cadence DP/HDMI PHY driver
+ *
+ * Copyright (C) 2022-2024 NXP Semiconductor, Inc.
+ */
+#include <linux/clk.h>
+#include <linux/kernel.h>
+#include <linux/phy/phy.h>
+#include <linux/platform_device.h>
+#include <linux/io.h>
+#include <linux/unaligned.h>
+#include <soc/cadence/cdns-mhdp-helper.h>
+
+#define ADDR_PHY_AFE	0x80000
+
+/* PHY registers */
+#define CMN_SSM_BIAS_TMR			0x0022
+#define CMN_PLLSM0_PLLEN_TMR			0x0029
+#define CMN_PLLSM0_PLLPRE_TMR			0x002a
+#define CMN_PLLSM0_PLLVREF_TMR			0x002b
+#define CMN_PLLSM0_PLLLOCK_TMR			0x002c
+#define CMN_PLLSM0_USER_DEF_CTRL		0x002f
+#define CMN_PSM_CLK_CTRL			0x0061
+#define CMN_CDIAG_REFCLK_CTRL			0x0062
+#define CMN_PLL0_VCOCAL_START			0x0081
+#define CMN_PLL0_VCOCAL_INIT_TMR		0x0084
+#define CMN_PLL0_VCOCAL_ITER_TMR		0x0085
+#define CMN_PLL0_INTDIV				0x0094
+#define CMN_PLL0_FRACDIV			0x0095
+#define CMN_PLL0_HIGH_THR			0x0096
+#define CMN_PLL0_DSM_DIAG			0x0097
+#define CMN_PLL0_SS_CTRL2			0x0099
+#define CMN_ICAL_INIT_TMR			0x00c4
+#define CMN_ICAL_ITER_TMR			0x00c5
+#define CMN_RXCAL_INIT_TMR			0x00d4
+#define CMN_RXCAL_ITER_TMR			0x00d5
+#define CMN_TXPUCAL_CTRL			0x00e0
+#define CMN_TXPUCAL_INIT_TMR			0x00e4
+#define CMN_TXPUCAL_ITER_TMR			0x00e5
+#define CMN_TXPDCAL_CTRL			0x00f0
+#define CMN_TXPDCAL_INIT_TMR			0x00f4
+#define CMN_TXPDCAL_ITER_TMR			0x00f5
+#define CMN_ICAL_ADJ_INIT_TMR			0x0102
+#define CMN_ICAL_ADJ_ITER_TMR			0x0103
+#define CMN_RX_ADJ_INIT_TMR			0x0106
+#define CMN_RX_ADJ_ITER_TMR			0x0107
+#define CMN_TXPU_ADJ_CTRL			0x0108
+#define CMN_TXPU_ADJ_INIT_TMR			0x010a
+#define CMN_TXPU_ADJ_ITER_TMR			0x010b
+#define CMN_TXPD_ADJ_CTRL			0x010c
+#define CMN_TXPD_ADJ_INIT_TMR			0x010e
+#define CMN_TXPD_ADJ_ITER_TMR			0x010f
+#define CMN_DIAG_PLL0_FBH_OVRD			0x01c0
+#define CMN_DIAG_PLL0_FBL_OVRD			0x01c1
+#define CMN_DIAG_PLL0_OVRD			0x01c2
+#define CMN_DIAG_PLL0_TEST_MODE			0x01c4
+#define CMN_DIAG_PLL0_V2I_TUNE			0x01c5
+#define CMN_DIAG_PLL0_CP_TUNE			0x01c6
+#define CMN_DIAG_PLL0_LF_PROG			0x01c7
+#define CMN_DIAG_PLL0_PTATIS_TUNE1		0x01c8
+#define CMN_DIAG_PLL0_PTATIS_TUNE2		0x01c9
+#define CMN_DIAG_PLL0_INCLK_CTRL		0x01ca
+#define CMN_DIAG_PLL0_PXL_DIVH			0x01cb
+#define CMN_DIAG_PLL0_PXL_DIVL			0x01cc
+#define CMN_DIAG_HSCLK_SEL			0x01e0
+#define CMN_DIAG_PER_CAL_ADJ			0x01ec
+#define CMN_DIAG_CAL_CTRL			0x01ed
+#define CMN_DIAG_ACYA				0x01ff
+#define XCVR_PSM_RCTRL				0x4001
+#define XCVR_PSM_CAL_TMR			0x4002
+#define XCVR_PSM_A0IN_TMR			0x4003
+#define TX_TXCC_CAL_SCLR_MULT_0			0x4047
+#define TX_TXCC_CPOST_MULT_00_0			0x404c
+#define XCVR_DIAG_PLLDRC_CTRL			0x40e0
+#define XCVR_DIAG_HSCLK_SEL			0x40e1
+#define XCVR_DIAG_BIDI_CTRL			0x40e8
+#define XCVR_DIAG_LANE_FCM_EN_MGN_TMR		0x40f2
+#define TX_PSC_A0				0x4100
+#define TX_PSC_A1				0x4101
+#define TX_PSC_A2				0x4102
+#define TX_PSC_A3				0x4103
+#define TX_RCVDET_EN_TMR			0x4122
+#define TX_RCVDET_ST_TMR			0x4123
+#define TX_DIAG_TX_CTRL				0x41e0
+#define TX_DIAG_TX_DRV				0x41e1
+#define TX_DIAG_BGREF_PREDRV_DELAY		0x41e7
+#define TX_DIAG_ACYA_0				0x41ff
+#define TX_DIAG_ACYA_1				0x43ff
+#define TX_DIAG_ACYA_2				0x45ff
+#define TX_DIAG_ACYA_3				0x47ff
+#define TX_ANA_CTRL_REG_1			0x5020
+#define TX_ANA_CTRL_REG_2			0x5021
+#define TX_DIG_CTRL_REG_1			0x5023
+#define TX_DIG_CTRL_REG_2			0x5024
+#define TXDA_CYA_AUXDA_CYA			0x5025
+#define TX_ANA_CTRL_REG_3			0x5026
+#define TX_ANA_CTRL_REG_4			0x5027
+#define TX_ANA_CTRL_REG_5			0x5029
+#define RX_PSC_A0				0x8000
+#define RX_PSC_CAL				0x8006
+#define PHY_HDP_MODE_CTRL			0xc008
+#define PHY_HDP_CLK_CTL				0xc009
+#define PHY_ISO_CMN_CTRL			0xc010
+#define PHY_PMA_CMN_CTRL1			0xc800
+#define PHY_PMA_ISO_CMN_CTRL			0xc810
+#define PHY_PMA_ISO_PLL_CTRL1			0xc812
+#define PHY_PMA_ISOLATION_CTRL			0xc81f
+
+/* PHY_HDP_CLK_CTL */
+#define PLL_DATA_RATE_CLK_DIV_MASK		GENMASK(15, 8)
+#define PLL_DATA_RATE_CLK_DIV_HBR		0x24
+#define PLL_DATA_RATE_CLK_DIV_HBR2		0x12
+#define PLL_CLK_EN_ACK				BIT(3)
+#define PLL_CLK_EN				BIT(2)
+#define PLL_READY				BIT(1)
+#define PLL_EN					BIT(0)
+
+/* PHY_PMA_CMN_CTRL1 */
+#define CMA_REF_CLK_DIG_DIV_MASK		GENMASK(13, 12)
+#define CMA_REF_CLK_SEL_MASK			GENMASK(6, 4)
+#define CMA_REF_CLK_RCV_EN_MASK			BIT(3)
+#define CMA_REF_CLK_RCV_EN			1
+#define CMN_READY				BIT(0)
+
+/* PHY_PMA_ISO_PLL_CTRL1 */
+#define CMN_PLL0_CLK_DATART_DIV_MASK		GENMASK(7, 0)
+
+/* TX_DIAG_TX_DRV */
+#define TX_DRIVER_PROG_BOOST_ENABLE		BIT(10)
+#define TX_DRIVER_PROG_BOOST_LEVEL_MASK		GENMASK(9, 8)
+#define TX_DRIVER_LDO_BG_DEPENDENT_REF_ENABLE	BIT(7)
+#define TX_DRIVER_LDO_BANDGAP_REF_ENABLE	BIT(6)
+
+/* TX_TXCC_CAL_SCLR_MULT_0 */
+#define SCALED_RESISTOR_CALIBRATION_CODE_ADD	BIT(8)
+#define RESISTOR_CAL_MULT_VAL_32_128		BIT(5)
+
+/* CMN_CDIAG_REFCLK_CTRL */
+#define DIG_REF_CLK_DIV_SCALER_MASK		GENMASK(14, 12)
+#define REFCLK_TERMINATION_EN_OVERRIDE_EN	BIT(7)
+#define REFCLK_TERMINATION_EN_OVERRIDE		BIT(6)
+
+/* CMN_DIAG_HSCLK_SEL */
+#define HSCLK1_SEL_MASK				GENMASK(5, 4)
+#define HSCLK0_SEL_MASK				GENMASK(1, 0)
+#define HSCLK_PLL0_DIV2				1
+
+/* XCVR_DIAG_HSCLK_SEL */
+#define HSCLK_SEL_MODE3_MASK			GENMASK(13, 12)
+#define HSCLK_SEL_MODE3_HSCLK1			1
+
+/* CMN_PLL0_VCOCAL_START */
+#define VCO_CALIB_CODE_START_POINT_VAL_MASK	GENMASK(8, 0)
+
+/* CMN_DIAG_PLL0_FBH_OVRD */
+#define PLL_FEEDBACK_DIV_HI_OVERRIDE_EN		BIT(15)
+
+/* CMN_DIAG_PLL0_FBL_OVRD */
+#define PLL_FEEDBACK_DIV_LO_OVERRIDE_EN		BIT(15)
+
+/* CMN_DIAG_PLL0_PXL_DIVH */
+#define PLL_PCLK_DIV_EN				BIT(15)
+
+/* XCVR_DIAG_PLLDRC_CTRL */
+#define DPLL_CLK_SEL_MODE3			BIT(14)
+#define DPLL_DATA_RATE_DIV_MODE3_MASK		GENMASK(13, 12)
+
+/* TX_DIAG_TX_CTRL */
+#define TX_IF_SUBRATE_MODE3_MASK		GENMASK(7, 6)
+
+/* PHY_HDP_MODE_CTRL */
+#define POWER_STATE_A3_ACK			BIT(7)
+#define POWER_STATE_A2_ACK			BIT(6)
+#define POWER_STATE_A1_ACK			BIT(5)
+#define POWER_STATE_A0_ACK			BIT(4)
+#define POWER_STATE_A3				BIT(3)
+#define POWER_STATE_A2				BIT(2)
+#define POWER_STATE_A1				BIT(1)
+#define POWER_STATE_A0				BIT(0)
+
+/* PHY_PMA_ISO_CMN_CTRL */
+#define CMN_MACRO_PWR_EN_ACK			BIT(5)
+
+#define KEEP_ALIVE		0x18
+
+/* FW check alive timeout */
+#define CDNS_KEEP_ALIVE_TIMEOUT		2000
+#define CDNS_KEEP_ALIVE_MASK		GENMASK(7, 0)
+
+#define REF_CLK_27MHZ		27000000
+
+#define LINK_RATE_2_7	270000
+#define MAX_LINK_RATE	540000
+
+#define CMN_REF_CLK_DIG_DIV	1
+#define REF_CLK_DIVIDER_SCALER	1
+
+/* HDMI TX clock control settings */
+struct hdptx_hdmi_ctrl {
+	u32 pixel_clk_freq;
+	u32 feedback_factor;
+	u32 cmnda_pll0_ip_div;
+	u32 pll_fb_div_total;
+	u32 cmnda_pll0_fb_div_low;
+	u32 cmnda_pll0_fb_div_high;
+	u32 cmnda_pll0_pxdiv_low;
+	u32 cmnda_pll0_pxdiv_high;
+	u32 vco_ring_select;
+	u32 cmnda_hs_clk_0_sel;
+	u32 cmnda_hs_clk_1_sel;
+	u32 hsclk_div_tx_sub_rate;
+	u32 cmnda_pll0_hs_sym_div_sel;
+};
+
+struct cdns_hdptx_phy {
+	struct cdns_mhdp_base base;
+
+	void __iomem *regs;	/* DPTX registers base */
+	struct device *dev;
+	struct phy *phy;
+	struct clk *ref_clk, *apb_clk;
+	u32 ref_clk_rate;
+	union {
+		struct phy_configure_opts_hdmi hdmi;
+		struct phy_configure_opts_dp dp;
+	};
+};
+
+/* HDMI TX clock control settings, pixel clock is output */
+static const struct hdptx_hdmi_ctrl pixel_clk_output_ctrl_table[] = {
+	/*  clk   fbak ipd totl div_l  div_h pd_l  pd_h  v h1 h2 sub sym*/
+	{  27000, 1000, 3, 240, 0x0bc, 0x30, 0x26, 0x26, 0, 2, 2, 4, 3 },
+	{  27000, 1250, 3, 300, 0x0ec, 0x3c, 0x30, 0x30, 0, 2, 2, 4, 3 },
+	{  27000, 1500, 3, 360, 0x11c, 0x48, 0x3a, 0x3a, 0, 2, 2, 4, 3 },
+	{  27000, 2000, 3, 240, 0x0bc, 0x30, 0x26, 0x26, 0, 2, 2, 4, 2 },
+	{  54000, 1000, 3, 480, 0x17c, 0x60, 0x26, 0x26, 1, 2, 2, 4, 3 },
+	{  54000, 1250, 4, 400, 0x13c, 0x50, 0x17, 0x17, 0, 1, 1, 4, 2 },
+	{  54000, 1500, 4, 480, 0x17c, 0x60, 0x1c, 0x1c, 0, 2, 2, 2, 2 },
+	{  54000, 2000, 3, 240, 0x0bc, 0x30, 0x12, 0x12, 0, 2, 2, 1, 1 },
+	{  74250, 1000, 3, 660, 0x20c, 0x84, 0x26, 0x26, 1, 2, 2, 4, 3 },
+	{  74250, 1250, 4, 550, 0x1b4, 0x6e, 0x17, 0x17, 1, 1, 1, 4, 2 },
+	{  74250, 1500, 4, 660, 0x20c, 0x84, 0x1c, 0x1c, 1, 2, 2, 2, 2 },
+	{  74250, 2000, 3, 330, 0x104, 0x42, 0x12, 0x12, 0, 2, 2, 1, 1 },
+	{  99000, 1000, 3, 440, 0x15c, 0x58, 0x12, 0x12, 1, 2, 2, 2, 2 },
+	{  99000, 1250, 3, 275, 0x0d8, 0x37, 0x0b, 0x0a, 0, 1, 1, 2, 1 },
+	{  99000, 1500, 3, 330, 0x104, 0x42, 0x0d, 0x0d, 0, 2, 2, 1, 1 },
+	{  99000, 2000, 3, 440, 0x15c, 0x58, 0x12, 0x12, 1, 2, 2, 1, 1 },
+	{ 148500, 1000, 3, 660, 0x20c, 0x84, 0x12, 0x12, 1, 2, 2, 2, 2 },
+	{ 148500, 1250, 4, 550, 0x1b4, 0x6e, 0x0b, 0x0a, 1, 1, 1, 2, 1 },
+	{ 148500, 1500, 3, 495, 0x188, 0x63, 0x0d, 0x0d, 1, 1, 1, 2, 1 },
+	{ 148500, 2000, 3, 660, 0x20c, 0x84, 0x12, 0x12, 1, 2, 2, 1, 1 },
+	{ 198000, 1000, 3, 220, 0x0ac, 0x2c, 0x03, 0x03, 0, 1, 1, 1, 0 },
+	{ 198000, 1250, 3, 550, 0x1b4, 0x6e, 0x0b, 0x0a, 1, 1, 1, 2, 1 },
+	{ 198000, 1500, 3, 330, 0x104, 0x42, 0x06, 0x05, 0, 1, 1, 1, 0 },
+	{ 198000, 2000, 3, 440, 0x15c, 0x58, 0x08, 0x08, 1, 1, 1, 1, 0 },
+	{ 297000, 1000, 3, 330, 0x104, 0x42, 0x03, 0x03, 0, 1, 1, 1, 0 },
+	{ 297000, 1500, 3, 495, 0x188, 0x63, 0x06, 0x05, 1, 1, 1, 1, 0 },
+	{ 297000, 2000, 3, 660, 0x20c, 0x84, 0x08, 0x08, 1, 1, 1, 1, 0 },
+	{ 594000, 1000, 3, 660, 0x20c, 0x84, 0x03, 0x03, 1, 1, 1, 1, 0 },
+	{ 594000,  750, 3, 495, 0x188, 0x63, 0x03, 0x03, 1, 1, 1, 1, 0 },
+	{ 594000,  625, 4, 550, 0x1b4, 0x6e, 0x03, 0x03, 1, 1, 1, 1, 0 },
+	{ 594000,  500, 3, 660, 0x20c, 0x84, 0x03, 0x03, 1, 1, 1, 2, 1 },
+};
+
+/* HDMI TX PLL tuning settings */
+struct hdptx_hdmi_pll_tuning {
+	u32 vco_freq;
+	u32 volt_to_current_coarse;
+	u32 volt_to_current;
+	u32 ndac_ctrl;
+	u32 pmos_ctrl;
+	u32 ptat_ndac_ctrl;
+	u32 feedback_div_total;
+	u32 charge_pump_gain;
+	u32 vco_cal_code;
+};
+
+/* HDMI TX PLL tuning settings, pixel clock is output */
+static const struct hdptx_hdmi_pll_tuning pixel_clk_output_pll_table[] = {
+	/*VCO_f  coar cu nd pm ptat fd_d gain  cal */
+	{ 1980000, 4, 3, 0, 9, 0x9, 220, 0x42, 183 },
+	{ 2160000, 4, 3, 0, 9, 0x9, 240, 0x42, 208 },
+	{ 2475000, 5, 3, 1, 0, 0x7, 275, 0x42, 209 },
+	{ 2700000, 5, 3, 1, 0, 0x7, 300, 0x42, 230 },
+	{ 2700000, 5, 3, 1, 0, 0x7, 400, 0x4c, 230 },
+	{ 2970000, 6, 3, 1, 0, 0x7, 330, 0x42, 225 },
+	{ 3240000, 6, 3, 1, 0, 0x7, 360, 0x42, 256 },
+	{ 3240000, 6, 3, 1, 0, 0x7, 480, 0x4c, 256 },
+	{ 3712500, 4, 3, 0, 7, 0xF, 550, 0x4c, 257 },
+	{ 3960000, 5, 3, 0, 7, 0xF, 440, 0x42, 226 },
+	{ 4320000, 5, 3, 1, 7, 0xF, 480, 0x42, 258 },
+	{ 4455000, 5, 3, 0, 7, 0xF, 495, 0x42, 272 },
+	{ 4455000, 5, 3, 0, 7, 0xF, 660, 0x4c, 272 },
+	{ 4950000, 6, 3, 1, 0, 0x7, 550, 0x42, 258 },
+	{ 5940000, 7, 3, 1, 0, 0x7, 660, 0x42, 292 },
+};
+
+struct phy_pll_reg {
+	u16 val[7];
+	u32 addr;
+};
+
+static const struct phy_pll_reg phy_pll_27m_cfg[] = {
+	/*  1.62    2.16    2.43    2.7     3.24    4.32    5.4      register address */
+	{{ 0x010e, 0x010e, 0x010e, 0x010e, 0x010e, 0x010e, 0x010e }, CMN_PLL0_VCOCAL_INIT_TMR },
+	{{ 0x001b, 0x001b, 0x001b, 0x001b, 0x001b, 0x001b, 0x001b }, CMN_PLL0_VCOCAL_ITER_TMR },
+	{{ 0x30b9, 0x3087, 0x3096, 0x30b4, 0x30b9, 0x3087, 0x30b4 }, CMN_PLL0_VCOCAL_START },
+	{{ 0x0077, 0x009f, 0x00b3, 0x00c7, 0x0077, 0x009f, 0x00c7 }, CMN_PLL0_INTDIV },
+	{{ 0xf9da, 0xf7cd, 0xf6c7, 0xf5c1, 0xf9da, 0xf7cd, 0xf5c1 }, CMN_PLL0_FRACDIV },
+	{{ 0x001e, 0x0028, 0x002d, 0x0032, 0x001e, 0x0028, 0x0032 }, CMN_PLL0_HIGH_THR },
+	{{ 0x0020, 0x0020, 0x0020, 0x0020, 0x0020, 0x0020, 0x0020 }, CMN_PLL0_DSM_DIAG },
+	{{ 0x0000, 0x1000, 0x1000, 0x1000, 0x0000, 0x1000, 0x1000 }, CMN_PLLSM0_USER_DEF_CTRL },
+	{{ 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000 }, CMN_DIAG_PLL0_OVRD },
+	{{ 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000 }, CMN_DIAG_PLL0_FBH_OVRD },
+	{{ 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000, 0x0000 }, CMN_DIAG_PLL0_FBL_OVRD },
+	{{ 0x0006, 0x0007, 0x0007, 0x0007, 0x0006, 0x0007, 0x0007 }, CMN_DIAG_PLL0_V2I_TUNE },
+	{{ 0x0043, 0x0043, 0x0043, 0x0042, 0x0043, 0x0043, 0x0042 }, CMN_DIAG_PLL0_CP_TUNE },
+	{{ 0x0008, 0x0008, 0x0008, 0x0008, 0x0008, 0x0008, 0x0008 }, CMN_DIAG_PLL0_LF_PROG },
+	{{ 0x0100, 0x0001, 0x0001, 0x0001, 0x0100, 0x0001, 0x0001 }, CMN_DIAG_PLL0_PTATIS_TUNE1 },
+	{{ 0x0007, 0x0001, 0x0001, 0x0001, 0x0007, 0x0001, 0x0001 }, CMN_DIAG_PLL0_PTATIS_TUNE2 },
+	{{ 0x0020, 0x0020, 0x0020, 0x0020, 0x0020, 0x0020, 0x0020 }, CMN_DIAG_PLL0_TEST_MODE},
+	{{ 0x0016, 0x0016, 0x0016, 0x0016, 0x0016, 0x0016, 0x0016 }, CMN_PSM_CLK_CTRL }
+};
+
+static int dp_link_rate_index(u32 rate)
+{
+	switch (rate) {
+	case 162000:
+		return 0;
+	case 216000:
+		return 1;
+	case 243000:
+		return 2;
+	case 270000:
+		return 3;
+	case 324000:
+		return 4;
+	case 432000:
+		return 5;
+	case 540000:
+		return 6;
+	default:
+		return -EINVAL;
+	}
+}
+
+static int cdns_phy_reg_write(struct cdns_hdptx_phy *cdns_phy, u32 addr, u32 val)
+{
+	return cdns_mhdp_reg_write(&cdns_phy->base, ADDR_PHY_AFE + (addr << 2), val);
+}
+
+static u32 cdns_phy_reg_read(struct cdns_hdptx_phy *cdns_phy, u32 addr)
+{
+	u32 reg32;
+
+	cdns_mhdp_reg_read(&cdns_phy->base, ADDR_PHY_AFE + (addr << 2), &reg32);
+
+	return reg32;
+}
+
+static void hdptx_dp_aux_cfg(struct cdns_hdptx_phy *cdns_phy)
+{
+	/* Power up Aux */
+	cdns_phy_reg_write(cdns_phy, TXDA_CYA_AUXDA_CYA, 1);
+
+	cdns_phy_reg_write(cdns_phy, TX_DIG_CTRL_REG_1, 0x3);
+	ndelay(150);
+	cdns_phy_reg_write(cdns_phy, TX_DIG_CTRL_REG_2, 36);
+	ndelay(150);
+	cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_2, 0x0100);
+	ndelay(150);
+	cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_2, 0x0300);
+	ndelay(150);
+	cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_3, 0x0000);
+	ndelay(150);
+	cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_1, 0x2008);
+	ndelay(150);
+	cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_1, 0x2018);
+	ndelay(150);
+	cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_1, 0xa018);
+	ndelay(150);
+	cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_2, 0x030c);
+	ndelay(150);
+	cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_5, 0x0000);
+	ndelay(150);
+	cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_4, 0x1001);
+	ndelay(150);
+	cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_1, 0xa098);
+	ndelay(150);
+	cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_1, 0xa198);
+	ndelay(150);
+	cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_2, 0x030d);
+	ndelay(150);
+	cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_2, 0x030f);
+}
+
+/* PMA common configuration for 27MHz */
+static void hdptx_dp_phy_pma_cmn_cfg_27mhz(struct cdns_hdptx_phy *cdns_phy)
+{
+	u32 num_lanes = cdns_phy->dp.lanes;
+	u16 val;
+	int k;
+
+	/* Enable PMA input ref clk(CMN_REF_CLK_RCV_EN) */
+	val = cdns_phy_reg_read(cdns_phy, PHY_PMA_CMN_CTRL1);
+	val &= ~CMA_REF_CLK_RCV_EN_MASK;
+	val |= FIELD_PREP(CMA_REF_CLK_RCV_EN_MASK, CMA_REF_CLK_RCV_EN);
+	cdns_phy_reg_write(cdns_phy, PHY_PMA_CMN_CTRL1, val);
+
+	/* Startup state machine registers */
+	cdns_phy_reg_write(cdns_phy, CMN_SSM_BIAS_TMR, 0x0087);
+	cdns_phy_reg_write(cdns_phy, CMN_PLLSM0_PLLEN_TMR, 0x001b);
+	cdns_phy_reg_write(cdns_phy, CMN_PLLSM0_PLLPRE_TMR, 0x0036);
+	cdns_phy_reg_write(cdns_phy, CMN_PLLSM0_PLLVREF_TMR, 0x001b);
+	cdns_phy_reg_write(cdns_phy, CMN_PLLSM0_PLLLOCK_TMR, 0x006c);
+
+	/* Current calibration registers */
+	cdns_phy_reg_write(cdns_phy, CMN_ICAL_INIT_TMR, 0x0044);
+	cdns_phy_reg_write(cdns_phy, CMN_ICAL_ITER_TMR, 0x0006);
+	cdns_phy_reg_write(cdns_phy, CMN_ICAL_ADJ_INIT_TMR, 0x0022);
+	cdns_phy_reg_write(cdns_phy, CMN_ICAL_ADJ_ITER_TMR, 0x0006);
+
+	/* Resistor calibration registers */
+	cdns_phy_reg_write(cdns_phy, CMN_TXPUCAL_INIT_TMR, 0x0022);
+	cdns_phy_reg_write(cdns_phy, CMN_TXPUCAL_ITER_TMR, 0x0006);
+	cdns_phy_reg_write(cdns_phy, CMN_TXPU_ADJ_INIT_TMR, 0x0022);
+	cdns_phy_reg_write(cdns_phy, CMN_TXPU_ADJ_ITER_TMR, 0x0006);
+	cdns_phy_reg_write(cdns_phy, CMN_TXPDCAL_INIT_TMR, 0x0022);
+	cdns_phy_reg_write(cdns_phy, CMN_TXPDCAL_ITER_TMR, 0x0006);
+	cdns_phy_reg_write(cdns_phy, CMN_TXPD_ADJ_INIT_TMR, 0x0022);
+	cdns_phy_reg_write(cdns_phy, CMN_TXPD_ADJ_ITER_TMR, 0x0006);
+	cdns_phy_reg_write(cdns_phy, CMN_RXCAL_INIT_TMR, 0x0022);
+	cdns_phy_reg_write(cdns_phy, CMN_RXCAL_ITER_TMR, 0x0006);
+	cdns_phy_reg_write(cdns_phy, CMN_RX_ADJ_INIT_TMR, 0x0022);
+	cdns_phy_reg_write(cdns_phy, CMN_RX_ADJ_ITER_TMR, 0x0006);
+
+	for (k = 0; k < num_lanes; k = k + 1) {
+		/* Power state machine registers */
+		cdns_phy_reg_write(cdns_phy, XCVR_PSM_CAL_TMR  | (k << 9), 0x016d);
+		cdns_phy_reg_write(cdns_phy, XCVR_PSM_A0IN_TMR | (k << 9), 0x016d);
+		/* Transceiver control and diagnostic registers */
+		cdns_phy_reg_write(cdns_phy, XCVR_DIAG_LANE_FCM_EN_MGN_TMR | (k << 9), 0x00a2);
+		cdns_phy_reg_write(cdns_phy, TX_DIAG_BGREF_PREDRV_DELAY | (k << 9), 0x0097);
+		/* Transmitter receiver detect registers */
+		cdns_phy_reg_write(cdns_phy, TX_RCVDET_EN_TMR | (k << 9), 0x0a8c);
+		cdns_phy_reg_write(cdns_phy, TX_RCVDET_ST_TMR | (k << 9), 0x0036);
+	}
+
+	cdns_phy_reg_write(cdns_phy, TX_DIAG_ACYA_0, 1);
+	cdns_phy_reg_write(cdns_phy, TX_DIAG_ACYA_1, 1);
+	cdns_phy_reg_write(cdns_phy, TX_DIAG_ACYA_2, 1);
+	cdns_phy_reg_write(cdns_phy, TX_DIAG_ACYA_3, 1);
+}
+
+static void hdptx_dp_phy_pma_cmn_pll0_27mhz(struct cdns_hdptx_phy *cdns_phy)
+{
+	u32 num_lanes = cdns_phy->dp.lanes;
+	u32 link_rate = cdns_phy->dp.link_rate;
+	u16 val;
+	int index, i, k;
+
+	/* DP PLL data rate 0/1 clock divider value */
+	val = cdns_phy_reg_read(cdns_phy, PHY_HDP_CLK_CTL);
+	val &= ~PLL_DATA_RATE_CLK_DIV_MASK;
+	if (link_rate <= LINK_RATE_2_7)
+		val |= FIELD_PREP(PLL_DATA_RATE_CLK_DIV_MASK,
+				  PLL_DATA_RATE_CLK_DIV_HBR);
+	else
+		val |= FIELD_PREP(PLL_DATA_RATE_CLK_DIV_MASK,
+				  PLL_DATA_RATE_CLK_DIV_HBR2);
+	cdns_phy_reg_write(cdns_phy, PHY_HDP_CLK_CTL, val);
+
+	/* High speed clock 0/1 div */
+	val = cdns_phy_reg_read(cdns_phy, CMN_DIAG_HSCLK_SEL);
+	val &= ~(HSCLK1_SEL_MASK | HSCLK0_SEL_MASK);
+	if (link_rate <= LINK_RATE_2_7) {
+		val |= FIELD_PREP(HSCLK1_SEL_MASK, HSCLK_PLL0_DIV2);
+		val |= FIELD_PREP(HSCLK0_SEL_MASK, HSCLK_PLL0_DIV2);
+	}
+	cdns_phy_reg_write(cdns_phy, CMN_DIAG_HSCLK_SEL, val);
+
+	for (k = 0; k < num_lanes; k++) {
+		val = cdns_phy_reg_read(cdns_phy, (XCVR_DIAG_HSCLK_SEL | (k << 9)));
+		val &= ~HSCLK_SEL_MODE3_MASK;
+		if (link_rate <= LINK_RATE_2_7)
+			val |= FIELD_PREP(HSCLK_SEL_MODE3_MASK, HSCLK_SEL_MODE3_HSCLK1);
+		cdns_phy_reg_write(cdns_phy, (XCVR_DIAG_HSCLK_SEL | (k << 9)), val);
+	}
+
+	/* DP PHY PLL 27MHz configuration */
+	index = dp_link_rate_index(link_rate);
+	if (index < 0) {
+		dev_err(cdns_phy->dev, "Not support link rate %d\n", link_rate);
+		return;
+	}
+
+	for (i = 0; i < ARRAY_SIZE(phy_pll_27m_cfg); i++)
+		cdns_phy_reg_write(cdns_phy, phy_pll_27m_cfg[i].addr,
+				   phy_pll_27m_cfg[i].val[index]);
+
+	/* Transceiver control and diagnostic registers */
+	for (k = 0; k < num_lanes; k++) {
+		val = cdns_phy_reg_read(cdns_phy, (XCVR_DIAG_PLLDRC_CTRL | (k << 9)));
+		val &= ~(DPLL_DATA_RATE_DIV_MODE3_MASK | DPLL_CLK_SEL_MODE3);
+		if (link_rate <= LINK_RATE_2_7)
+			val |= FIELD_PREP(DPLL_DATA_RATE_DIV_MODE3_MASK, 2);
+		else
+			val |= FIELD_PREP(DPLL_DATA_RATE_DIV_MODE3_MASK, 1);
+		cdns_phy_reg_write(cdns_phy, (XCVR_DIAG_PLLDRC_CTRL | (k << 9)), val);
+	}
+
+	for (k = 0; k < num_lanes; k = k + 1) {
+		/* Power state machine registers */
+		cdns_phy_reg_write(cdns_phy, (XCVR_PSM_RCTRL | (k << 9)), 0xbefc);
+		cdns_phy_reg_write(cdns_phy, (TX_PSC_A0 | (k << 9)), 0x6799);
+		cdns_phy_reg_write(cdns_phy, (TX_PSC_A1 | (k << 9)), 0x6798);
+		cdns_phy_reg_write(cdns_phy, (TX_PSC_A2 | (k << 9)), 0x0098);
+		cdns_phy_reg_write(cdns_phy, (TX_PSC_A3 | (k << 9)), 0x0098);
+		/* Receiver calibration power state definition register */
+		val = cdns_phy_reg_read(cdns_phy, RX_PSC_CAL | (k << 9));
+		val &= 0xffbb;
+		cdns_phy_reg_write(cdns_phy, (RX_PSC_CAL | (k << 9)), val);
+		val = cdns_phy_reg_read(cdns_phy, RX_PSC_A0 | (k << 9));
+		val &= 0xffbb;
+		cdns_phy_reg_write(cdns_phy, (RX_PSC_A0 | (k << 9)), val);
+	}
+}
+
+static void hdptx_dp_phy_ref_clock_type(struct cdns_hdptx_phy *cdns_phy)
+{
+	u32 val;
+
+	val = cdns_phy_reg_read(cdns_phy, PHY_PMA_CMN_CTRL1);
+	val &= ~CMA_REF_CLK_SEL_MASK;
+	/*
+	 * single ended reference clock (val |= 0x0030);
+	 * differential clock  (val |= 0x0000);
+	 *
+	 * for differential clock on the refclk_p and
+	 * refclk_m off chip pins: CMN_DIAG_ACYA[8]=1'b1
+	 * cdns_phy_reg_write(cdns_phy, CMN_DIAG_ACYA, 0x0100);
+	 */
+	val |= FIELD_PREP(CMA_REF_CLK_SEL_MASK, 3);
+	cdns_phy_reg_write(cdns_phy, PHY_PMA_CMN_CTRL1, val);
+}
+
+static int wait_for_ack(struct cdns_hdptx_phy *cdns_phy,
+			u32 reg, u32 mask,
+			const char *err_msg)
+{
+	int ret;
+	u32 val;
+
+	ret = read_poll_timeout(cdns_phy_reg_read,
+				val, val & mask, 20, 1000,
+				false, cdns_phy, reg);
+	if (ret < 0)
+		dev_err(cdns_phy->dev, "%s\n", err_msg);
+
+	return ret;
+}
+
+static int wait_for_ack_clear(struct cdns_hdptx_phy *cdns_phy,
+			      u32 reg, u32 mask,
+			      const char *err_msg)
+{
+	int ret;
+	u32 val;
+
+	ret = read_poll_timeout(cdns_phy_reg_read,
+				val, !(val & mask), 20, 1000,
+				false, cdns_phy, reg);
+	if (ret < 0)
+		dev_err(cdns_phy->dev, "%s\n", err_msg);
+
+	return ret;
+}
+
+static int hdptx_dp_phy_power_up(struct cdns_hdptx_phy *cdns_phy)
+{
+	u32 val;
+	int ret;
+
+	/* Enable HDP PLL's for high speed clocks */
+	val = cdns_phy_reg_read(cdns_phy, PHY_HDP_CLK_CTL);
+	val |= PLL_EN;
+	cdns_phy_reg_write(cdns_phy, PHY_HDP_CLK_CTL, val);
+	ret = wait_for_ack(cdns_phy, PHY_HDP_CLK_CTL, PLL_READY,
+			   "Wait PLL Ack failed");
+	if (ret < 0)
+		return ret;
+
+	/* Enable HDP PLL's data rate and full rate clocks out of PMA. */
+	val = cdns_phy_reg_read(cdns_phy, PHY_HDP_CLK_CTL);
+	val |= PLL_CLK_EN;
+	cdns_phy_reg_write(cdns_phy, PHY_HDP_CLK_CTL, val);
+	ret = wait_for_ack(cdns_phy, PHY_HDP_CLK_CTL, PLL_CLK_EN_ACK,
+			   "Wait PLL clock enable ACK failed");
+	if (ret < 0)
+		return ret;
+
+	/* Configure PHY in A2 Mode */
+	cdns_phy_reg_write(cdns_phy, PHY_HDP_MODE_CTRL, POWER_STATE_A2);
+	ret = wait_for_ack(cdns_phy, PHY_HDP_MODE_CTRL, POWER_STATE_A2_ACK,
+			   "Wait A2 Ack failed");
+	if (ret < 0)
+		return ret;
+
+	/* Configure PHY in A0 mode (PHY must be in the A0 power
+	 * state in order to transmit data)
+	 */
+	cdns_phy_reg_write(cdns_phy, PHY_HDP_MODE_CTRL, POWER_STATE_A0);
+
+	return wait_for_ack(cdns_phy, PHY_HDP_MODE_CTRL, POWER_STATE_A0_ACK,
+			   "Wait A0 Ack failed");
+}
+
+static int hdptx_dp_phy_power_down(struct cdns_hdptx_phy *cdns_phy)
+{
+	u16 val;
+	int ret;
+
+	/* Place the PHY lanes in the A3 power state. */
+	cdns_phy_reg_write(cdns_phy, PHY_HDP_MODE_CTRL, POWER_STATE_A3);
+	ret = wait_for_ack(cdns_phy, PHY_HDP_MODE_CTRL, POWER_STATE_A3_ACK,
+			   "Wait A3 Ack failed");
+	if (ret)
+		return ret;
+
+	/* Disable HDP PLL's data rate and full rate clocks out of PMA. */
+	val = cdns_phy_reg_read(cdns_phy, PHY_HDP_CLK_CTL);
+	val &= ~PLL_CLK_EN;
+	cdns_phy_reg_write(cdns_phy, PHY_HDP_CLK_CTL, val);
+	ret = wait_for_ack_clear(cdns_phy, PHY_HDP_CLK_CTL, PLL_CLK_EN_ACK,
+				 "Wait PLL clock Ack clear failed");
+	if (ret)
+		return ret;
+
+	/* Disable HDP PLL's for high speed clocks */
+	val = cdns_phy_reg_read(cdns_phy, PHY_HDP_CLK_CTL);
+	val &= ~PLL_EN;
+	cdns_phy_reg_write(cdns_phy, PHY_HDP_CLK_CTL, val);
+
+	return  wait_for_ack_clear(cdns_phy, PHY_HDP_CLK_CTL, PLL_READY,
+				 "Wait PLL Ack clear failed");
+}
+
+static int hdptx_dp_configure(struct phy *phy,
+			      union phy_configure_opts *opts)
+{
+	const struct phy_configure_opts_dp *dp_opts = &opts->dp;
+	struct cdns_hdptx_phy *cdns_phy = phy_get_drvdata(phy);
+
+	if (opts->dp.link_rate > MAX_LINK_RATE) {
+		dev_err(cdns_phy->dev, "Link Rate(%d) Not supported\n", opts->dp.link_rate);
+		return false;
+	}
+
+	memcpy(&cdns_phy->dp, dp_opts, sizeof(*dp_opts));
+
+	hdptx_dp_phy_pma_cmn_cfg_27mhz(cdns_phy);
+	hdptx_dp_phy_pma_cmn_pll0_27mhz(cdns_phy);
+
+	return 0;
+}
+
+static int hdptx_clk_enable(struct cdns_hdptx_phy *cdns_phy)
+{
+	struct device *dev = cdns_phy->dev;
+	u32 ref_clk_rate;
+
+	cdns_phy->ref_clk =  devm_clk_get_enabled(dev, "ref");
+	if (IS_ERR(cdns_phy->ref_clk)) {
+		dev_err(dev, "phy ref clock not found\n");
+		return PTR_ERR(cdns_phy->ref_clk);
+	}
+
+	ref_clk_rate = clk_get_rate(cdns_phy->ref_clk);
+	if (!ref_clk_rate) {
+		dev_err(cdns_phy->dev, "Failed to get ref clock rate\n");
+		return -EINVAL;
+	}
+
+	if (ref_clk_rate == REF_CLK_27MHZ) {
+		cdns_phy->ref_clk_rate = ref_clk_rate;
+	} else {
+		dev_err(cdns_phy->dev, "Not support Ref Clock Rate(%dHz)\n", ref_clk_rate);
+		return -EINVAL;
+	}
+
+	cdns_phy->apb_clk =  devm_clk_get_enabled(dev, "apb");
+	if (IS_ERR(cdns_phy->apb_clk)) {
+		dev_err(dev, "phy apb clock not found\n");
+		return PTR_ERR(cdns_phy->apb_clk);
+	}
+
+	return 0;
+}
+
+static void hdptx_hdmi_arc_config(struct cdns_hdptx_phy *cdns_phy)
+{
+	u16 txpu_calib_code;
+	u16 txpd_calib_code;
+	u16 txpu_adj_calib_code;
+	u16 txpd_adj_calib_code;
+	u16 prev_calib_code;
+	u16 new_calib_code;
+	u16 rdata;
+
+	/* Power ARC */
+	cdns_phy_reg_write(cdns_phy, TXDA_CYA_AUXDA_CYA, 0x0001);
+
+	prev_calib_code = cdns_phy_reg_read(cdns_phy, TX_DIG_CTRL_REG_2);
+	txpu_calib_code = cdns_phy_reg_read(cdns_phy, CMN_TXPUCAL_CTRL);
+	txpd_calib_code = cdns_phy_reg_read(cdns_phy, CMN_TXPDCAL_CTRL);
+	txpu_adj_calib_code = cdns_phy_reg_read(cdns_phy, CMN_TXPU_ADJ_CTRL);
+	txpd_adj_calib_code = cdns_phy_reg_read(cdns_phy, CMN_TXPD_ADJ_CTRL);
+
+	new_calib_code = ((txpu_calib_code + txpd_calib_code) / 2)
+		+ txpu_adj_calib_code + txpd_adj_calib_code;
+
+	if (new_calib_code != prev_calib_code) {
+		rdata = cdns_phy_reg_read(cdns_phy, TX_ANA_CTRL_REG_1);
+		rdata &= 0xdfff;
+		cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_1, rdata);
+		cdns_phy_reg_write(cdns_phy, TX_DIG_CTRL_REG_2, new_calib_code);
+		mdelay(10);
+		rdata |= 0x2000;
+		cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_1, rdata);
+		usleep_range(150, 250);
+	}
+
+	cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_2, 0x0100);
+	usleep_range(100, 200);
+	cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_2, 0x0300);
+	usleep_range(100, 200);
+	cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_3, 0x0000);
+	usleep_range(100, 200);
+	cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_1, 0x2008);
+	usleep_range(100, 200);
+	cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_1, 0x2018);
+	usleep_range(100, 200);
+	cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_1, 0x2098);
+	cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_2, 0x030c);
+	cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_5, 0x0010);
+	usleep_range(100, 200);
+	cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_4, 0x4001);
+	mdelay(5);
+	cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_1, 0x2198);
+	mdelay(5);
+	cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_2, 0x030d);
+	usleep_range(100, 200);
+	cdns_phy_reg_write(cdns_phy, TX_ANA_CTRL_REG_2, 0x030f);
+}
+
+static void hdptx_hdmi_phy_set_vswing(struct cdns_hdptx_phy *cdns_phy)
+{
+	u32 k;
+	const u32 num_lanes = 4;
+
+	for (k = 0; k < num_lanes; k++) {
+		cdns_phy_reg_write(cdns_phy, (TX_DIAG_TX_DRV | (k << 9)),
+				   TX_DRIVER_PROG_BOOST_ENABLE |
+				   FIELD_PREP(TX_DRIVER_PROG_BOOST_LEVEL_MASK, 3) |
+				   TX_DRIVER_LDO_BG_DEPENDENT_REF_ENABLE |
+				   TX_DRIVER_LDO_BANDGAP_REF_ENABLE);
+		cdns_phy_reg_write(cdns_phy, (TX_TXCC_CPOST_MULT_00_0 | (k << 9)), 0x0);
+		cdns_phy_reg_write(cdns_phy, (TX_TXCC_CAL_SCLR_MULT_0 | (k << 9)),
+				   SCALED_RESISTOR_CALIBRATION_CODE_ADD |
+				   RESISTOR_CAL_MULT_VAL_32_128);
+	}
+}
+
+static int hdptx_hdmi_phy_config(struct cdns_hdptx_phy *cdns_phy,
+				 const struct hdptx_hdmi_ctrl *p_ctrl_table,
+				 const struct hdptx_hdmi_pll_tuning *p_pll_table,
+				 bool pclk_in)
+{
+	const u32 num_lanes = 4;
+	u32 val, k;
+	int ret;
+
+	/* enable PHY isolation mode only for CMN */
+	cdns_phy_reg_write(cdns_phy, PHY_PMA_ISOLATION_CTRL, 0xd000);
+
+	/* set cmn_pll0_clk_datart1_div/cmn_pll0_clk_datart0_div dividers */
+	val = cdns_phy_reg_read(cdns_phy, PHY_PMA_ISO_PLL_CTRL1);
+	val &= ~CMN_PLL0_CLK_DATART_DIV_MASK;
+	val |= FIELD_PREP(CMN_PLL0_CLK_DATART_DIV_MASK, 0x12);
+	cdns_phy_reg_write(cdns_phy, PHY_PMA_ISO_PLL_CTRL1, val);
+
+	/* assert PHY reset from isolation register */
+	cdns_phy_reg_write(cdns_phy, PHY_ISO_CMN_CTRL, 0x0000);
+	/* assert PMA CMN reset */
+	cdns_phy_reg_write(cdns_phy, PHY_PMA_ISO_CMN_CTRL, 0x0000);
+
+	/* register XCVR_DIAG_BIDI_CTRL */
+	for (k = 0; k < num_lanes; k++)
+		cdns_phy_reg_write(cdns_phy, XCVR_DIAG_BIDI_CTRL | (k << 9), 0x00ff);
+
+	/* Describing Task phy_cfg_hdp */
+	val = cdns_phy_reg_read(cdns_phy, PHY_PMA_CMN_CTRL1);
+	val &= ~CMA_REF_CLK_RCV_EN_MASK;
+	val |= FIELD_PREP(CMA_REF_CLK_RCV_EN_MASK, CMA_REF_CLK_RCV_EN);
+	cdns_phy_reg_write(cdns_phy, PHY_PMA_CMN_CTRL1, val);
+
+	/* PHY Registers */
+	val = cdns_phy_reg_read(cdns_phy, PHY_PMA_CMN_CTRL1);
+	val &= ~CMA_REF_CLK_DIG_DIV_MASK;
+	val |= FIELD_PREP(CMA_REF_CLK_DIG_DIV_MASK, CMN_REF_CLK_DIG_DIV);
+	cdns_phy_reg_write(cdns_phy, PHY_PMA_CMN_CTRL1, val);
+
+	val = cdns_phy_reg_read(cdns_phy, PHY_HDP_CLK_CTL);
+	val &= ~PLL_DATA_RATE_CLK_DIV_MASK;
+	val |= FIELD_PREP(PLL_DATA_RATE_CLK_DIV_MASK,
+			  PLL_DATA_RATE_CLK_DIV_HBR2);
+	cdns_phy_reg_write(cdns_phy, PHY_HDP_CLK_CTL, val);
+
+	/* Common control module control and diagnostic registers */
+	val = cdns_phy_reg_read(cdns_phy, CMN_CDIAG_REFCLK_CTRL);
+	val &= ~DIG_REF_CLK_DIV_SCALER_MASK;
+	val |= FIELD_PREP(DIG_REF_CLK_DIV_SCALER_MASK, REF_CLK_DIVIDER_SCALER);
+	val |= REFCLK_TERMINATION_EN_OVERRIDE_EN | REFCLK_TERMINATION_EN_OVERRIDE;
+	cdns_phy_reg_write(cdns_phy, CMN_CDIAG_REFCLK_CTRL, val);
+
+	/* High speed clock used */
+	val = cdns_phy_reg_read(cdns_phy, CMN_DIAG_HSCLK_SEL);
+	val &= ~(HSCLK1_SEL_MASK | HSCLK0_SEL_MASK);
+	val |= FIELD_PREP(HSCLK1_SEL_MASK, (p_ctrl_table->cmnda_hs_clk_1_sel >> 1));
+	val |= FIELD_PREP(HSCLK0_SEL_MASK, (p_ctrl_table->cmnda_hs_clk_0_sel >> 1));
+	cdns_phy_reg_write(cdns_phy, CMN_DIAG_HSCLK_SEL, val);
+
+	for (k = 0; k < num_lanes; k++) {
+		val = cdns_phy_reg_read(cdns_phy, (XCVR_DIAG_HSCLK_SEL | (k << 9)));
+		val &= ~HSCLK_SEL_MODE3_MASK;
+		val |= FIELD_PREP(HSCLK_SEL_MODE3_MASK,
+				  (p_ctrl_table->cmnda_hs_clk_0_sel >> 1));
+		cdns_phy_reg_write(cdns_phy, (XCVR_DIAG_HSCLK_SEL | (k << 9)), val);
+	}
+
+	/* PLL 0 control state machine registers */
+	val = p_ctrl_table->vco_ring_select << 12;
+	cdns_phy_reg_write(cdns_phy, CMN_PLLSM0_USER_DEF_CTRL, val);
+
+	if (pclk_in) {
+		val = 0x30a0;
+	} else {
+		val = cdns_phy_reg_read(cdns_phy, CMN_PLL0_VCOCAL_START);
+		val &= ~VCO_CALIB_CODE_START_POINT_VAL_MASK;
+		val |= FIELD_PREP(VCO_CALIB_CODE_START_POINT_VAL_MASK,
+				  p_pll_table->vco_cal_code);
+	}
+	cdns_phy_reg_write(cdns_phy, CMN_PLL0_VCOCAL_START, val);
+
+	cdns_phy_reg_write(cdns_phy, CMN_PLL0_VCOCAL_INIT_TMR, 0x0064);
+	cdns_phy_reg_write(cdns_phy, CMN_PLL0_VCOCAL_ITER_TMR, 0x000a);
+
+	/* Common functions control and diagnostics registers */
+	val = p_ctrl_table->cmnda_pll0_hs_sym_div_sel << 8;
+	val |= p_ctrl_table->cmnda_pll0_ip_div;
+	cdns_phy_reg_write(cdns_phy, CMN_DIAG_PLL0_INCLK_CTRL, val);
+
+	cdns_phy_reg_write(cdns_phy, CMN_DIAG_PLL0_OVRD, 0x0000);
+
+	val = p_ctrl_table->cmnda_pll0_fb_div_high;
+	val |= PLL_FEEDBACK_DIV_HI_OVERRIDE_EN;
+	cdns_phy_reg_write(cdns_phy, CMN_DIAG_PLL0_FBH_OVRD, val);
+
+	val = p_ctrl_table->cmnda_pll0_fb_div_low;
+	val |= PLL_FEEDBACK_DIV_LO_OVERRIDE_EN;
+	cdns_phy_reg_write(cdns_phy, CMN_DIAG_PLL0_FBL_OVRD, val);
+
+	if (!pclk_in) {
+		val = p_ctrl_table->cmnda_pll0_pxdiv_low;
+		cdns_phy_reg_write(cdns_phy, CMN_DIAG_PLL0_PXL_DIVL, val);
+
+		val = p_ctrl_table->cmnda_pll0_pxdiv_high;
+		val |= PLL_PCLK_DIV_EN;
+		cdns_phy_reg_write(cdns_phy, CMN_DIAG_PLL0_PXL_DIVH, val);
+	}
+
+	val = p_pll_table->volt_to_current_coarse;
+	val |= (p_pll_table->volt_to_current) << 4;
+	cdns_phy_reg_write(cdns_phy, CMN_DIAG_PLL0_V2I_TUNE, val);
+
+	val = p_pll_table->charge_pump_gain;
+	cdns_phy_reg_write(cdns_phy, CMN_DIAG_PLL0_CP_TUNE, val);
+
+	cdns_phy_reg_write(cdns_phy, CMN_DIAG_PLL0_LF_PROG, 0x0008);
+
+	val = p_pll_table->pmos_ctrl;
+	val |= (p_pll_table->ndac_ctrl) << 8;
+	cdns_phy_reg_write(cdns_phy, CMN_DIAG_PLL0_PTATIS_TUNE1, val);
+
+	val = p_pll_table->ptat_ndac_ctrl;
+	cdns_phy_reg_write(cdns_phy, CMN_DIAG_PLL0_PTATIS_TUNE2, val);
+
+	if (pclk_in)
+		cdns_phy_reg_write(cdns_phy, CMN_DIAG_PLL0_TEST_MODE, 0x0022);
+	else
+		cdns_phy_reg_write(cdns_phy, CMN_DIAG_PLL0_TEST_MODE, 0x0020);
+
+	cdns_phy_reg_write(cdns_phy, CMN_PSM_CLK_CTRL, 0x0016);
+
+	/* Transceiver control and diagnostic registers */
+	for (k = 0; k < num_lanes; k++) {
+		val = cdns_phy_reg_read(cdns_phy, (XCVR_DIAG_PLLDRC_CTRL | (k << 9)));
+		val &= ~DPLL_CLK_SEL_MODE3;
+		cdns_phy_reg_write(cdns_phy, (XCVR_DIAG_PLLDRC_CTRL | (k << 9)), val);
+	}
+
+	for (k = 0; k < num_lanes; k++) {
+		val = cdns_phy_reg_read(cdns_phy, (TX_DIAG_TX_CTRL | (k << 9)));
+		val &= ~TX_IF_SUBRATE_MODE3_MASK;
+		val |= FIELD_PREP(TX_IF_SUBRATE_MODE3_MASK,
+				  (p_ctrl_table->hsclk_div_tx_sub_rate >> 1));
+		cdns_phy_reg_write(cdns_phy, (TX_DIAG_TX_CTRL | (k << 9)), val);
+	}
+
+	val = cdns_phy_reg_read(cdns_phy, PHY_PMA_CMN_CTRL1);
+	val &= ~CMA_REF_CLK_SEL_MASK;
+	/*
+	 * single ended reference clock (val |= 0x0030);
+	 * differential clock  (val |= 0x0000);
+	 * for differential clock on the refclk_p and
+	 * refclk_m off chip pins: CMN_DIAG_ACYA[8]=1'b1
+	 * cdns_phy_reg_write(cdns_phy, CMN_DIAG_ACYA, 0x0100);
+	 */
+	val |= FIELD_PREP(CMA_REF_CLK_SEL_MASK, 3);
+	cdns_phy_reg_write(cdns_phy, PHY_PMA_CMN_CTRL1, val);
+
+	/* Deassert PHY reset */
+	cdns_phy_reg_write(cdns_phy, PHY_ISO_CMN_CTRL, 0x0001);
+	cdns_phy_reg_write(cdns_phy, PHY_PMA_ISO_CMN_CTRL, 0x0003);
+
+	/* Power state machine registers */
+	for (k = 0; k < num_lanes; k++)
+		cdns_phy_reg_write(cdns_phy, XCVR_PSM_RCTRL | (k << 9), 0xfefc);
+
+	/* Assert cmn_macro_pwr_en */
+	cdns_phy_reg_write(cdns_phy, PHY_PMA_ISO_CMN_CTRL, 0x0013);
+
+	/* wait for cmn_macro_pwr_en_ack */
+	ret = wait_for_ack(cdns_phy, PHY_PMA_ISO_CMN_CTRL, CMN_MACRO_PWR_EN_ACK,
+			   "MA output macro power up failed");
+	if (ret < 0)
+		return ret;
+
+	/* wait for cmn_ready */
+	ret = wait_for_ack(cdns_phy, PHY_PMA_CMN_CTRL1, CMN_READY,
+			   "PMA output ready failed");
+	if (ret < 0)
+		return ret;
+
+	for (k = 0; k < num_lanes; k++) {
+		cdns_phy_reg_write(cdns_phy, TX_PSC_A0 | (k << 9), 0x6791);
+		cdns_phy_reg_write(cdns_phy, TX_PSC_A1 | (k << 9), 0x6790);
+		cdns_phy_reg_write(cdns_phy, TX_PSC_A2 | (k << 9), 0x0090);
+		cdns_phy_reg_write(cdns_phy, TX_PSC_A3 | (k << 9), 0x0090);
+
+		val = cdns_phy_reg_read(cdns_phy, RX_PSC_CAL | (k << 9));
+		val &= 0xffbb;
+		cdns_phy_reg_write(cdns_phy, RX_PSC_CAL | (k << 9), val);
+
+		val = cdns_phy_reg_read(cdns_phy, RX_PSC_A0 | (k << 9));
+		val &= 0xffbb;
+		cdns_phy_reg_write(cdns_phy, RX_PSC_A0 | (k << 9), val);
+	}
+
+	return 0;
+}
+
+static int hdptx_hdmi_phy_cfg(struct cdns_hdptx_phy *cdns_phy, unsigned long long char_rate)
+{
+	const struct hdptx_hdmi_ctrl *p_ctrl_table;
+	const struct hdptx_hdmi_pll_tuning *p_pll_table;
+	const u32 refclk_freq_khz = cdns_phy->ref_clk_rate / 1000;
+	const bool pclk_in = false;
+	u32 char_rate_khz = char_rate / 1000;
+	u32 vco_freq, rate;
+	u32 div_total, i;
+
+	dev_dbg(cdns_phy->dev, "character clock: %d KHz\n ", char_rate_khz);
+
+	/* Get right row from the ctrl_table table.
+	 * check the character rate.
+	 */
+	for (i = 0; i < ARRAY_SIZE(pixel_clk_output_ctrl_table); i++) {
+		rate = pixel_clk_output_ctrl_table[i].feedback_factor *
+		       pixel_clk_output_ctrl_table[i].pixel_clk_freq / 1000;
+		if (char_rate_khz == rate) {
+			p_ctrl_table = &pixel_clk_output_ctrl_table[i];
+			break;
+		}
+	}
+	if (i == ARRAY_SIZE(pixel_clk_output_ctrl_table)) {
+		dev_warn(cdns_phy->dev,
+			 "char clk (%d KHz) not supported\n", char_rate_khz);
+		return -EINVAL;
+	}
+
+	div_total = p_ctrl_table->pll_fb_div_total;
+	vco_freq = refclk_freq_khz * div_total / p_ctrl_table->cmnda_pll0_ip_div;
+
+	/* Get right row from the pixel_clk_output_pll_table table.
+	 * Check if vco_freq_khz and feedback_div_total
+	 * column matching with pixel_clk_output_pll_table.
+	 */
+	for (i = 0; i < ARRAY_SIZE(pixel_clk_output_pll_table); i++) {
+		if (vco_freq == pixel_clk_output_pll_table[i].vco_freq &&
+		    div_total == pixel_clk_output_pll_table[i].feedback_div_total) {
+			p_pll_table = &pixel_clk_output_pll_table[i];
+			break;
+		}
+	}
+	if (i == ARRAY_SIZE(pixel_clk_output_pll_table)) {
+		dev_warn(cdns_phy->dev, "VCO (%d KHz) not supported\n", vco_freq);
+		return -EINVAL;
+	}
+	dev_dbg(cdns_phy->dev, "VCO frequency is (%d KHz)\n", vco_freq);
+
+	return hdptx_hdmi_phy_config(cdns_phy, p_ctrl_table, p_pll_table, pclk_in);
+}
+
+static int hdptx_hdmi_phy_power_up(struct cdns_hdptx_phy *cdns_phy)
+{
+	int ret;
+
+	/* set Power State to A2 */
+	cdns_phy_reg_write(cdns_phy, PHY_HDP_MODE_CTRL, POWER_STATE_A2);
+
+	cdns_phy_reg_write(cdns_phy, TX_DIAG_ACYA_0, 1);
+	cdns_phy_reg_write(cdns_phy, TX_DIAG_ACYA_1, 1);
+	cdns_phy_reg_write(cdns_phy, TX_DIAG_ACYA_2, 1);
+	cdns_phy_reg_write(cdns_phy, TX_DIAG_ACYA_3, 1);
+
+	ret = wait_for_ack(cdns_phy, PHY_HDP_MODE_CTRL, POWER_STATE_A2_ACK,
+			   "Wait A2 Ack failed");
+	if (ret < 0)
+		return ret;
+
+	/* Power up ARC */
+	hdptx_hdmi_arc_config(cdns_phy);
+
+	/* Configure PHY in A0 mode (PHY must be in the A0 power
+	 * state in order to transmit data)
+	 */
+	cdns_phy_reg_write(cdns_phy, PHY_HDP_MODE_CTRL, POWER_STATE_A0);
+
+	return wait_for_ack(cdns_phy, PHY_HDP_MODE_CTRL, POWER_STATE_A0_ACK,
+			    "Wait A0 Ack failed");
+}
+
+static int hdptx_hdmi_phy_power_down(struct cdns_hdptx_phy *cdns_phy)
+{
+	u32 val;
+
+	val = cdns_phy_reg_read(cdns_phy, PHY_HDP_MODE_CTRL);
+	val &= ~(POWER_STATE_A0 | POWER_STATE_A1 | POWER_STATE_A2 | POWER_STATE_A3);
+	/* PHY_DP_MODE_CTL set to A3 power state */
+	cdns_phy_reg_write(cdns_phy, PHY_HDP_MODE_CTRL, val | POWER_STATE_A3);
+
+	return wait_for_ack(cdns_phy, PHY_HDP_MODE_CTRL, POWER_STATE_A3_ACK,
+			    "Wait A3 Ack failed");
+}
+
+static int hdptx_hdmi_configure(struct phy *phy,
+				union phy_configure_opts *opts)
+{
+	struct cdns_hdptx_phy *cdns_phy = phy_get_drvdata(phy);
+	u32 reg;
+	int ret;
+
+	cdns_phy->hdmi.tmds_char_rate = opts->hdmi.tmds_char_rate;
+
+	/* Check HDMI FW alive before HDMI PHY init */
+	ret = readl_poll_timeout(cdns_phy->regs + KEEP_ALIVE, reg,
+				 reg & CDNS_KEEP_ALIVE_MASK, 500,
+				 CDNS_KEEP_ALIVE_TIMEOUT);
+	if (ret < 0) {
+		dev_err(cdns_phy->dev, "NO HDMI FW running\n");
+		return -ENXIO;
+	}
+
+	/* Configure PHY */
+	if (hdptx_hdmi_phy_cfg(cdns_phy, cdns_phy->hdmi.tmds_char_rate) < 0) {
+		dev_err(cdns_phy->dev, "failed to set phy pclock\n");
+		return -EINVAL;
+	}
+
+	hdptx_hdmi_phy_set_vswing(cdns_phy);
+
+	return 0;
+}
+
+static int cdns_hdptx_phy_on(struct phy *phy)
+{
+	struct cdns_hdptx_phy *cdns_phy = phy_get_drvdata(phy);
+
+	if (phy->attrs.mode == PHY_MODE_DP)
+		return hdptx_dp_phy_power_up(cdns_phy);
+	else
+		return hdptx_hdmi_phy_power_up(cdns_phy);
+}
+
+static int cdns_hdptx_phy_off(struct phy *phy)
+{
+	struct cdns_hdptx_phy *cdns_phy = phy_get_drvdata(phy);
+
+	if (phy->attrs.mode == PHY_MODE_DP)
+		return hdptx_dp_phy_power_down(cdns_phy);
+	else
+		return hdptx_hdmi_phy_power_down(cdns_phy);
+}
+
+static int
+cdns_hdptx_phy_valid(struct phy *phy, enum phy_mode mode,
+		     int submode, union phy_configure_opts *opts)
+{
+	u32 rate = opts->hdmi.tmds_char_rate / 1000;
+	int i;
+
+	if (mode == PHY_MODE_DP)
+		return 0;
+
+	for (i = 0; i < ARRAY_SIZE(pixel_clk_output_ctrl_table); i++)
+		if (rate == pixel_clk_output_ctrl_table[i].pixel_clk_freq)
+			return 0;
+
+	return -EINVAL;
+}
+
+static int cdns_hdptx_phy_set_mode(struct phy *phy, enum phy_mode mode, int submode)
+{
+	struct cdns_hdptx_phy *cdns_phy = phy_get_drvdata(phy);
+	int ret = 0;
+
+	if (mode == PHY_MODE_DP) {
+		hdptx_dp_phy_ref_clock_type(cdns_phy);
+		hdptx_dp_aux_cfg(cdns_phy);
+	} else if (mode != PHY_MODE_HDMI) {
+		dev_err(&phy->dev, "Invalid PHY mode: %u\n", mode);
+		return -EINVAL;
+	}
+
+	return ret;
+}
+
+static int cdns_hdptx_configure(struct phy *phy,
+				union phy_configure_opts *opts)
+{
+	if (phy->attrs.mode == PHY_MODE_DP)
+		return hdptx_dp_configure(phy, opts);
+	else
+		return hdptx_hdmi_configure(phy, opts);
+}
+
+static const struct phy_ops cdns_hdptx_phy_ops = {
+	.set_mode = cdns_hdptx_phy_set_mode,
+	.configure = cdns_hdptx_configure,
+	.power_on = cdns_hdptx_phy_on,
+	.power_off = cdns_hdptx_phy_off,
+	.validate = cdns_hdptx_phy_valid,
+	.owner = THIS_MODULE,
+};
+
+static int cdns_hdptx_phy_probe(struct platform_device *pdev)
+{
+	struct cdns_hdptx_phy *cdns_phy;
+	struct device *dev = &pdev->dev;
+	struct device_node *node = dev->of_node;
+	struct phy_provider *phy_provider;
+	struct resource *res;
+	struct phy *phy;
+	int ret;
+
+	cdns_phy = devm_kzalloc(dev, sizeof(*cdns_phy), GFP_KERNEL);
+	if (!cdns_phy)
+		return -ENOMEM;
+
+	dev_set_drvdata(dev, cdns_phy);
+	cdns_phy->dev = dev;
+
+	res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+	if (!res)
+		return -ENODEV;
+	cdns_phy->regs = devm_ioremap(dev, res->start, resource_size(res));
+	if (IS_ERR(cdns_phy->regs))
+		return PTR_ERR(cdns_phy->regs);
+
+	phy = devm_phy_create(dev, node, &cdns_hdptx_phy_ops);
+	if (IS_ERR(phy))
+		return PTR_ERR(phy);
+
+	cdns_phy->phy = phy;
+	phy_set_drvdata(phy, cdns_phy);
+
+	/* init base struct for access mhdp mailbox */
+	cdns_phy->base.dev = cdns_phy->dev;
+	cdns_phy->base.regs = cdns_phy->regs;
+
+	ret = hdptx_clk_enable(cdns_phy);
+	if (ret)
+		return -EINVAL;
+
+	phy_provider = devm_of_phy_provider_register(dev, of_phy_simple_xlate);
+	if (IS_ERR(phy_provider))
+		return PTR_ERR(phy_provider);
+
+	return 0;
+}
+
+static const struct of_device_id cdns_hdptx_phy_of_match[] = {
+	{.compatible = "fsl,imx8mq-hdptx-phy" },
+	{ /* sentinel */ }
+};
+MODULE_DEVICE_TABLE(of, cdns_hdptx_phy_of_match);
+
+static struct platform_driver cdns_hdptx_phy_driver = {
+	.probe = cdns_hdptx_phy_probe,
+	.driver = {
+		.name	= "cdns-hdptx-phy",
+		.of_match_table	= cdns_hdptx_phy_of_match,
+	}
+};
+module_platform_driver(cdns_hdptx_phy_driver);
+
+MODULE_AUTHOR("Sandor Yu <sandor.yu@nxp.com>");
+MODULE_DESCRIPTION("Cadence HDP-TX DP/HDMI PHY driver");
+MODULE_LICENSE("GPL");

From patchwork Tue Dec 17 06:51:50 2024
Content-Type: text/plain; charset="utf-8"
MIME-Version: 1.0
Content-Transfer-Encoding: 7bit
Subject: [v20,8/9] arm64: dts: imx8mq: Add DCSS + HDMI/DP display pipeline
From: Sandor Yu <Sandor.yu@nxp.com>
X-Patchwork-Id: 629295
Message-Id: 
 <b730433022fc3af7b271827e86fc4193229862e7.1734340233.git.Sandor.yu@nxp.com>
To: dmitry.baryshkov@linaro.org, andrzej.hajda@intel.com,
 neil.armstrong@linaro.org, Laurent.pinchart@ideasonboard.com,
 jonas@kwiboo.se, jernej.skrabec@gmail.com, airlied@gmail.com,
 daniel@ffwll.ch, robh+dt@kernel.org, krzysztof.kozlowski+dt@linaro.org,
 shawnguo@kernel.org, s.hauer@pengutronix.de, festevam@gmail.com,
 vkoul@kernel.org, dri-devel@lists.freedesktop.org,
 devicetree@vger.kernel.org, linux-arm-kernel@lists.infradead.org,
 linux-kernel@vger.kernel.org, linux-phy@lists.infradead.org,
 mripard@kernel.org
Cc: kernel@pengutronix.de, linux-imx@nxp.com, Sandor.yu@nxp.com,
 oliver.brown@nxp.com, alexander.stein@ew.tq-group.com, sam@ravnborg.org
Date: Tue, 17 Dec 2024 14:51:50 +0800

From: Alexander Stein <alexander.stein@ew.tq-group.com>

This adds DCSS + MHDP + MHDP PHY nodes. PHY mode (DP/HDMI) is selected
by the connector type connected to mhdp port@1 endpoint.

Signed-off-by: Alexander Stein <alexander.stein@ew.tq-group.com>
---
v17->v20:
 *No change

 arch/arm64/boot/dts/freescale/imx8mq.dtsi | 68 +++++++++++++++++++++++
 1 file changed, 68 insertions(+)

diff --git a/arch/arm64/boot/dts/freescale/imx8mq.dtsi b/arch/arm64/boot/dts/freescale/imx8mq.dtsi
index d51de8d899b2b..df8ba1d5391ae 100644
--- a/arch/arm64/boot/dts/freescale/imx8mq.dtsi
+++ b/arch/arm64/boot/dts/freescale/imx8mq.dtsi
@@ -1602,6 +1602,74 @@ aips4: bus@32c00000 { /* AIPS4 */
 			#size-cells = <1>;
 			ranges = <0x32c00000 0x32c00000 0x400000>;
 
+			mdhp_phy: phy@32c00000 {
+				compatible = "fsl,imx8mq-hdptx-phy";
+				reg = <0x32c00000 0x100000>;
+				#phy-cells = <0>;
+				clocks = <&hdmi_phy_27m>, <&clk IMX8MQ_CLK_DISP_APB_ROOT>;
+				clock-names = "ref", "apb";
+			};
+
+			mhdp: bridge@32c00000 {
+				compatible = "fsl,imx8mq-mhdp8501";
+				reg = <0x32c00000 0x100000>;
+				interrupts = <GIC_SPI 16 IRQ_TYPE_LEVEL_HIGH>,
+					     <GIC_SPI 25 IRQ_TYPE_LEVEL_HIGH>;
+				interrupt-names = "plug_in", "plug_out";
+				clocks = <&clk IMX8MQ_CLK_DISP_APB_ROOT>;
+				phys = <&mdhp_phy>;
+				status = "disabled";
+
+				ports {
+					#address-cells = <1>;
+					#size-cells = <0>;
+
+					port@0 {
+						reg = <0>;
+
+						mhdp_in: endpoint {
+							remote-endpoint = <&dcss_out>;
+						};
+					};
+
+					port@1 {
+						reg = <1>;
+
+						mhdp_out: endpoint {
+						};
+					};
+				};
+			};
+
+			dcss: display-controller@32e00000 {
+				compatible = "nxp,imx8mq-dcss";
+				reg = <0x32e00000 0x2d000>, <0x32e2f000 0x1000>;
+				interrupt-parent = <&irqsteer>;
+				interrupts = <6>, <8>, <9>;
+				interrupt-names = "ctxld", "ctxld_kick", "vblank";
+				clocks = <&clk IMX8MQ_CLK_DISP_APB_ROOT>,
+					 <&clk IMX8MQ_CLK_DISP_AXI_ROOT>,
+					 <&clk IMX8MQ_CLK_DISP_RTRM_ROOT>,
+					 <&clk IMX8MQ_VIDEO2_PLL_OUT>,
+					 <&clk IMX8MQ_CLK_DISP_DTRC>;
+				clock-names = "apb", "axi", "rtrm", "pix", "dtrc";
+				assigned-clocks = <&clk IMX8MQ_CLK_DISP_AXI>,
+						  <&clk IMX8MQ_CLK_DISP_RTRM>,
+						  <&clk IMX8MQ_VIDEO2_PLL1_REF_SEL>;
+				assigned-clock-parents = <&clk IMX8MQ_SYS1_PLL_800M>,
+							 <&clk IMX8MQ_SYS1_PLL_800M>,
+							 <&clk IMX8MQ_CLK_27M>;
+				assigned-clock-rates = <800000000>,
+						       <400000000>;
+				status = "disabled";
+
+				port {
+					dcss_out: endpoint {
+						remote-endpoint = <&mhdp_in>;
+					};
+				};
+			};
+
 			irqsteer: interrupt-controller@32e2d000 {
 				compatible = "fsl,imx8m-irqsteer", "fsl,imx-irqsteer";
 				reg = <0x32e2d000 0x1000>;

From patchwork Tue Dec 17 06:51:51 2024
Content-Type: text/plain; charset="utf-8"
MIME-Version: 1.0
Content-Transfer-Encoding: 7bit
Subject: [v20,9/9] arm64: dts: imx8mq: tqma8mq-mba8mx: Enable HDMI support
From: Sandor Yu <Sandor.yu@nxp.com>
X-Patchwork-Id: 629296
Message-Id: 
 <e72920a199e245d0e1f71f3a62af6c603e4b1f39.1734340233.git.Sandor.yu@nxp.com>
To: dmitry.baryshkov@linaro.org, andrzej.hajda@intel.com,
 neil.armstrong@linaro.org, Laurent.pinchart@ideasonboard.com,
 jonas@kwiboo.se, jernej.skrabec@gmail.com, airlied@gmail.com,
 daniel@ffwll.ch, robh+dt@kernel.org, krzysztof.kozlowski+dt@linaro.org,
 shawnguo@kernel.org, s.hauer@pengutronix.de, festevam@gmail.com,
 vkoul@kernel.org, dri-devel@lists.freedesktop.org,
 devicetree@vger.kernel.org, linux-arm-kernel@lists.infradead.org,
 linux-kernel@vger.kernel.org, linux-phy@lists.infradead.org,
 mripard@kernel.org
Cc: kernel@pengutronix.de, linux-imx@nxp.com, Sandor.yu@nxp.com,
 oliver.brown@nxp.com, alexander.stein@ew.tq-group.com, sam@ravnborg.org
Date: Tue, 17 Dec 2024 14:51:51 +0800

From: Alexander Stein <alexander.stein@ew.tq-group.com>

Add HDMI connector and connect it to MHDP output. Enable peripherals
for HDMI output.

Signed-off-by: Alexander Stein <alexander.stein@ew.tq-group.com>
---
v19->v20:
 *No change

v18->v19:
- Move property data-lanes to endpoint of port@1

v17->v18:
- replace lane-mapping with data-lanes

 .../dts/freescale/imx8mq-tqma8mq-mba8mx.dts   | 26 +++++++++++++++++++
 arch/arm64/boot/dts/freescale/mba8mx.dtsi     | 11 ++++++++
 2 files changed, 37 insertions(+)

diff --git a/arch/arm64/boot/dts/freescale/imx8mq-tqma8mq-mba8mx.dts b/arch/arm64/boot/dts/freescale/imx8mq-tqma8mq-mba8mx.dts
index 0165f3a259853..5ba06a411c6a1 100644
--- a/arch/arm64/boot/dts/freescale/imx8mq-tqma8mq-mba8mx.dts
+++ b/arch/arm64/boot/dts/freescale/imx8mq-tqma8mq-mba8mx.dts
@@ -53,6 +53,10 @@ &btn2 {
 	gpios = <&gpio3 17 GPIO_ACTIVE_LOW>;
 };
 
+&dcss {
+	status = "okay";
+};
+
 &gpio_leds {
 	led3 {
 		label = "led3";
@@ -60,6 +64,14 @@ led3 {
 	};
 };
 
+&hdmi_connector {
+	port {
+		hdmi_connector_in: endpoint {
+			remote-endpoint = <&mhdp_out>;
+		};
+	};
+};
+
 &i2c1 {
 	expander2: gpio@25 {
 		compatible = "nxp,pca9555";
@@ -91,6 +103,20 @@ &led2 {
 	gpios = <&gpio3 16 GPIO_ACTIVE_HIGH>;
 };
 
+&mhdp {
+	status = "okay";
+	ports {
+		port@1 {
+			reg = <1>;
+
+			mhdp_out: endpoint {
+				remote-endpoint = <&hdmi_connector_in>;
+				data-lanes = <0 1 2 3>;
+			};
+		};
+	};
+};
+
 /* PCIe slot on X36 */
 &pcie0 {
 	reset-gpio = <&expander0 14 GPIO_ACTIVE_LOW>;
diff --git a/arch/arm64/boot/dts/freescale/mba8mx.dtsi b/arch/arm64/boot/dts/freescale/mba8mx.dtsi
index 58e3865c28895..d04b75a76dfe6 100644
--- a/arch/arm64/boot/dts/freescale/mba8mx.dtsi
+++ b/arch/arm64/boot/dts/freescale/mba8mx.dtsi
@@ -89,6 +89,17 @@ gpio_delays: gpio-delays {
 		gpio-line-names = "LVDS_BRIDGE_EN_1V8";
 	};
 
+	hdmi_connector: connector {
+		compatible = "hdmi-connector";
+		label = "X11";
+		type = "a";
+
+		port {
+			hdmi_connector_in: endpoint {
+			};
+		};
+	};
+
 	panel: panel-lvds {
 		/*
 		 * Display is not fixed, so compatible has to be added from
