From d3f81ed48b5f275372fc0a7f083dd1af0b5bef0a Mon Sep 17 00:00:00 2001
From: Alex Bee <knaerzche@gmail.com>
Date: Wed, 5 May 2021 19:11:12 +0200
Subject: [PATCH 44/59] WIP/1002: arm64: boot: dts: Increase ACLK_PERILP0 clock
 rate for RK3399

As per vendor kernel. Leaving this clock at the lower rate will
result in poor DMA controller performance

Signed-off-by: Alex Bee <knaerzche@gmail.com>
---
 arch/arm64/boot/dts/rockchip/rk3399-base.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/arch/arm64/boot/dts/rockchip/rk3399-base.dtsi b/arch/arm64/boot/dts/rockchip/rk3399-base.dtsi
index d27e3fa9ff80..f06147581fab 100644
--- a/arch/arm64/boot/dts/rockchip/rk3399-base.dtsi
+++ b/arch/arm64/boot/dts/rockchip/rk3399-base.dtsi
@@ -1592,7 +1592,7 @@ cru: clock-controller@ff760000 {
 			<1000000000>,
 			 <150000000>,   <75000000>,
 			  <37500000>,
-			 <100000000>,  <100000000>,
+			 <300000000>,  <100000000>,
 			  <50000000>, <600000000>,
 			 <100000000>,   <50000000>,
 			 <400000000>, <400000000>,
-- 
2.34.1

