# Use direct path to firmware as update script doesn't dereference sym links.
FIRMWARE_ROOT="/usr/lib/kernel-overlays/base/lib/firmware/raspberrypi/bootloader"
FIRMWARE_BACKUP_DIR="/storage/.config/rpifw-backup"
BOOTFS=${BOOTFS:-/flash}

if [ -f /storage/.config/rpi-eeprom-update ]; then
  . /storage/.config/rpi-eeprom-update
fi
