From 3bd9c85894e889f86176850f5f31e3009b637037 Mon Sep 17 00:00:00 2001
From: Alex Bee <knaerzche@gmail.com>
Date: Sat, 27 Feb 2021 18:01:13 +0100
Subject: [PATCH 40/59] WIP/1002: arm64: dts: rockchip: Add ir-receiver node
 for RK3328 ROC CC

Signed-off-by: Alex Bee <knaerzche@gmail.com>
---
 arch/arm64/boot/dts/rockchip/rk3328-roc.dtsi | 14 ++++++++++++++
 1 file changed, 14 insertions(+)

diff --git a/arch/arm64/boot/dts/rockchip/rk3328-roc.dtsi b/arch/arm64/boot/dts/rockchip/rk3328-roc.dtsi
index 7eef6f7f108f..3fe0c17fd2b1 100644
--- a/arch/arm64/boot/dts/rockchip/rk3328-roc.dtsi
+++ b/arch/arm64/boot/dts/rockchip/rk3328-roc.dtsi
@@ -84,6 +84,13 @@ vcc_phy: regulator-vcc-phy {
 		regulator-boot-on;
 	};
 
+	ir-receiver {
+		compatible = "gpio-ir-receiver";
+		gpios = <&gpio2 RK_PA2 GPIO_ACTIVE_LOW>;
+		pinctrl-0 = <&ir_int>;
+		pinctrl-names = "default";
+	};
+
 	leds {
 		compatible = "gpio-leds";
 
@@ -304,6 +311,13 @@ &io_domains {
 };
 
 &pinctrl {
+
+	ir {
+		ir_int: ir-int {
+			rockchip,pins = <2 RK_PA2 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+
 	pmic {
 		pmic_int_l: pmic-int-l {
 			rockchip,pins = <1 RK_PD0 RK_FUNC_GPIO &pcfg_pull_up>;
-- 
2.34.1

