From 0202435665464cbf0bf9a3bb59e0da36aab17385 Mon Sep 17 00:00:00 2001
From: Alex Bee <knaerzche@gmail.com>
Date: Sun, 18 Sep 2022 10:35:52 +0200
Subject: [PATCH 47/59] WIP/1002: arm64: dts: rockchip: disable fusb for
 rk3399-roc-pc

As it will lead to an unbootable device in case one if those ports
is used to power up the device.

See https://lkml.org/lkml/2022/6/20/413
---
 arch/arm64/boot/dts/rockchip/rk3399-roc-pc.dtsi | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

diff --git a/arch/arm64/boot/dts/rockchip/rk3399-roc-pc.dtsi b/arch/arm64/boot/dts/rockchip/rk3399-roc-pc.dtsi
index fc9279627ef6..610518ff30ee 100644
--- a/arch/arm64/boot/dts/rockchip/rk3399-roc-pc.dtsi
+++ b/arch/arm64/boot/dts/rockchip/rk3399-roc-pc.dtsi
@@ -215,7 +215,7 @@ vdd_log: regulator-vdd-log {
 		regulator-name = "vdd_log";
 		regulator-always-on;
 		regulator-boot-on;
-		regulator-min-microvolt = <450000>;
+		regulator-min-microvolt = <430000>;
 		regulator-max-microvolt = <1400000>;
 		pwm-supply = <&vcc3v3_sys>;
 	};
@@ -536,7 +536,7 @@ fusb1: usb-typec@22 {
 		pinctrl-names = "default";
 		pinctrl-0 = <&fusb1_int>;
 		vbus-supply = <&vcc_vbus_typec1>;
-		status = "okay";
+		status = "disabled";
 	};
 };
 
@@ -553,7 +553,7 @@ fusb0: usb-typec@22 {
 		pinctrl-names = "default";
 		pinctrl-0 = <&fusb0_int>;
 		vbus-supply = <&vcc_vbus_typec0>;
-		status = "okay";
+		status = "disabled";
 	};
 
 	mp8859: regulator@66 {
-- 
2.34.1

