From ca832abe5bd81104aa5d2d193f9c279be4b15ee4 Mon Sep 17 00:00:00 2001
From: Alex Bee <knaerzche@gmail.com>
Date: Fri, 2 Apr 2021 17:54:22 +0200
Subject: [PATCH 38/59] WIP/1002: ARM/arm64: dts: rockchip: align sound card
 names

Signed-off-by: Alex Bee <knaerzche@gmail.com>
---
 arch/arm/boot/dts/rockchip/rk3288-tinker.dtsi | 2 +-
 arch/arm64/boot/dts/rockchip/rk3399-base.dtsi | 2 +-
 2 files changed, 2 insertions(+), 2 deletions(-)

diff --git a/arch/arm/boot/dts/rockchip/rk3288-tinker.dtsi b/arch/arm/boot/dts/rockchip/rk3288-tinker.dtsi
index 8e27a20f2845..b83b122d00f1 100644
--- a/arch/arm/boot/dts/rockchip/rk3288-tinker.dtsi
+++ b/arch/arm/boot/dts/rockchip/rk3288-tinker.dtsi
@@ -73,7 +73,7 @@ sdio_pwrseq: sdio-pwrseq {
 	sound {
 		compatible = "simple-audio-card";
 		simple-audio-card,format = "i2s";
-		simple-audio-card,name = "rockchip,tinker-codec";
+		simple-audio-card,name = "HDMI";
 		simple-audio-card,mclk-fs = <512>;
 
 		simple-audio-card,codec {
diff --git a/arch/arm64/boot/dts/rockchip/rk3399-base.dtsi b/arch/arm64/boot/dts/rockchip/rk3399-base.dtsi
index b031d77f3763..d27e3fa9ff80 100644
--- a/arch/arm64/boot/dts/rockchip/rk3399-base.dtsi
+++ b/arch/arm64/boot/dts/rockchip/rk3399-base.dtsi
@@ -2008,7 +2008,7 @@ hdmi_sound: hdmi-sound {
 		compatible = "simple-audio-card";
 		simple-audio-card,format = "i2s";
 		simple-audio-card,mclk-fs = <256>;
-		simple-audio-card,name = "hdmi-sound";
+		simple-audio-card,name = "HDMI";
 		status = "disabled";
 
 		simple-audio-card,cpu {
-- 
2.34.1

