From 74a72c367573ad521becf6cc4d649e14387b3c64 Mon Sep 17 00:00:00 2001
From: Bitterblue Smith <rtl8821cerfe2@gmail.com>
Date: Wed, 18 Dec 2024 02:16:11 +0200
Subject: [PATCH 32/35] wifi: rtw88: 8821a/8812a: Set ptct_efuse_size to 0

Some RTL8812AU devices fail to probe:

[   12.478774] rtw_8812au 1-1.3:1.0: failed to dump efuse logical map
[   12.487712] rtw_8812au 1-1.3:1.0: failed to setup chip efuse info
[   12.487742] rtw_8812au 1-1.3:1.0: failed to setup chip information
[   12.491077] rtw_8812au: probe of 1-1.3:1.0 failed with error -22

It turns out these chips don't need to "protect" any bytes at the end of
the efuse.

The original value of 96 was copied from rtw8821c.c.

No one reported any failures with RTL8821AU yet, but the vendor driver
uses the same efuse reading code for both chips.

Signed-off-by: Bitterblue Smith <rtl8821cerfe2@gmail.com>
Acked-by: Ping-Ke Shih <pkshih@realtek.com>
Signed-off-by: Ping-Ke Shih <pkshih@realtek.com>
Link: https://patch.msgid.link/1a477adb-60c3-463c-b158-3f86c94cb821@gmail.com
---
 drivers/net/wireless/realtek/rtw88/rtw8812a.c | 2 +-
 drivers/net/wireless/realtek/rtw88/rtw8821a.c | 2 +-
 2 files changed, 2 insertions(+), 2 deletions(-)

diff --git a/drivers/net/wireless/realtek/rtw88/rtw8812a.c b/drivers/net/wireless/realtek/rtw88/rtw8812a.c
index d8f0ed70777f..21795286a1a0 100644
--- a/drivers/net/wireless/realtek/rtw88/rtw8812a.c
+++ b/drivers/net/wireless/realtek/rtw88/rtw8812a.c
@@ -1027,7 +1027,7 @@ const struct rtw_chip_info rtw8812a_hw_spec = {
 	.rx_buf_desc_sz = 8,
 	.phy_efuse_size = 512,
 	.log_efuse_size = 512,
-	.ptct_efuse_size = 96 + 1, /* TODO or just 18? */
+	.ptct_efuse_size = 0,
 	.txff_size = 131072,
 	.rxff_size = 16128,
 	.rsvd_drv_pg_num = 9,
diff --git a/drivers/net/wireless/realtek/rtw88/rtw8821a.c b/drivers/net/wireless/realtek/rtw88/rtw8821a.c
index db242c9ad68f..dafab2af33bc 100644
--- a/drivers/net/wireless/realtek/rtw88/rtw8821a.c
+++ b/drivers/net/wireless/realtek/rtw88/rtw8821a.c
@@ -1118,7 +1118,7 @@ const struct rtw_chip_info rtw8821a_hw_spec = {
 	.rx_buf_desc_sz = 8,
 	.phy_efuse_size = 512,
 	.log_efuse_size = 512,
-	.ptct_efuse_size = 96 + 1, /* TODO or just 18? */
+	.ptct_efuse_size = 0,
 	.txff_size = 65536,
 	.rxff_size = 16128,
 	.rsvd_drv_pg_num = 8,
-- 
2.43.0

