################################################################################
# setup device defaults
################################################################################

  # The TARGET_CPU variable controls which processor should be targeted for
  # generated code.
    case $TARGET_ARCH in
      aarch64)
        TARGET_CPU="cortex-a53"
        TARGET_CPU_FLAGS="+crc+fp+simd"
        ;;
      arm)
        TARGET_KERNEL_ARCH="arm64"
        TARGET_FLOAT="hard"
        TARGET_CPU="cortex-a53"
        TARGET_CPU_FLAGS="+crc"
        TARGET_FPU="neon-fp-armv8"
        ;;
    esac

  # OpenGL-ES implementation to use
    OPENGLES="mesa"

  # Graphic drivers to use
    GRAPHIC_DRIVERS="lima panfrost"

  # KODI Player implementation to use
    KODIPLAYER_DRIVER="$OPENGLES"

  # Mali GPU family
    MALI_FAMILY="450 t820 g31 g52"

  # Set the addon project
    ADDON_PROJECT="ARMv8"
