From a5b67cd0fd28b9557c9b9011a98e2c0a85b4c90f Mon Sep 17 00:00:00 2001
From: Alex Bee <knaerzche@gmail.com>
Date: Mon, 1 Mar 2021 19:22:15 +0100
Subject: [PATCH 42/59] WIP/1002: HACK: arm64: dts: enable FE phy for Beelink
 A1 also

---
 arch/arm64/boot/dts/rockchip/rk3328-a1.dts | 8 ++++++++
 1 file changed, 8 insertions(+)

diff --git a/arch/arm64/boot/dts/rockchip/rk3328-a1.dts b/arch/arm64/boot/dts/rockchip/rk3328-a1.dts
index b276a29bdd85..962c3b3b804e 100644
--- a/arch/arm64/boot/dts/rockchip/rk3328-a1.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3328-a1.dts
@@ -147,6 +147,14 @@ rtl8211f: ethernet-phy@0 {
 	};
 };
 
+&gmac2phy {
+	clock_in_out = "output";
+	assigned-clock-rate = <50000000>;
+	assigned-clocks = <&cru SCLK_MAC2PHY>;
+	assigned-clock-parents = <&cru SCLK_MAC2PHY_SRC>;
+	status = "okay";
+};
+
 &gpu {
 	mali-supply = <&vdd_logic>;
 };
-- 
2.34.1

