From 5d0117163c35c896fca347fb2391b1f16251a35b Mon Sep 17 00:00:00 2001
From: Alex Bee <knaerzche@gmail.com>
Date: Mon, 1 Mar 2021 21:24:15 +0100
Subject: [PATCH 41/59] WIP/1002: ARM: dts: add cec pinctrl for RK3288 miqi
 board

---
 arch/arm/boot/dts/rockchip/rk3288-miqi.dts | 2 ++
 1 file changed, 2 insertions(+)

diff --git a/arch/arm/boot/dts/rockchip/rk3288-miqi.dts b/arch/arm/boot/dts/rockchip/rk3288-miqi.dts
index 20df626547bd..a5f5c6d38f80 100644
--- a/arch/arm/boot/dts/rockchip/rk3288-miqi.dts
+++ b/arch/arm/boot/dts/rockchip/rk3288-miqi.dts
@@ -145,6 +145,8 @@ &gpu {
 
 &hdmi {
 	ddc-i2c-bus = <&i2c5>;
+	pinctrl-names = "default";
+	pinctrl-0 = <&hdmi_cec_c0>;
 	status = "okay";
 };
 
-- 
2.34.1

