From 157ab827903e68cfb141f5bc600096ca822fffdf Mon Sep 17 00:00:00 2001
From: Jonas Karlman <jonas@kwiboo.se>
Date: Sun, 19 Jul 2020 16:35:11 +0000
Subject: [PATCH 18/59] WIP/1000: HACK: dts: rockchip: do not use vopl for hdmi

---
 arch/arm/boot/dts/rockchip/rk3288.dtsi        | 10 ----------
 arch/arm64/boot/dts/rockchip/rk3399-base.dtsi |  9 ---------
 2 files changed, 19 deletions(-)

diff --git a/arch/arm/boot/dts/rockchip/rk3288.dtsi b/arch/arm/boot/dts/rockchip/rk3288.dtsi
index bf0416834a5d..5f3e3cc8757c 100644
--- a/arch/arm/boot/dts/rockchip/rk3288.dtsi
+++ b/arch/arm/boot/dts/rockchip/rk3288.dtsi
@@ -1089,11 +1089,6 @@ vopl_out: port {
 			#address-cells = <1>;
 			#size-cells = <0>;
 
-			vopl_out_hdmi: endpoint@0 {
-				reg = <0>;
-				remote-endpoint = <&hdmi_in_vopl>;
-			};
-
 			vopl_out_edp: endpoint@1 {
 				reg = <1>;
 				remote-endpoint = <&edp_in_vopl>;
@@ -1260,11 +1255,6 @@ hdmi_in_vopb: endpoint@0 {
 					reg = <0>;
 					remote-endpoint = <&vopb_out_hdmi>;
 				};
-
-				hdmi_in_vopl: endpoint@1 {
-					reg = <1>;
-					remote-endpoint = <&vopl_out_hdmi>;
-				};
 			};
 
 			hdmi_out: port@1 {
diff --git a/arch/arm64/boot/dts/rockchip/rk3399-base.dtsi b/arch/arm64/boot/dts/rockchip/rk3399-base.dtsi
index 9d5f5b083e3c..ec5ca40b2159 100644
--- a/arch/arm64/boot/dts/rockchip/rk3399-base.dtsi
+++ b/arch/arm64/boot/dts/rockchip/rk3399-base.dtsi
@@ -1846,11 +1846,6 @@ vopl_out_edp: endpoint@1 {
 				remote-endpoint = <&edp_in_vopl>;
 			};
 
-			vopl_out_hdmi: endpoint@2 {
-				reg = <2>;
-				remote-endpoint = <&hdmi_in_vopl>;
-			};
-
 			vopl_out_mipi1: endpoint@3 {
 				reg = <3>;
 				remote-endpoint = <&mipi1_in_vopl>;
@@ -2048,10 +2043,6 @@ hdmi_in_vopb: endpoint@0 {
 					reg = <0>;
 					remote-endpoint = <&vopb_out_hdmi>;
 				};
-				hdmi_in_vopl: endpoint@1 {
-					reg = <1>;
-					remote-endpoint = <&vopl_out_hdmi>;
-				};
 			};
 
 			hdmi_out: port@1 {
-- 
2.34.1

