From a11c3b6c96c3be4f3dc6d14eca1c6f6f41297da7 Mon Sep 17 00:00:00 2001
From: Alex Bee <knaerzche@gmail.com>
Date: Sat, 21 Aug 2021 17:04:46 +0200
Subject: [PATCH 45/59] WIP/1002: arm64: dts: rockchip: Enable USB3 for rk3328
 Beelink A1

Signed-off-by: Alex Bee <knaerzche@gmail.com>
---
 arch/arm64/boot/dts/rockchip/rk3328-a1.dts | 5 +++++
 1 file changed, 5 insertions(+)

diff --git a/arch/arm64/boot/dts/rockchip/rk3328-a1.dts b/arch/arm64/boot/dts/rockchip/rk3328-a1.dts
index 962c3b3b804e..4feba4ae7a29 100644
--- a/arch/arm64/boot/dts/rockchip/rk3328-a1.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3328-a1.dts
@@ -389,6 +389,11 @@ &usb_host0_ehci {
 	status = "okay";
 };
 
+&usbdrd3 {
+	dr_mode = "host";
+	status = "okay";
+};
+
 &vop {
 	status = "okay";
 };
-- 
2.34.1

