From 93bbd545a8d3226afddac5c556e55727c21cc93a Mon Sep 17 00:00:00 2001
From: Jonas Karlman <jonas@kwiboo.se>
Date: Sat, 10 Oct 2020 14:33:30 +0000
Subject: [PATCH 06/59] WIP/1000: ARM: dts: rockchip: split rk3288 vop

Signed-off-by: Jonas Karlman <jonas@kwiboo.se>
---
 arch/arm/boot/dts/rockchip/rk3288.dtsi | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

diff --git a/arch/arm/boot/dts/rockchip/rk3288.dtsi b/arch/arm/boot/dts/rockchip/rk3288.dtsi
index 42d705b544ec..60ff3bf14efe 100644
--- a/arch/arm/boot/dts/rockchip/rk3288.dtsi
+++ b/arch/arm/boot/dts/rockchip/rk3288.dtsi
@@ -1023,7 +1023,7 @@ rga: rga@ff920000 {
 	};
 
 	vopb: vop@ff930000 {
-		compatible = "rockchip,rk3288-vop";
+		compatible = "rockchip,rk3288-vop-big";
 		reg = <0x0 0xff930000 0x0 0x19c>, <0x0 0xff931000 0x0 0x1000>;
 		interrupts = <GIC_SPI 15 IRQ_TYPE_LEVEL_HIGH>;
 		clocks = <&cru ACLK_VOP0>, <&cru DCLK_VOP0>, <&cru HCLK_VOP0>;
@@ -1072,7 +1072,7 @@ vopb_mmu: iommu@ff930300 {
 	};
 
 	vopl: vop@ff940000 {
-		compatible = "rockchip,rk3288-vop";
+		compatible = "rockchip,rk3288-vop-lit";
 		reg = <0x0 0xff940000 0x0 0x19c>, <0x0 0xff941000 0x0 0x1000>;
 		interrupts = <GIC_SPI 16 IRQ_TYPE_LEVEL_HIGH>;
 		clocks = <&cru ACLK_VOP1>, <&cru DCLK_VOP1>, <&cru HCLK_VOP1>;
-- 
2.34.1

